From c9289ca2b21ff678a5e6805f493de9285f404adb Mon Sep 17 00:00:00 2001
From: Hao Chen <chenhao288@hisilicon.com>
Date: Tue, 28 Sep 2021 11:52:08 +0800
Subject: [PATCH 116/283] net: hns3: add required space in comment

mainline inclusion
from mainline-v5.15-rc1
commit 0cb0704149f0d9d3b7c68ebab932fc27222c740b
category: feature
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EMYT
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=0cb0704149f0d9d3b7c68ebab932fc27222c740b

----------------------------------------------------------------------

Add some required spaces in comment for cleanup.

Signed-off-by: Hao Chen <chenhao288@hisilicon.com>
Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Reviewed-by: Yongxin Li <liyongxin1@huawei.com>
Signed-off-by: Junxin Chen <chenjunxin1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>
---
 drivers/net/ethernet/hisilicon/hns3/hclge_mbx.h         | 2 +-
 drivers/net/ethernet/hisilicon/hns3/hns3_enet.h         | 2 +-
 drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h  | 2 +-
 drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_main.c | 2 +-
 4 files changed, 4 insertions(+), 4 deletions(-)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hclge_mbx.h b/drivers/net/ethernet/hisilicon/hns3/hclge_mbx.h
index 5a13eea2742d..98045a4649e8 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hclge_mbx.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hclge_mbx.h
@@ -9,7 +9,7 @@
 
 enum HCLGE_MBX_OPCODE {
 	HCLGE_MBX_RESET = 0x01,		/* (VF -> PF) assert reset */
-	HCLGE_MBX_ASSERTING_RESET,	/* (PF -> VF) PF is asserting reset*/
+	HCLGE_MBX_ASSERTING_RESET,	/* (PF -> VF) PF is asserting reset */
 	HCLGE_MBX_SET_UNICAST,		/* (VF -> PF) set UC addr */
 	HCLGE_MBX_SET_MULTICAST,	/* (VF -> PF) set MC addr */
 	HCLGE_MBX_SET_VLAN,		/* (VF -> PF) set VLAN */
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h
index 3df794363632..9278c742e3b0 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h
@@ -340,7 +340,7 @@ enum hns3_pkt_l3type {
 	HNS3_L3_TYPE_LLDP,
 	HNS3_L3_TYPE_BPDU,
 	HNS3_L3_TYPE_MAC_PAUSE,
-	HNS3_L3_TYPE_PFC_PAUSE,/* 0x9*/
+	HNS3_L3_TYPE_PFC_PAUSE, /* 0x9 */
 
 	/* reserved for 0xA~0xB */
 
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h b/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h
index d17c85959507..c06070cfd4bc 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h
@@ -443,7 +443,7 @@ struct hclge_tc_thrd {
 };
 
 struct hclge_priv_buf {
-	struct hclge_waterline wl;	/* Waterline for low and high*/
+	struct hclge_waterline wl;	/* Waterline for low and high */
 	u32 buf_size;	/* TC private buffer size */
 	u32 tx_buf_size;
 	u32 enable;	/* Enable TC private buffer or not */
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_main.c b/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_main.c
index 2e1639eeae4d..30c98e0d12d4 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_main.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_main.c
@@ -3375,7 +3375,7 @@ static irqreturn_t hclge_misc_irq_handle(int irq, void *data)
 	hclge_enable_vector(&hdev->misc_vector, false);
 	event_cause = hclge_check_event_cause(hdev, &clearval);
 
-	/* vector 0 interrupt is shared with reset and mailbox source events.*/
+	/* vector 0 interrupt is shared with reset and mailbox source events. */
 	switch (event_cause) {
 	case HCLGE_VECTOR0_EVENT_ERR:
 		hclge_errhand_task_schedule(hdev);
-- 
2.34.1

