From 6b47ae6a2b6de16ce9d89f30012767f24b22f203 Mon Sep 17 00:00:00 2001
From: Hao Lan <lanhao@huawei.com>
Date: Thu, 25 May 2023 00:22:46 +0800
Subject: [PATCH 237/283] net: hns3: fix the imp capability bit cannot exceed
 32 bits issue

driver inclusion
category: bugfix
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EN49
CVE: NA

----------------------------------------------------------------------

Current only the first 32 bits of the capability flag bit are considered.
When the matching capability flag bit is greater than 31 bits,
it will get an error bit.This patch use bitmap to solve this issue.
It can handle each capability bit whitout bit width limit.

Fixes: da77aef9cc58 ("net: hns3: create common cmdq resource allocate/free/query APIs")
Signed-off-by: Hao Lan <lanhao@huawei.com>
(cherry picked from commit 702c687cf9c1a8da10769f2dd4adb4b97e7b868b)
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>

 Conflicts:
	drivers/net/ethernet/hisilicon/hns3/hnae3.h
---
 drivers/net/ethernet/hisilicon/hns3/hnae3.h   |  3 ++-
 .../hns3/hns3_common/hclge_comm_cmd.c         | 21 ++++++++++++++++---
 2 files changed, 20 insertions(+), 4 deletions(-)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hnae3.h b/drivers/net/ethernet/hisilicon/hns3/hnae3.h
index ec9aa9233506..36a7285f68cf 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hnae3.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hnae3.h
@@ -30,6 +30,7 @@
 #include <linux/pci.h>
 #include <linux/pkt_sched.h>
 #include <linux/types.h>
+#include <linux/bitmap.h>
 #include <net/pkt_cls.h>
 
 #define HNAE3_MOD_VERSION "24.3.1"
@@ -428,7 +429,7 @@ struct hnae3_ae_dev {
 #ifndef __GENKSYMS__
 	struct hnae3_dev_specs dev_specs;
 	u32 dev_version;
-	unsigned long caps[BITS_TO_LONGS(HNAE3_DEV_CAPS_MAX_NUM)];
+	DECLARE_BITMAP(caps, HNAE3_DEV_CAPS_MAX_NUM);
 #endif
 	void *priv;
 };
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c b/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c
index c4d647519977..a3ed8e531b25 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c
@@ -173,6 +173,20 @@ static const struct hclge_comm_caps_bit_map hclge_vf_cmd_caps[] = {
 	{HCLGE_COMM_CAP_GRO_B, HNAE3_DEV_SUPPORT_GRO_B},
 };
 
+static void
+hclge_comm_capability_to_bitmap(unsigned long *bitmap, __le32 *caps)
+{
+	const unsigned int words = HCLGE_COMM_QUERY_CAP_LENGTH;
+	u32 val[HCLGE_COMM_QUERY_CAP_LENGTH];
+	unsigned int i;
+
+	for (i = 0; i < words; i++)
+		val[i] = __le32_to_cpu(caps[i]);
+
+	bitmap_from_arr32(bitmap, val,
+			  HCLGE_COMM_QUERY_CAP_LENGTH * BITS_PER_TYPE(u32));
+}
+
 static void
 hclge_comm_parse_capability(struct hnae3_ae_dev *ae_dev, bool is_pf,
 			    struct hclge_comm_query_version_cmd *cmd)
@@ -181,11 +195,12 @@ hclge_comm_parse_capability(struct hnae3_ae_dev *ae_dev, bool is_pf,
 				is_pf ? hclge_pf_cmd_caps : hclge_vf_cmd_caps;
 	u32 size = is_pf ? ARRAY_SIZE(hclge_pf_cmd_caps) :
 				ARRAY_SIZE(hclge_vf_cmd_caps);
-	u32 caps, i;
+	DECLARE_BITMAP(caps, HCLGE_COMM_QUERY_CAP_LENGTH * BITS_PER_TYPE(u32));
+	u32 i;
 
-	caps = __le32_to_cpu(cmd->caps[0]);
+	hclge_comm_capability_to_bitmap(caps, cmd->caps);
 	for (i = 0; i < size; i++)
-		if (hnae3_get_bit(caps, caps_map[i].imp_bit))
+		if (test_bit(caps_map[i].imp_bit, caps))
 			set_bit(caps_map[i].local_bit, ae_dev->caps);
 }
 
-- 
2.34.1

