From 7901f6e0c3c188badd67a49ba546df8da2f0a123 Mon Sep 17 00:00:00 2001
From: Qi Liu <liuqi115@huawei.com>
Date: Thu, 16 Jul 2020 17:19:25 +0800
Subject: [PATCH 08/55] drivers/perf: Fix kernel panic when rmmod PMU modules
 during perf sampling

mainline inclusion
from mainline-v5.8-rc1
commit bdc5c744c7b6457d18a95c26769dad0e7f480a08
category: bugfix
bugzilla: https://gitee.com/openeuler/kernel/issues/I8AU2M

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=bdc5c744c7b6457d18a95c26769dad0e7f480a08

----------------------------------------------------------------------

When users try to remove PMU modules during perf sampling, kernel panic
will happen because the pmu->read() is a NULL pointer here.

INFO on HiSilicon hip08 platform as follow:
pc : hisi_uncore_pmu_event_update+0x30/0xa4 [hisi_uncore_pmu]
lr : hisi_uncore_pmu_read+0x20/0x2c [hisi_uncore_pmu]
sp : ffff800010103e90
x29: ffff800010103e90 x28: ffff0027db0c0e40
x27: ffffa29a76f129d8 x26: ffffa29a77ceb000
x25: ffffa29a773a5000 x24: ffffa29a77392000
x23: ffffddffe5943f08 x22: ffff002784285960
x21: ffff002784285800 x20: ffff0027d2e76c80
x19: ffff0027842859e0 x18: ffff80003498bcc8
x17: ffffa29a76afe910 x16: ffffa29a7583f530
x15: 16151a1512061a1e x14: 0000000000000000
x13: ffffa29a76f1e238 x12: 0000000000000001
x11: 0000000000000400 x10: 00000000000009f0
x9 : ffff8000107b3e70 x8 : ffff0027db0c1890
x7 : ffffa29a773a7000 x6 : 00000007f5131013
x5 : 00000007f5131013 x4 : 09f257d417c00000
x3 : 00000002187bd7ce x2 : ffffa29a38f0f0d8
x1 : ffffa29a38eae268 x0 : ffff0027d2e76c80
Call trace:
hisi_uncore_pmu_event_update+0x30/0xa4 [hisi_uncore_pmu]
hisi_uncore_pmu_read+0x20/0x2c [hisi_uncore_pmu]
__perf_event_read+0x1a0/0x1f8
flush_smp_call_function_queue+0xa0/0x160
generic_smp_call_function_single_interrupt+0x18/0x20
handle_IPI+0x31c/0x4dc
gic_handle_irq+0x2c8/0x310
el1_irq+0xcc/0x180
arch_cpu_idle+0x4c/0x20c
default_idle_call+0x20/0x30
do_idle+0x1b4/0x270
cpu_startup_entry+0x28/0x30
secondary_start_kernel+0x1a4/0x1fc

To solve the above issue, current module should be registered to kernel,
so that try_module_get() can be invoked when perf sampling starts. This
adds the reference counting of module and could prevent users from removing
modules during sampling.

Reported-by: Haifeng Wang <wang.wanghaifeng@huawei.com>
Signed-off-by: Qi Liu <liuqi115@huawei.com>
Reviewed-by: John Garry <john.garry@huawei.com>
Link: https://lore.kernel.org/r/1594891165-8228-1-git-send-email-liuqi115@huawei.com
Signed-off-by: Will Deacon <will@kernel.org>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>

 Conflicts:
	drivers/perf/fsl_imx8_ddr_perf.c
	drivers/perf/arm_smmuv3_pmu.c
---
 drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c | 1 +
 drivers/perf/hisilicon/hisi_uncore_hha_pmu.c  | 1 +
 drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c  | 1 +
 3 files changed, 3 insertions(+)

diff --git a/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c b/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c
index b3488ae1f2b8..620fa1345150 100644
--- a/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c
+++ b/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c
@@ -386,6 +386,7 @@ static int hisi_ddrc_pmu_probe(struct platform_device *pdev)
 			      ddrc_pmu->sccl_id, ddrc_pmu->index_id);
 	ddrc_pmu->pmu = (struct pmu) {
 		.name		= name,
+		.module		= THIS_MODULE,
 		.task_ctx_nr	= perf_invalid_context,
 		.event_init	= hisi_uncore_pmu_event_init,
 		.pmu_enable	= hisi_uncore_pmu_enable,
diff --git a/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c b/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c
index f0215d50d84d..33a0da941be2 100644
--- a/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c
+++ b/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c
@@ -397,6 +397,7 @@ static int hisi_hha_pmu_probe(struct platform_device *pdev)
 			      hha_pmu->sccl_id, hha_pmu->index_id);
 	hha_pmu->pmu = (struct pmu) {
 		.name		= name,
+		.module		= THIS_MODULE,
 		.task_ctx_nr	= perf_invalid_context,
 		.event_init	= hisi_uncore_pmu_event_init,
 		.pmu_enable	= hisi_uncore_pmu_enable,
diff --git a/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c b/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c
index 11563e29d983..92485f00dcc8 100644
--- a/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c
+++ b/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c
@@ -387,6 +387,7 @@ static int hisi_l3c_pmu_probe(struct platform_device *pdev)
 			      l3c_pmu->sccl_id, l3c_pmu->index_id);
 	l3c_pmu->pmu = (struct pmu) {
 		.name		= name,
+		.module		= THIS_MODULE,
 		.task_ctx_nr	= perf_invalid_context,
 		.event_init	= hisi_uncore_pmu_event_init,
 		.pmu_enable	= hisi_uncore_pmu_enable,
-- 
2.27.0

