From 143cb127cf1ed993e2540e5c43427e6e1ad8106e Mon Sep 17 00:00:00 2001
From: Jie Wang <wangjie125@huawei.com>
Date: Wed, 12 Jan 2022 15:16:52 +0800
Subject: [PATCH 246/283] net: hns3: create common cmdq resource
 allocate/free/query APIs

mainline inclusion
from mainline-v5.17-rc1
commit da77aef9cc58ed820097b3d905e9fa474d42dbd4
category: feature
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EN49
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=da77aef9cc58ed820097b3d905e9fa474d42dbd4

----------------------------------------------------------------------

The PF and VF cmdq module resource allocate/free/query APIs are almost the
same espect the suffixes of API names. These same implementations bring
double development and bugfix work.

This patch creates common cmdq resource allocate/free/query APIs called by
PF and VF cmdq init/uninit APIs. The next patch will use the new unified
APIs to replace init/uninit APIs.

Signed-off-by: Jie Wang <wangjie125@huawei.com>
Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Reviewed-by: Jian Shen <shenjian15@huawei.com>
Reviewed-by: Yue Haibing <yuehaibing@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>

 Conflicts:
	drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c
	drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.h
---
 .../hns3/hns3_common/hclge_comm_cmd.c         |  70 ++---
 .../hns3/hns3_common/hclge_comm_cmd.h         | 266 +++++++++++++++++-
 .../hisilicon/hns3/hns3pf/hclge_cmd.h         | 251 -----------------
 3 files changed, 292 insertions(+), 295 deletions(-)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c b/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c
index cdfce19de621..c96620269037 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.c
@@ -53,14 +53,47 @@ void hclge_comm_cmd_reuse_desc(struct hclge_desc *desc, bool is_read)
 static void hclge_comm_set_default_capability(struct hnae3_ae_dev *ae_dev,
 					      bool is_pf)
 {
+	set_bit(HNAE3_DEV_SUPPORT_FD_B, ae_dev->caps);
 	set_bit(HNAE3_DEV_SUPPORT_GRO_B, ae_dev->caps);
-	if (is_pf) {
-		set_bit(HNAE3_DEV_SUPPORT_FD_B, ae_dev->caps);
+	if (is_pf && ae_dev->dev_version == HNAE3_DEVICE_VERSION_V2) {
 		set_bit(HNAE3_DEV_SUPPORT_FEC_B, ae_dev->caps);
 		set_bit(HNAE3_DEV_SUPPORT_PAUSE_B, ae_dev->caps);
 	}
 }
 
+void hclge_comm_free_cmd_desc(struct hclge_comm_cmq_ring *ring)
+{
+	int size  = ring->desc_num * sizeof(struct hclge_desc);
+
+	if (!ring->desc)
+		return;
+
+	dma_free_coherent(&ring->pdev->dev, size,
+			  ring->desc, ring->desc_dma_addr);
+	ring->desc = NULL;
+}
+
+static int hclge_comm_alloc_cmd_desc(struct hclge_comm_cmq_ring *ring)
+{
+	int size  = ring->desc_num * sizeof(struct hclge_desc);
+
+	ring->desc = dma_alloc_coherent(&ring->pdev->dev,
+					size, &ring->desc_dma_addr, GFP_KERNEL);
+	if (!ring->desc)
+		return -ENOMEM;
+
+	return 0;
+}
+
+static __le32 hclge_comm_build_api_caps(void)
+{
+	u32 api_caps = 0;
+
+	hnae3_set_bit(api_caps, HCLGE_COMM_API_CAP_FLEX_RSS_TBL_B, 1);
+
+	return cpu_to_le32(api_caps);
+}
+
 void hclge_comm_cmd_setup_basic_desc(struct hclge_desc *desc,
 				     enum hclge_opcode_type opcode,
 				     bool is_read)
@@ -100,39 +133,6 @@ int hclge_comm_firmware_compat_config(struct hnae3_ae_dev *ae_dev,
 	return hclge_comm_cmd_send(hw, &desc, 1);
 }
 
-void hclge_comm_free_cmd_desc(struct hclge_comm_cmq_ring *ring)
-{
-	int size  = ring->desc_num * sizeof(struct hclge_desc);
-
-	if (!ring->desc)
-		return;
-
-	dma_free_coherent(&ring->pdev->dev, size,
-			  ring->desc, ring->desc_dma_addr);
-	ring->desc = NULL;
-}
-
-static int hclge_comm_alloc_cmd_desc(struct hclge_comm_cmq_ring *ring)
-{
-	int size  = ring->desc_num * sizeof(struct hclge_desc);
-
-	ring->desc = dma_alloc_coherent(&ring->pdev->dev,
-					size, &ring->desc_dma_addr, GFP_KERNEL);
-	if (!ring->desc)
-		return -ENOMEM;
-
-	return 0;
-}
-
-static __le32 hclge_comm_build_api_caps(void)
-{
-	u32 api_caps = 0;
-
-	hnae3_set_bit(api_caps, HCLGE_COMM_API_CAP_FLEX_RSS_TBL_B, 1);
-
-	return cpu_to_le32(api_caps);
-}
-
 static const struct hclge_comm_caps_bit_map hclge_pf_cmd_caps[] = {
 	{HCLGE_COMM_CAP_UDP_GSO_B, HNAE3_DEV_SUPPORT_UDP_GSO_B},
 	{HCLGE_COMM_CAP_PTP_B, HNAE3_DEV_SUPPORT_PTP_B},
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.h b/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.h
index 2b9c92a00049..393953e828af 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_cmd.h
@@ -57,8 +57,256 @@
 #define HCLGE_COMM_CMDQ_TX_TIMEOUT_DEFAULT	30000
 #define HCLGE_COMM_CMDQ_TX_TIMEOUT_500MS	500000
 
-enum hclge_opcode_type;
-
+enum hclge_opcode_type {
+	/* Generic commands */
+	HCLGE_OPC_QUERY_FW_VER		= 0x0001,
+	HCLGE_OPC_CFG_RST_TRIGGER	= 0x0020,
+	HCLGE_OPC_GBL_RST_STATUS	= 0x0021,
+	HCLGE_OPC_QUERY_FUNC_STATUS	= 0x0022,
+	HCLGE_OPC_QUERY_PF_RSRC		= 0x0023,
+	HCLGE_OPC_QUERY_VF_RSRC		= 0x0024,
+	HCLGE_OPC_GET_CFG_PARAM		= 0x0025,
+	HCLGE_OPC_PF_RST_DONE		= 0x0026,
+	HCLGE_OPC_QUERY_VF_RST_RDY	= 0x0027,
+
+	HCLGE_OPC_STATS_64_BIT		= 0x0030,
+	HCLGE_OPC_STATS_32_BIT		= 0x0031,
+	HCLGE_OPC_STATS_MAC		= 0x0032,
+	HCLGE_OPC_QUERY_MAC_REG_NUM	= 0x0033,
+	HCLGE_OPC_STATS_MAC_ALL		= 0x0034,
+
+	HCLGE_OPC_QUERY_REG_NUM		= 0x0040,
+	HCLGE_OPC_QUERY_32_BIT_REG	= 0x0041,
+	HCLGE_OPC_QUERY_64_BIT_REG	= 0x0042,
+	HCLGE_OPC_DFX_BD_NUM		= 0x0043,
+	HCLGE_OPC_DFX_BIOS_COMMON_REG	= 0x0044,
+	HCLGE_OPC_DFX_SSU_REG_0		= 0x0045,
+	HCLGE_OPC_DFX_SSU_REG_1		= 0x0046,
+	HCLGE_OPC_DFX_IGU_EGU_REG	= 0x0047,
+	HCLGE_OPC_DFX_RPU_REG_0		= 0x0048,
+	HCLGE_OPC_DFX_RPU_REG_1		= 0x0049,
+	HCLGE_OPC_DFX_NCSI_REG		= 0x004A,
+	HCLGE_OPC_DFX_RTC_REG		= 0x004B,
+	HCLGE_OPC_DFX_PPP_REG		= 0x004C,
+	HCLGE_OPC_DFX_RCB_REG		= 0x004D,
+	HCLGE_OPC_DFX_TQP_REG		= 0x004E,
+	HCLGE_OPC_DFX_SSU_REG_2		= 0x004F,
+
+	HCLGE_OPC_QUERY_DEV_SPECS	= 0x0050,
+
+	/* MAC command */
+	HCLGE_OPC_CONFIG_MAC_MODE	= 0x0301,
+	HCLGE_OPC_CONFIG_AN_MODE	= 0x0304,
+	HCLGE_OPC_QUERY_LINK_STATUS	= 0x0307,
+	HCLGE_OPC_CONFIG_MAX_FRM_SIZE	= 0x0308,
+	HCLGE_OPC_CONFIG_SPEED_DUP	= 0x0309,
+	HCLGE_OPC_QUERY_MAC_TNL_INT	= 0x0310,
+	HCLGE_OPC_MAC_TNL_INT_EN	= 0x0311,
+	HCLGE_OPC_CLEAR_MAC_TNL_INT	= 0x0312,
+	HCLGE_OPC_COMMON_LOOPBACK       = 0x0315,
+	HCLGE_OPC_QUERY_FEC_STATS       = 0x0316,
+	HCLGE_OPC_CONFIG_FEC_MODE	= 0x031A,
+	/* check sum command */
+	HCLGE_OPC_CFG_CHECKSUM_EN       = 0x0601,
+
+	/* PTP commands */
+	HCLGE_OPC_PTP_INT_EN		= 0x0501,
+	HCLGE_OPC_PTP_MODE_CFG		= 0x0507,
+
+	/* PFC/Pause commands */
+	HCLGE_OPC_CFG_MAC_PAUSE_EN      = 0x0701,
+	HCLGE_OPC_CFG_PFC_PAUSE_EN      = 0x0702,
+	HCLGE_OPC_CFG_MAC_PARA          = 0x0703,
+	HCLGE_OPC_CFG_PFC_PARA          = 0x0704,
+	HCLGE_OPC_QUERY_MAC_TX_PKT_CNT  = 0x0705,
+	HCLGE_OPC_QUERY_MAC_RX_PKT_CNT  = 0x0706,
+	HCLGE_OPC_QUERY_PFC_TX_PKT_CNT  = 0x0707,
+	HCLGE_OPC_QUERY_PFC_RX_PKT_CNT  = 0x0708,
+	HCLGE_OPC_PRI_TO_TC_MAPPING     = 0x0709,
+	HCLGE_OPC_QOS_MAP               = 0x070A,
+
+	/* ETS/scheduler commands */
+	HCLGE_OPC_TM_PG_TO_PRI_LINK	= 0x0804,
+	HCLGE_OPC_TM_QS_TO_PRI_LINK     = 0x0805,
+	HCLGE_OPC_TM_NQ_TO_QS_LINK      = 0x0806,
+	HCLGE_OPC_TM_RQ_TO_QS_LINK      = 0x0807,
+	HCLGE_OPC_TM_PORT_WEIGHT        = 0x0808,
+	HCLGE_OPC_TM_PG_WEIGHT          = 0x0809,
+	HCLGE_OPC_TM_QS_WEIGHT          = 0x080A,
+	HCLGE_OPC_TM_PRI_WEIGHT         = 0x080B,
+	HCLGE_OPC_TM_PRI_C_SHAPPING     = 0x080C,
+	HCLGE_OPC_TM_PRI_P_SHAPPING     = 0x080D,
+	HCLGE_OPC_TM_PG_C_SHAPPING      = 0x080E,
+	HCLGE_OPC_TM_PG_P_SHAPPING      = 0x080F,
+	HCLGE_OPC_TM_PORT_SHAPPING      = 0x0810,
+	HCLGE_OPC_TM_PG_SCH_MODE_CFG    = 0x0812,
+	HCLGE_OPC_TM_PRI_SCH_MODE_CFG   = 0x0813,
+	HCLGE_OPC_TM_QS_SCH_MODE_CFG    = 0x0814,
+	HCLGE_OPC_TM_BP_TO_QSET_MAPPING = 0x0815,
+	HCLGE_OPC_TM_NODES		= 0x0816,
+	HCLGE_OPC_ETS_TC_WEIGHT		= 0x0843,
+	HCLGE_OPC_QSET_DFX_STS		= 0x0844,
+	HCLGE_OPC_PRI_DFX_STS		= 0x0845,
+	HCLGE_OPC_PG_DFX_STS		= 0x0846,
+	HCLGE_OPC_PORT_DFX_STS		= 0x0847,
+	HCLGE_OPC_SCH_NQ_CNT		= 0x0848,
+	HCLGE_OPC_SCH_RQ_CNT		= 0x0849,
+	HCLGE_OPC_TM_INTERNAL_STS	= 0x0850,
+	HCLGE_OPC_TM_INTERNAL_CNT	= 0x0851,
+	HCLGE_OPC_TM_INTERNAL_STS_1	= 0x0852,
+	HCLGE_OPC_TM_FLUSH		= 0x0872,
+
+	/* Packet buffer allocate commands */
+	HCLGE_OPC_TX_BUFF_ALLOC		= 0x0901,
+	HCLGE_OPC_RX_PRIV_BUFF_ALLOC	= 0x0902,
+	HCLGE_OPC_RX_PRIV_WL_ALLOC	= 0x0903,
+	HCLGE_OPC_RX_COM_THRD_ALLOC	= 0x0904,
+	HCLGE_OPC_RX_COM_WL_ALLOC	= 0x0905,
+	HCLGE_OPC_RX_GBL_PKT_CNT	= 0x0906,
+
+	/* TQP management command */
+	HCLGE_OPC_SET_TQP_MAP		= 0x0A01,
+
+	/* TQP commands */
+	HCLGE_OPC_CFG_TX_QUEUE		= 0x0B01,
+	HCLGE_OPC_QUERY_TX_POINTER	= 0x0B02,
+	HCLGE_OPC_QUERY_TX_STATS	= 0x0B03,
+	HCLGE_OPC_TQP_TX_QUEUE_TC	= 0x0B04,
+	HCLGE_OPC_CFG_RX_QUEUE		= 0x0B11,
+	HCLGE_OPC_QUERY_RX_POINTER	= 0x0B12,
+	HCLGE_OPC_QUERY_RX_STATS	= 0x0B13,
+	HCLGE_OPC_STASH_RX_QUEUE_LRO	= 0x0B16,
+	HCLGE_OPC_CFG_RX_QUEUE_LRO	= 0x0B17,
+	HCLGE_OPC_CFG_COM_TQP_QUEUE	= 0x0B20,
+	HCLGE_OPC_RESET_TQP_QUEUE	= 0x0B22,
+
+	/* PPU commands */
+	HCLGE_OPC_PPU_PF_OTHER_INT_DFX	= 0x0B4A,
+
+	/* TSO command */
+	HCLGE_OPC_TSO_GENERIC_CONFIG	= 0x0C01,
+	HCLGE_OPC_GRO_GENERIC_CONFIG    = 0x0C10,
+
+	/* RSS commands */
+	HCLGE_OPC_RSS_GENERIC_CONFIG	= 0x0D01,
+	HCLGE_OPC_RSS_INDIR_TABLE	= 0x0D07,
+	HCLGE_OPC_RSS_TC_MODE		= 0x0D08,
+	HCLGE_OPC_RSS_INPUT_TUPLE	= 0x0D02,
+
+	/* Promisuous mode command */
+	HCLGE_OPC_CFG_PROMISC_MODE	= 0x0E01,
+
+	/* Vlan offload commands */
+	HCLGE_OPC_VLAN_PORT_TX_CFG	= 0x0F01,
+	HCLGE_OPC_VLAN_PORT_RX_CFG	= 0x0F02,
+
+	/* Interrupts commands */
+	HCLGE_OPC_ADD_RING_TO_VECTOR	= 0x1503,
+	HCLGE_OPC_DEL_RING_TO_VECTOR	= 0x1504,
+
+	/* MAC commands */
+	HCLGE_OPC_MAC_VLAN_ADD		    = 0x1000,
+	HCLGE_OPC_MAC_VLAN_REMOVE	    = 0x1001,
+	HCLGE_OPC_MAC_VLAN_TYPE_ID	    = 0x1002,
+	HCLGE_OPC_MAC_VLAN_INSERT	    = 0x1003,
+	HCLGE_OPC_MAC_VLAN_ALLOCATE	    = 0x1004,
+	HCLGE_OPC_MAC_ETHTYPE_ADD	    = 0x1010,
+	HCLGE_OPC_MAC_ETHTYPE_REMOVE	= 0x1011,
+
+	/* MAC VLAN commands */
+	HCLGE_OPC_MAC_VLAN_SWITCH_PARAM	= 0x1033,
+
+	/* VLAN commands */
+	HCLGE_OPC_VLAN_FILTER_CTRL	    = 0x1100,
+	HCLGE_OPC_VLAN_FILTER_PF_CFG	= 0x1101,
+	HCLGE_OPC_VLAN_FILTER_VF_CFG	= 0x1102,
+
+	/* Flow Director commands */
+	HCLGE_OPC_FD_MODE_CTRL		= 0x1200,
+	HCLGE_OPC_FD_GET_ALLOCATION	= 0x1201,
+	HCLGE_OPC_FD_KEY_CONFIG		= 0x1202,
+	HCLGE_OPC_FD_TCAM_OP		= 0x1203,
+	HCLGE_OPC_FD_AD_OP		= 0x1204,
+	HCLGE_OPC_FD_CNT_OP		= 0x1205,
+	HCLGE_OPC_FD_USER_DEF_OP	= 0x1207,
+	HCLGE_OPC_FD_QB_CTRL		= 0x1210,
+	HCLGE_OPC_FD_QB_AD_OP		= 0x1211,
+
+	/* MDIO command */
+	HCLGE_OPC_MDIO_CONFIG		= 0x1900,
+
+	/* QCN commands */
+	HCLGE_OPC_QCN_MOD_CFG		= 0x1A01,
+	HCLGE_OPC_QCN_GRP_TMPLT_CFG	= 0x1A02,
+	HCLGE_OPC_QCN_SHAPPING_CFG	= 0x1A03,
+	HCLGE_OPC_QCN_SHAPPING_BS_CFG	= 0x1A04,
+	HCLGE_OPC_QCN_QSET_LINK_CFG	= 0x1A05,
+	HCLGE_OPC_QCN_RP_STATUS_GET	= 0x1A06,
+	HCLGE_OPC_QCN_AJUST_INIT	= 0x1A07,
+	HCLGE_OPC_QCN_DFX_CNT_STATUS    = 0x1A08,
+
+	/* Mailbox command */
+	HCLGEVF_OPC_MBX_PF_TO_VF	= 0x2000,
+
+	/* Led command */
+	HCLGE_OPC_LED_STATUS_CFG	= 0xB000,
+
+	/* clear hardware resource command */
+	HCLGE_OPC_CLEAR_HW_RESOURCE	= 0x700B,
+
+	/* NCL config command */
+	HCLGE_OPC_QUERY_NCL_CONFIG	= 0x7011,
+
+	/* IMP stats command */
+	HCLGE_OPC_IMP_STATS_BD		= 0x7012,
+	HCLGE_OPC_IMP_STATS_INFO		= 0x7013,
+	HCLGE_OPC_IMP_COMPAT_CFG		= 0x701A,
+
+	/* SFP command */
+	HCLGE_OPC_GET_SFP_EEPROM	= 0x7100,
+	HCLGE_OPC_GET_SFP_EXIST		= 0x7101,
+	HCLGE_OPC_GET_SFP_INFO		= 0x7104,
+
+	/* Error INT commands */
+	HCLGE_MAC_COMMON_INT_EN		= 0x030E,
+	HCLGE_TM_SCH_ECC_INT_EN		= 0x0829,
+	HCLGE_SSU_ECC_INT_CMD		= 0x0989,
+	HCLGE_SSU_COMMON_INT_CMD	= 0x098C,
+	HCLGE_PPU_MPF_ECC_INT_CMD	= 0x0B40,
+	HCLGE_PPU_MPF_OTHER_INT_CMD	= 0x0B41,
+	HCLGE_PPU_PF_OTHER_INT_CMD	= 0x0B42,
+	HCLGE_COMMON_ECC_INT_CFG	= 0x1505,
+	HCLGE_QUERY_RAS_INT_STS_BD_NUM	= 0x1510,
+	HCLGE_QUERY_CLEAR_MPF_RAS_INT	= 0x1511,
+	HCLGE_QUERY_CLEAR_PF_RAS_INT	= 0x1512,
+	HCLGE_QUERY_MSIX_INT_STS_BD_NUM	= 0x1513,
+	HCLGE_QUERY_CLEAR_ALL_MPF_MSIX_INT	= 0x1514,
+	HCLGE_QUERY_CLEAR_ALL_PF_MSIX_INT	= 0x1515,
+	HCLGE_QUERY_ALL_ERR_BD_NUM		= 0x1516,
+	HCLGE_QUERY_ALL_ERR_INFO		= 0x1517,
+	HCLGE_CONFIG_ROCEE_RAS_INT_EN	= 0x1580,
+	HCLGE_QUERY_CLEAR_ROCEE_RAS_INT = 0x1581,
+	HCLGE_ROCEE_PF_RAS_INT_CMD	= 0x1584,
+	HCLGE_QUERY_ROCEE_ECC_RAS_INFO_CMD	= 0x1585,
+	HCLGE_QUERY_ROCEE_AXI_RAS_INFO_CMD	= 0x1586,
+	HCLGE_IGU_EGU_TNL_INT_EN	= 0x1803,
+	HCLGE_IGU_COMMON_INT_EN		= 0x1806,
+	HCLGE_TM_QCN_MEM_INT_CFG	= 0x1A14,
+	HCLGE_PPP_CMD0_INT_CMD		= 0x2100,
+	HCLGE_PPP_CMD1_INT_CMD		= 0x2101,
+	HCLGE_PPP_MAC_VLAN_IDX_RD	= 0x2104,
+	HCLGE_MAC_ETHERTYPE_IDX_RD      = 0x2105,
+	HCLGE_OPC_WOL_CFG               = 0x2200,
+	HCLGE_OPC_WOL_GET_SUPPORTED_MODE        = 0x2201,
+	HCLGE_NCSI_INT_EN		= 0x2401,
+
+	/* PHY command */
+	HCLGE_OPC_PHY_LINK_KSETTING	= 0x7025,
+	HCLGE_OPC_PHY_REG		= 0x7026,
+
+	/* Query link diagnosis info command */
+	HCLGE_OPC_QUERY_LINK_DIAGNOSIS	= 0x702A,
+};
 enum hclge_comm_cmd_return_status {
 	HCLGE_COMM_CMD_EXEC_SUCCESS	= 0,
 	HCLGE_COMM_CMD_NO_AUTH		= 1,
@@ -102,13 +350,18 @@ enum HCLGE_COMM_CAP_BITS {
 	HCLGE_COMM_CAP_TM_FLUSH_B = 31,
 };
 
+struct hclge_cmdq_tx_timeout_map {
+	u32 opcode;
+	u32 tx_timeout;
+};
+
 enum HCLGE_COMM_API_CAP_BITS {
 	HCLGE_COMM_API_CAP_FLEX_RSS_TBL_B,
 };
 
 enum hclge_comm_opcode_type {
-	HCLGE_COMM_OPC_QUERY_FW_VER             = 0x0001,
-	HCLGE_COMM_OPC_IMP_COMPAT_CFG           = 0x701A,
+	HCLGE_COMM_OPC_QUERY_FW_VER		= 0x0001,
+	HCLGE_COMM_OPC_IMP_COMPAT_CFG		= 0x701A,
 };
 
 /* capabilities bits map between imp firmware and local driver */
@@ -117,11 +370,6 @@ struct hclge_comm_caps_bit_map {
 	u16 local_bit;
 };
 
-struct hclge_cmdq_tx_timeout_map {
-	u32 opcode;
-	u32 tx_timeout;
-};
-
 struct hclge_comm_firmware_compat_cmd {
 	__le32 compat;
 	u8 rsv[20];
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h b/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h
index 1a980ba5e59d..c2b23b31690e 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_cmd.h
@@ -30,257 +30,6 @@ struct hclge_misc_vector {
 #define HCLGE_CMD_FLAG_NO_INTR	BIT(4)
 #define HCLGE_CMD_FLAG_ERR_INTR	BIT(5)
 
-enum hclge_opcode_type {
-	/* Generic commands */
-	HCLGE_OPC_QUERY_FW_VER		= 0x0001,
-	HCLGE_OPC_CFG_RST_TRIGGER	= 0x0020,
-	HCLGE_OPC_GBL_RST_STATUS	= 0x0021,
-	HCLGE_OPC_QUERY_FUNC_STATUS	= 0x0022,
-	HCLGE_OPC_QUERY_PF_RSRC		= 0x0023,
-	HCLGE_OPC_QUERY_VF_RSRC		= 0x0024,
-	HCLGE_OPC_GET_CFG_PARAM		= 0x0025,
-	HCLGE_OPC_PF_RST_DONE		= 0x0026,
-	HCLGE_OPC_QUERY_VF_RST_RDY	= 0x0027,
-
-	HCLGE_OPC_STATS_64_BIT		= 0x0030,
-	HCLGE_OPC_STATS_32_BIT		= 0x0031,
-	HCLGE_OPC_STATS_MAC		= 0x0032,
-	HCLGE_OPC_QUERY_MAC_REG_NUM	= 0x0033,
-	HCLGE_OPC_STATS_MAC_ALL		= 0x0034,
-
-	HCLGE_OPC_QUERY_REG_NUM		= 0x0040,
-	HCLGE_OPC_QUERY_32_BIT_REG	= 0x0041,
-	HCLGE_OPC_QUERY_64_BIT_REG	= 0x0042,
-	HCLGE_OPC_DFX_BD_NUM		= 0x0043,
-	HCLGE_OPC_DFX_BIOS_COMMON_REG	= 0x0044,
-	HCLGE_OPC_DFX_SSU_REG_0		= 0x0045,
-	HCLGE_OPC_DFX_SSU_REG_1		= 0x0046,
-	HCLGE_OPC_DFX_IGU_EGU_REG	= 0x0047,
-	HCLGE_OPC_DFX_RPU_REG_0		= 0x0048,
-	HCLGE_OPC_DFX_RPU_REG_1		= 0x0049,
-	HCLGE_OPC_DFX_NCSI_REG		= 0x004A,
-	HCLGE_OPC_DFX_RTC_REG		= 0x004B,
-	HCLGE_OPC_DFX_PPP_REG		= 0x004C,
-	HCLGE_OPC_DFX_RCB_REG		= 0x004D,
-	HCLGE_OPC_DFX_TQP_REG		= 0x004E,
-	HCLGE_OPC_DFX_SSU_REG_2		= 0x004F,
-
-	HCLGE_OPC_QUERY_DEV_SPECS	= 0x0050,
-
-	/* MAC command */
-	HCLGE_OPC_CONFIG_MAC_MODE	= 0x0301,
-	HCLGE_OPC_CONFIG_AN_MODE	= 0x0304,
-	HCLGE_OPC_QUERY_LINK_STATUS	= 0x0307,
-	HCLGE_OPC_CONFIG_MAX_FRM_SIZE	= 0x0308,
-	HCLGE_OPC_CONFIG_SPEED_DUP	= 0x0309,
-	HCLGE_OPC_QUERY_MAC_TNL_INT	= 0x0310,
-	HCLGE_OPC_MAC_TNL_INT_EN	= 0x0311,
-	HCLGE_OPC_CLEAR_MAC_TNL_INT	= 0x0312,
-	HCLGE_OPC_COMMON_LOOPBACK       = 0x0315,
-	HCLGE_OPC_QUERY_FEC_STATS       = 0x0316,
-	HCLGE_OPC_CONFIG_FEC_MODE	= 0x031A,
-	/* check sum command */
-	HCLGE_OPC_CFG_CHECKSUM_EN       = 0x0601,
-
-	/* PTP commands */
-	HCLGE_OPC_PTP_INT_EN		= 0x0501,
-	HCLGE_OPC_PTP_MODE_CFG		= 0x0507,
-
-	/* PFC/Pause commands */
-	HCLGE_OPC_CFG_MAC_PAUSE_EN      = 0x0701,
-	HCLGE_OPC_CFG_PFC_PAUSE_EN      = 0x0702,
-	HCLGE_OPC_CFG_MAC_PARA          = 0x0703,
-	HCLGE_OPC_CFG_PFC_PARA          = 0x0704,
-	HCLGE_OPC_QUERY_MAC_TX_PKT_CNT  = 0x0705,
-	HCLGE_OPC_QUERY_MAC_RX_PKT_CNT  = 0x0706,
-	HCLGE_OPC_QUERY_PFC_TX_PKT_CNT  = 0x0707,
-	HCLGE_OPC_QUERY_PFC_RX_PKT_CNT  = 0x0708,
-	HCLGE_OPC_PRI_TO_TC_MAPPING     = 0x0709,
-	HCLGE_OPC_QOS_MAP               = 0x070A,
-
-	/* ETS/scheduler commands */
-	HCLGE_OPC_TM_PG_TO_PRI_LINK	= 0x0804,
-	HCLGE_OPC_TM_QS_TO_PRI_LINK     = 0x0805,
-	HCLGE_OPC_TM_NQ_TO_QS_LINK      = 0x0806,
-	HCLGE_OPC_TM_RQ_TO_QS_LINK      = 0x0807,
-	HCLGE_OPC_TM_PORT_WEIGHT        = 0x0808,
-	HCLGE_OPC_TM_PG_WEIGHT          = 0x0809,
-	HCLGE_OPC_TM_QS_WEIGHT          = 0x080A,
-	HCLGE_OPC_TM_PRI_WEIGHT         = 0x080B,
-	HCLGE_OPC_TM_PRI_C_SHAPPING     = 0x080C,
-	HCLGE_OPC_TM_PRI_P_SHAPPING     = 0x080D,
-	HCLGE_OPC_TM_PG_C_SHAPPING      = 0x080E,
-	HCLGE_OPC_TM_PG_P_SHAPPING      = 0x080F,
-	HCLGE_OPC_TM_PORT_SHAPPING      = 0x0810,
-	HCLGE_OPC_TM_PG_SCH_MODE_CFG    = 0x0812,
-	HCLGE_OPC_TM_PRI_SCH_MODE_CFG   = 0x0813,
-	HCLGE_OPC_TM_QS_SCH_MODE_CFG    = 0x0814,
-	HCLGE_OPC_TM_BP_TO_QSET_MAPPING = 0x0815,
-	HCLGE_OPC_TM_NODES		= 0x0816,
-	HCLGE_OPC_ETS_TC_WEIGHT		= 0x0843,
-	HCLGE_OPC_QSET_DFX_STS		= 0x0844,
-	HCLGE_OPC_PRI_DFX_STS		= 0x0845,
-	HCLGE_OPC_PG_DFX_STS		= 0x0846,
-	HCLGE_OPC_PORT_DFX_STS		= 0x0847,
-	HCLGE_OPC_SCH_NQ_CNT		= 0x0848,
-	HCLGE_OPC_SCH_RQ_CNT		= 0x0849,
-	HCLGE_OPC_TM_INTERNAL_STS	= 0x0850,
-	HCLGE_OPC_TM_INTERNAL_CNT	= 0x0851,
-	HCLGE_OPC_TM_INTERNAL_STS_1	= 0x0852,
-	HCLGE_OPC_TM_FLUSH		= 0x0872,
-
-	/* Packet buffer allocate commands */
-	HCLGE_OPC_TX_BUFF_ALLOC		= 0x0901,
-	HCLGE_OPC_RX_PRIV_BUFF_ALLOC	= 0x0902,
-	HCLGE_OPC_RX_PRIV_WL_ALLOC	= 0x0903,
-	HCLGE_OPC_RX_COM_THRD_ALLOC	= 0x0904,
-	HCLGE_OPC_RX_COM_WL_ALLOC	= 0x0905,
-	HCLGE_OPC_RX_GBL_PKT_CNT	= 0x0906,
-
-	/* TQP management command */
-	HCLGE_OPC_SET_TQP_MAP		= 0x0A01,
-
-	/* TQP commands */
-	HCLGE_OPC_CFG_TX_QUEUE		= 0x0B01,
-	HCLGE_OPC_QUERY_TX_POINTER	= 0x0B02,
-	HCLGE_OPC_QUERY_TX_STATS	= 0x0B03,
-	HCLGE_OPC_TQP_TX_QUEUE_TC	= 0x0B04,
-	HCLGE_OPC_CFG_RX_QUEUE		= 0x0B11,
-	HCLGE_OPC_QUERY_RX_POINTER	= 0x0B12,
-	HCLGE_OPC_QUERY_RX_STATS	= 0x0B13,
-	HCLGE_OPC_STASH_RX_QUEUE_LRO	= 0x0B16,
-	HCLGE_OPC_CFG_RX_QUEUE_LRO	= 0x0B17,
-	HCLGE_OPC_CFG_COM_TQP_QUEUE	= 0x0B20,
-	HCLGE_OPC_RESET_TQP_QUEUE	= 0x0B22,
-
-	/* PPU commands */
-	HCLGE_OPC_PPU_PF_OTHER_INT_DFX	= 0x0B4A,
-
-	/* TSO command */
-	HCLGE_OPC_TSO_GENERIC_CONFIG	= 0x0C01,
-	HCLGE_OPC_GRO_GENERIC_CONFIG    = 0x0C10,
-
-	/* RSS commands */
-	HCLGE_OPC_RSS_GENERIC_CONFIG	= 0x0D01,
-	HCLGE_OPC_RSS_INDIR_TABLE	= 0x0D07,
-	HCLGE_OPC_RSS_TC_MODE		= 0x0D08,
-	HCLGE_OPC_RSS_INPUT_TUPLE	= 0x0D02,
-
-	/* Promisuous mode command */
-	HCLGE_OPC_CFG_PROMISC_MODE	= 0x0E01,
-
-	/* Vlan offload commands */
-	HCLGE_OPC_VLAN_PORT_TX_CFG	= 0x0F01,
-	HCLGE_OPC_VLAN_PORT_RX_CFG	= 0x0F02,
-
-	/* Interrupts commands */
-	HCLGE_OPC_ADD_RING_TO_VECTOR	= 0x1503,
-	HCLGE_OPC_DEL_RING_TO_VECTOR	= 0x1504,
-
-	/* MAC commands */
-	HCLGE_OPC_MAC_VLAN_ADD		    = 0x1000,
-	HCLGE_OPC_MAC_VLAN_REMOVE	    = 0x1001,
-	HCLGE_OPC_MAC_VLAN_TYPE_ID	    = 0x1002,
-	HCLGE_OPC_MAC_VLAN_INSERT	    = 0x1003,
-	HCLGE_OPC_MAC_VLAN_ALLOCATE	    = 0x1004,
-	HCLGE_OPC_MAC_ETHTYPE_ADD	    = 0x1010,
-	HCLGE_OPC_MAC_ETHTYPE_REMOVE	= 0x1011,
-
-	/* MAC VLAN commands */
-	HCLGE_OPC_MAC_VLAN_SWITCH_PARAM	= 0x1033,
-
-	/* VLAN commands */
-	HCLGE_OPC_VLAN_FILTER_CTRL	    = 0x1100,
-	HCLGE_OPC_VLAN_FILTER_PF_CFG	= 0x1101,
-	HCLGE_OPC_VLAN_FILTER_VF_CFG	= 0x1102,
-
-	/* Flow Director commands */
-	HCLGE_OPC_FD_MODE_CTRL		= 0x1200,
-	HCLGE_OPC_FD_GET_ALLOCATION	= 0x1201,
-	HCLGE_OPC_FD_KEY_CONFIG		= 0x1202,
-	HCLGE_OPC_FD_TCAM_OP		= 0x1203,
-	HCLGE_OPC_FD_AD_OP		= 0x1204,
-	HCLGE_OPC_FD_CNT_OP		= 0x1205,
-	HCLGE_OPC_FD_USER_DEF_OP	= 0x1207,
-	HCLGE_OPC_FD_QB_CTRL		= 0x1210,
-	HCLGE_OPC_FD_QB_AD_OP		= 0x1211,
-
-	/* MDIO command */
-	HCLGE_OPC_MDIO_CONFIG		= 0x1900,
-
-	/* QCN commands */
-	HCLGE_OPC_QCN_MOD_CFG		= 0x1A01,
-	HCLGE_OPC_QCN_GRP_TMPLT_CFG	= 0x1A02,
-	HCLGE_OPC_QCN_SHAPPING_CFG	= 0x1A03,
-	HCLGE_OPC_QCN_SHAPPING_BS_CFG	= 0x1A04,
-	HCLGE_OPC_QCN_QSET_LINK_CFG	= 0x1A05,
-	HCLGE_OPC_QCN_RP_STATUS_GET	= 0x1A06,
-	HCLGE_OPC_QCN_AJUST_INIT	= 0x1A07,
-	HCLGE_OPC_QCN_DFX_CNT_STATUS    = 0x1A08,
-
-	/* Mailbox command */
-	HCLGEVF_OPC_MBX_PF_TO_VF	= 0x2000,
-
-	/* Led command */
-	HCLGE_OPC_LED_STATUS_CFG	= 0xB000,
-
-	/* clear hardware resource command */
-	HCLGE_OPC_CLEAR_HW_RESOURCE	= 0x700B,
-
-	/* NCL config command */
-	HCLGE_OPC_QUERY_NCL_CONFIG	= 0x7011,
-
-	/* IMP stats command */
-	HCLGE_OPC_IMP_STATS_BD		= 0x7012,
-	HCLGE_OPC_IMP_STATS_INFO		= 0x7013,
-	HCLGE_OPC_IMP_COMPAT_CFG		= 0x701A,
-
-	/* SFP command */
-	HCLGE_OPC_GET_SFP_EEPROM	= 0x7100,
-	HCLGE_OPC_GET_SFP_EXIST		= 0x7101,
-	HCLGE_OPC_GET_SFP_INFO		= 0x7104,
-
-	/* Error INT commands */
-	HCLGE_MAC_COMMON_INT_EN		= 0x030E,
-	HCLGE_TM_SCH_ECC_INT_EN		= 0x0829,
-	HCLGE_SSU_ECC_INT_CMD		= 0x0989,
-	HCLGE_SSU_COMMON_INT_CMD	= 0x098C,
-	HCLGE_PPU_MPF_ECC_INT_CMD	= 0x0B40,
-	HCLGE_PPU_MPF_OTHER_INT_CMD	= 0x0B41,
-	HCLGE_PPU_PF_OTHER_INT_CMD	= 0x0B42,
-	HCLGE_COMMON_ECC_INT_CFG	= 0x1505,
-	HCLGE_QUERY_RAS_INT_STS_BD_NUM	= 0x1510,
-	HCLGE_QUERY_CLEAR_MPF_RAS_INT	= 0x1511,
-	HCLGE_QUERY_CLEAR_PF_RAS_INT	= 0x1512,
-	HCLGE_QUERY_MSIX_INT_STS_BD_NUM	= 0x1513,
-	HCLGE_QUERY_CLEAR_ALL_MPF_MSIX_INT	= 0x1514,
-	HCLGE_QUERY_CLEAR_ALL_PF_MSIX_INT	= 0x1515,
-	HCLGE_QUERY_ALL_ERR_BD_NUM		= 0x1516,
-	HCLGE_QUERY_ALL_ERR_INFO		= 0x1517,
-	HCLGE_CONFIG_ROCEE_RAS_INT_EN	= 0x1580,
-	HCLGE_QUERY_CLEAR_ROCEE_RAS_INT = 0x1581,
-	HCLGE_ROCEE_PF_RAS_INT_CMD	= 0x1584,
-	HCLGE_QUERY_ROCEE_ECC_RAS_INFO_CMD	= 0x1585,
-	HCLGE_QUERY_ROCEE_AXI_RAS_INFO_CMD	= 0x1586,
-	HCLGE_IGU_EGU_TNL_INT_EN	= 0x1803,
-	HCLGE_IGU_COMMON_INT_EN		= 0x1806,
-	HCLGE_TM_QCN_MEM_INT_CFG	= 0x1A14,
-	HCLGE_PPP_CMD0_INT_CMD		= 0x2100,
-	HCLGE_PPP_CMD1_INT_CMD		= 0x2101,
-	HCLGE_PPP_MAC_VLAN_IDX_RD	= 0x2104,
-	HCLGE_MAC_ETHERTYPE_IDX_RD      = 0x2105,
-	HCLGE_OPC_WOL_CFG               = 0x2200,
-	HCLGE_OPC_WOL_GET_SUPPORTED_MODE        = 0x2201,
-	HCLGE_NCSI_INT_EN		= 0x2401,
-
-	/* PHY command */
-	HCLGE_OPC_PHY_LINK_KSETTING	= 0x7025,
-	HCLGE_OPC_PHY_REG		= 0x7026,
-
-	/* Query link diagnosis info command */
-	HCLGE_OPC_QUERY_LINK_DIAGNOSIS	= 0x702A,
-};
-
 #define HCLGE_TQP_REG_OFFSET		0x80000
 #define HCLGE_TQP_REG_SIZE		0x200
 
-- 
2.34.1

