From 218242a0d5c4f6c0eb1b933e8af7d61ab109dd2f Mon Sep 17 00:00:00 2001
From: Guangbin Huang <huangguangbin2@huawei.com>
Date: Sat, 21 Aug 2021 17:00:38 +0800
Subject: [PATCH 098/283] docs: ethtool: Add two link extended substates of bad
 signal integrity

mainline inclusion
from mainline-v5.15-rc1
commit 958ab281eb3e0543a995457fd2d9cb4504cde4b8
category: feature
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EMYT
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=958ab281eb3e0543a995457fd2d9cb4504cde4b8

----------------------------------------------------------------------

Add documentation for two bad signal integrity substates:
ETHTOOL_LINK_EXT_SUBSTATE_BSI_SERDES_REFERENCE_CLOCK_LOST
ETHTOOL_LINK_EXT_SUBSTATE_BSI_SERDES_ALOS.

Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
Reviewed-by: Yongxin Li <liyongxin1@huawei.com>
Signed-off-by: Junxin Chen <chenjunxin1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>

 Conflicts:
	Documentation/networking/ethtool-netlink.rst
---
 Documentation/networking/ethtool-netlink.rst | 1388 ++++++++++++++++++
 1 file changed, 1388 insertions(+)
 create mode 100644 Documentation/networking/ethtool-netlink.rst

diff --git a/Documentation/networking/ethtool-netlink.rst b/Documentation/networking/ethtool-netlink.rst
new file mode 100644
index 000000000000..f7b88ee9227d
--- /dev/null
+++ b/Documentation/networking/ethtool-netlink.rst
@@ -0,0 +1,1388 @@
+=============================
+Netlink interface for ethtool
+=============================
+
+
+Basic information
+=================
+
+Netlink interface for ethtool uses generic netlink family ``ethtool``
+(userspace application should use macros ``ETHTOOL_GENL_NAME`` and
+``ETHTOOL_GENL_VERSION`` defined in ``<linux/ethtool_netlink.h>`` uapi
+header). This family does not use a specific header, all information in
+requests and replies is passed using netlink attributes.
+
+The ethtool netlink interface uses extended ACK for error and warning
+reporting, userspace application developers are encouraged to make these
+messages available to user in a suitable way.
+
+Requests can be divided into three categories: "get" (retrieving information),
+"set" (setting parameters) and "action" (invoking an action).
+
+All "set" and "action" type requests require admin privileges
+(``CAP_NET_ADMIN`` in the namespace). Most "get" type requests are allowed for
+anyone but there are exceptions (where the response contains sensitive
+information). In some cases, the request as such is allowed for anyone but
+unprivileged users have attributes with sensitive information (e.g.
+wake-on-lan password) omitted.
+
+
+Conventions
+===========
+
+Attributes which represent a boolean value usually use NLA_U8 type so that we
+can distinguish three states: "on", "off" and "not present" (meaning the
+information is not available in "get" requests or value is not to be changed
+in "set" requests). For these attributes, the "true" value should be passed as
+number 1 but any non-zero value should be understood as "true" by recipient.
+In the tables below, "bool" denotes NLA_U8 attributes interpreted in this way.
+
+In the message structure descriptions below, if an attribute name is suffixed
+with "+", parent nest can contain multiple attributes of the same type. This
+implements an array of entries.
+
+
+Request header
+==============
+
+Each request or reply message contains a nested attribute with common header.
+Structure of this header is
+
+  ==============================  ======  =============================
+  ``ETHTOOL_A_HEADER_DEV_INDEX``  u32     device ifindex
+  ``ETHTOOL_A_HEADER_DEV_NAME``   string  device name
+  ``ETHTOOL_A_HEADER_FLAGS``      u32     flags common for all requests
+  ==============================  ======  =============================
+
+``ETHTOOL_A_HEADER_DEV_INDEX`` and ``ETHTOOL_A_HEADER_DEV_NAME`` identify the
+device message relates to. One of them is sufficient in requests, if both are
+used, they must identify the same device. Some requests, e.g. global string
+sets, do not require device identification. Most ``GET`` requests also allow
+dump requests without device identification to query the same information for
+all devices providing it (each device in a separate message).
+
+``ETHTOOL_A_HEADER_FLAGS`` is a bitmap of request flags common for all request
+types. The interpretation of these flags is the same for all request types but
+the flags may not apply to requests. Recognized flags are:
+
+  =================================  ===================================
+  ``ETHTOOL_FLAG_COMPACT_BITSETS``   use compact format bitsets in reply
+  ``ETHTOOL_FLAG_OMIT_REPLY``        omit optional reply (_SET and _ACT)
+  ``ETHTOOL_FLAG_STATS``             include optional device statistics
+  =================================  ===================================
+
+New request flags should follow the general idea that if the flag is not set,
+the behaviour is backward compatible, i.e. requests from old clients not aware
+of the flag should be interpreted the way the client expects. A client must
+not set flags it does not understand.
+
+
+Bit sets
+========
+
+For short bitmaps of (reasonably) fixed length, standard ``NLA_BITFIELD32``
+type is used. For arbitrary length bitmaps, ethtool netlink uses a nested
+attribute with contents of one of two forms: compact (two binary bitmaps
+representing bit values and mask of affected bits) and bit-by-bit (list of
+bits identified by either index or name).
+
+Verbose (bit-by-bit) bitsets allow sending symbolic names for bits together
+with their values which saves a round trip (when the bitset is passed in a
+request) or at least a second request (when the bitset is in a reply). This is
+useful for one shot applications like traditional ethtool command. On the
+other hand, long running applications like ethtool monitor (displaying
+notifications) or network management daemons may prefer fetching the names
+only once and using compact form to save message size. Notifications from
+ethtool netlink interface always use compact form for bitsets.
+
+A bitset can represent either a value/mask pair (``ETHTOOL_A_BITSET_NOMASK``
+not set) or a single bitmap (``ETHTOOL_A_BITSET_NOMASK`` set). In requests
+modifying a bitmap, the former changes the bit set in mask to values set in
+value and preserves the rest; the latter sets the bits set in the bitmap and
+clears the rest.
+
+Compact form: nested (bitset) atrribute contents:
+
+  ============================  ======  ============================
+  ``ETHTOOL_A_BITSET_NOMASK``   flag    no mask, only a list
+  ``ETHTOOL_A_BITSET_SIZE``     u32     number of significant bits
+  ``ETHTOOL_A_BITSET_VALUE``    binary  bitmap of bit values
+  ``ETHTOOL_A_BITSET_MASK``     binary  bitmap of valid bits
+  ============================  ======  ============================
+
+Value and mask must have length at least ``ETHTOOL_A_BITSET_SIZE`` bits
+rounded up to a multiple of 32 bits. They consist of 32-bit words in host byte
+order, words ordered from least significant to most significant (i.e. the same
+way as bitmaps are passed with ioctl interface).
+
+For compact form, ``ETHTOOL_A_BITSET_SIZE`` and ``ETHTOOL_A_BITSET_VALUE`` are
+mandatory. ``ETHTOOL_A_BITSET_MASK`` attribute is mandatory if
+``ETHTOOL_A_BITSET_NOMASK`` is not set (bitset represents a value/mask pair);
+if ``ETHTOOL_A_BITSET_NOMASK`` is not set, ``ETHTOOL_A_BITSET_MASK`` is not
+allowed (bitset represents a single bitmap.
+
+Kernel bit set length may differ from userspace length if older application is
+used on newer kernel or vice versa. If userspace bitmap is longer, an error is
+issued only if the request actually tries to set values of some bits not
+recognized by kernel.
+
+Bit-by-bit form: nested (bitset) attribute contents:
+
+ +------------------------------------+--------+-----------------------------+
+ | ``ETHTOOL_A_BITSET_NOMASK``        | flag   | no mask, only a list        |
+ +------------------------------------+--------+-----------------------------+
+ | ``ETHTOOL_A_BITSET_SIZE``          | u32    | number of significant bits  |
+ +------------------------------------+--------+-----------------------------+
+ | ``ETHTOOL_A_BITSET_BITS``          | nested | array of bits               |
+ +-+----------------------------------+--------+-----------------------------+
+ | | ``ETHTOOL_A_BITSET_BITS_BIT+``   | nested | one bit                     |
+ +-+-+--------------------------------+--------+-----------------------------+
+ | | | ``ETHTOOL_A_BITSET_BIT_INDEX`` | u32    | bit index (0 for LSB)       |
+ +-+-+--------------------------------+--------+-----------------------------+
+ | | | ``ETHTOOL_A_BITSET_BIT_NAME``  | string | bit name                    |
+ +-+-+--------------------------------+--------+-----------------------------+
+ | | | ``ETHTOOL_A_BITSET_BIT_VALUE`` | flag   | present if bit is set       |
+ +-+-+--------------------------------+--------+-----------------------------+
+
+Bit size is optional for bit-by-bit form. ``ETHTOOL_A_BITSET_BITS`` nest can
+only contain ``ETHTOOL_A_BITSET_BITS_BIT`` attributes but there can be an
+arbitrary number of them.  A bit may be identified by its index or by its
+name. When used in requests, listed bits are set to 0 or 1 according to
+``ETHTOOL_A_BITSET_BIT_VALUE``, the rest is preserved. A request fails if
+index exceeds kernel bit length or if name is not recognized.
+
+When ``ETHTOOL_A_BITSET_NOMASK`` flag is present, bitset is interpreted as
+a simple bitmap. ``ETHTOOL_A_BITSET_BIT_VALUE`` attributes are not used in
+such case. Such bitset represents a bitmap with listed bits set and the rest
+zero.
+
+In requests, application can use either form. Form used by kernel in reply is
+determined by ``ETHTOOL_FLAG_COMPACT_BITSETS`` flag in flags field of request
+header. Semantics of value and mask depends on the attribute.
+
+
+List of message types
+=====================
+
+All constants identifying message types use ``ETHTOOL_CMD_`` prefix and suffix
+according to message purpose:
+
+  ==============    ======================================
+  ``_GET``          userspace request to retrieve data
+  ``_SET``          userspace request to set data
+  ``_ACT``          userspace request to perform an action
+  ``_GET_REPLY``    kernel reply to a ``GET`` request
+  ``_SET_REPLY``    kernel reply to a ``SET`` request
+  ``_ACT_REPLY``    kernel reply to an ``ACT`` request
+  ``_NTF``          kernel notification
+  ==============    ======================================
+
+Userspace to kernel:
+
+  ===================================== ================================
+  ``ETHTOOL_MSG_STRSET_GET``            get string set
+  ``ETHTOOL_MSG_LINKINFO_GET``          get link settings
+  ``ETHTOOL_MSG_LINKINFO_SET``          set link settings
+  ``ETHTOOL_MSG_LINKMODES_GET``         get link modes info
+  ``ETHTOOL_MSG_LINKMODES_SET``         set link modes info
+  ``ETHTOOL_MSG_LINKSTATE_GET``         get link state
+  ``ETHTOOL_MSG_DEBUG_GET``             get debugging settings
+  ``ETHTOOL_MSG_DEBUG_SET``             set debugging settings
+  ``ETHTOOL_MSG_WOL_GET``               get wake-on-lan settings
+  ``ETHTOOL_MSG_WOL_SET``               set wake-on-lan settings
+  ``ETHTOOL_MSG_FEATURES_GET``          get device features
+  ``ETHTOOL_MSG_FEATURES_SET``          set device features
+  ``ETHTOOL_MSG_PRIVFLAGS_GET``         get private flags
+  ``ETHTOOL_MSG_PRIVFLAGS_SET``         set private flags
+  ``ETHTOOL_MSG_RINGS_GET``             get ring sizes
+  ``ETHTOOL_MSG_RINGS_SET``             set ring sizes
+  ``ETHTOOL_MSG_CHANNELS_GET``          get channel counts
+  ``ETHTOOL_MSG_CHANNELS_SET``          set channel counts
+  ``ETHTOOL_MSG_COALESCE_GET``          get coalescing parameters
+  ``ETHTOOL_MSG_COALESCE_SET``          set coalescing parameters
+  ``ETHTOOL_MSG_PAUSE_GET``             get pause parameters
+  ``ETHTOOL_MSG_PAUSE_SET``             set pause parameters
+  ``ETHTOOL_MSG_EEE_GET``               get EEE settings
+  ``ETHTOOL_MSG_EEE_SET``               set EEE settings
+  ``ETHTOOL_MSG_TSINFO_GET``		get timestamping info
+  ``ETHTOOL_MSG_CABLE_TEST_ACT``        action start cable test
+  ``ETHTOOL_MSG_CABLE_TEST_TDR_ACT``    action start raw TDR cable test
+  ``ETHTOOL_MSG_TUNNEL_INFO_GET``       get tunnel offload info
+  ===================================== ================================
+
+Kernel to userspace:
+
+  ===================================== =================================
+  ``ETHTOOL_MSG_STRSET_GET_REPLY``      string set contents
+  ``ETHTOOL_MSG_LINKINFO_GET_REPLY``    link settings
+  ``ETHTOOL_MSG_LINKINFO_NTF``          link settings notification
+  ``ETHTOOL_MSG_LINKMODES_GET_REPLY``   link modes info
+  ``ETHTOOL_MSG_LINKMODES_NTF``         link modes notification
+  ``ETHTOOL_MSG_LINKSTATE_GET_REPLY``   link state info
+  ``ETHTOOL_MSG_DEBUG_GET_REPLY``       debugging settings
+  ``ETHTOOL_MSG_DEBUG_NTF``             debugging settings notification
+  ``ETHTOOL_MSG_WOL_GET_REPLY``         wake-on-lan settings
+  ``ETHTOOL_MSG_WOL_NTF``               wake-on-lan settings notification
+  ``ETHTOOL_MSG_FEATURES_GET_REPLY``    device features
+  ``ETHTOOL_MSG_FEATURES_SET_REPLY``    optional reply to FEATURES_SET
+  ``ETHTOOL_MSG_FEATURES_NTF``          netdev features notification
+  ``ETHTOOL_MSG_PRIVFLAGS_GET_REPLY``   private flags
+  ``ETHTOOL_MSG_PRIVFLAGS_NTF``         private flags
+  ``ETHTOOL_MSG_RINGS_GET_REPLY``       ring sizes
+  ``ETHTOOL_MSG_RINGS_NTF``             ring sizes
+  ``ETHTOOL_MSG_CHANNELS_GET_REPLY``    channel counts
+  ``ETHTOOL_MSG_CHANNELS_NTF``          channel counts
+  ``ETHTOOL_MSG_COALESCE_GET_REPLY``    coalescing parameters
+  ``ETHTOOL_MSG_COALESCE_NTF``          coalescing parameters
+  ``ETHTOOL_MSG_PAUSE_GET_REPLY``       pause parameters
+  ``ETHTOOL_MSG_PAUSE_NTF``             pause parameters
+  ``ETHTOOL_MSG_EEE_GET_REPLY``         EEE settings
+  ``ETHTOOL_MSG_EEE_NTF``               EEE settings
+  ``ETHTOOL_MSG_TSINFO_GET_REPLY``	timestamping info
+  ``ETHTOOL_MSG_CABLE_TEST_NTF``        Cable test results
+  ``ETHTOOL_MSG_CABLE_TEST_TDR_NTF``    Cable test TDR results
+  ``ETHTOOL_MSG_TUNNEL_INFO_GET_REPLY`` tunnel offload info
+  ===================================== =================================
+
+``GET`` requests are sent by userspace applications to retrieve device
+information. They usually do not contain any message specific attributes.
+Kernel replies with corresponding "GET_REPLY" message. For most types, ``GET``
+request with ``NLM_F_DUMP`` and no device identification can be used to query
+the information for all devices supporting the request.
+
+If the data can be also modified, corresponding ``SET`` message with the same
+layout as corresponding ``GET_REPLY`` is used to request changes. Only
+attributes where a change is requested are included in such request (also, not
+all attributes may be changed). Replies to most ``SET`` request consist only
+of error code and extack; if kernel provides additional data, it is sent in
+the form of corresponding ``SET_REPLY`` message which can be suppressed by
+setting ``ETHTOOL_FLAG_OMIT_REPLY`` flag in request header.
+
+Data modification also triggers sending a ``NTF`` message with a notification.
+These usually bear only a subset of attributes which was affected by the
+change. The same notification is issued if the data is modified using other
+means (mostly ioctl ethtool interface). Unlike notifications from ethtool
+netlink code which are only sent if something actually changed, notifications
+triggered by ioctl interface may be sent even if the request did not actually
+change any data.
+
+``ACT`` messages request kernel (driver) to perform a specific action. If some
+information is reported by kernel (which can be suppressed by setting
+``ETHTOOL_FLAG_OMIT_REPLY`` flag in request header), the reply takes form of
+an ``ACT_REPLY`` message. Performing an action also triggers a notification
+(``NTF`` message).
+
+Later sections describe the format and semantics of these messages.
+
+
+STRSET_GET
+==========
+
+Requests contents of a string set as provided by ioctl commands
+``ETHTOOL_GSSET_INFO`` and ``ETHTOOL_GSTRINGS.`` String sets are not user
+writeable so that the corresponding ``STRSET_SET`` message is only used in
+kernel replies. There are two types of string sets: global (independent of
+a device, e.g. device feature names) and device specific (e.g. device private
+flags).
+
+Request contents:
+
+ +---------------------------------------+--------+------------------------+
+ | ``ETHTOOL_A_STRSET_HEADER``           | nested | request header         |
+ +---------------------------------------+--------+------------------------+
+ | ``ETHTOOL_A_STRSET_STRINGSETS``       | nested | string set to request  |
+ +-+-------------------------------------+--------+------------------------+
+ | | ``ETHTOOL_A_STRINGSETS_STRINGSET+`` | nested | one string set         |
+ +-+-+-----------------------------------+--------+------------------------+
+ | | | ``ETHTOOL_A_STRINGSET_ID``        | u32    | set id                 |
+ +-+-+-----------------------------------+--------+------------------------+
+
+Kernel response contents:
+
+ +---------------------------------------+--------+-----------------------+
+ | ``ETHTOOL_A_STRSET_HEADER``           | nested | reply header          |
+ +---------------------------------------+--------+-----------------------+
+ | ``ETHTOOL_A_STRSET_STRINGSETS``       | nested | array of string sets  |
+ +-+-------------------------------------+--------+-----------------------+
+ | | ``ETHTOOL_A_STRINGSETS_STRINGSET+`` | nested | one string set        |
+ +-+-+-----------------------------------+--------+-----------------------+
+ | | | ``ETHTOOL_A_STRINGSET_ID``        | u32    | set id                |
+ +-+-+-----------------------------------+--------+-----------------------+
+ | | | ``ETHTOOL_A_STRINGSET_COUNT``     | u32    | number of strings     |
+ +-+-+-----------------------------------+--------+-----------------------+
+ | | | ``ETHTOOL_A_STRINGSET_STRINGS``   | nested | array of strings      |
+ +-+-+-+---------------------------------+--------+-----------------------+
+ | | | | ``ETHTOOL_A_STRINGS_STRING+``   | nested | one string            |
+ +-+-+-+-+-------------------------------+--------+-----------------------+
+ | | | | | ``ETHTOOL_A_STRING_INDEX``    | u32    | string index          |
+ +-+-+-+-+-------------------------------+--------+-----------------------+
+ | | | | | ``ETHTOOL_A_STRING_VALUE``    | string | string value          |
+ +-+-+-+-+-------------------------------+--------+-----------------------+
+ | ``ETHTOOL_A_STRSET_COUNTS_ONLY``      | flag   | return only counts    |
+ +---------------------------------------+--------+-----------------------+
+
+Device identification in request header is optional. Depending on its presence
+a and ``NLM_F_DUMP`` flag, there are three type of ``STRSET_GET`` requests:
+
+ - no ``NLM_F_DUMP,`` no device: get "global" stringsets
+ - no ``NLM_F_DUMP``, with device: get string sets related to the device
+ - ``NLM_F_DUMP``, no device: get device related string sets for all devices
+
+If there is no ``ETHTOOL_A_STRSET_STRINGSETS`` array, all string sets of
+requested type are returned, otherwise only those specified in the request.
+Flag ``ETHTOOL_A_STRSET_COUNTS_ONLY`` tells kernel to only return string
+counts of the sets, not the actual strings.
+
+
+LINKINFO_GET
+============
+
+Requests link settings as provided by ``ETHTOOL_GLINKSETTINGS`` except for
+link modes and autonegotiation related information. The request does not use
+any attributes.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_LINKINFO_HEADER``         nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_LINKINFO_HEADER``         nested  reply header
+  ``ETHTOOL_A_LINKINFO_PORT``           u8      physical port
+  ``ETHTOOL_A_LINKINFO_PHYADDR``        u8      phy MDIO address
+  ``ETHTOOL_A_LINKINFO_TP_MDIX``        u8      MDI(-X) status
+  ``ETHTOOL_A_LINKINFO_TP_MDIX_CTRL``   u8      MDI(-X) control
+  ``ETHTOOL_A_LINKINFO_TRANSCEIVER``    u8      transceiver
+  ====================================  ======  ==========================
+
+Attributes and their values have the same meaning as matching members of the
+corresponding ioctl structures.
+
+``LINKINFO_GET`` allows dump requests (kernel returns reply message for all
+devices supporting the request).
+
+
+LINKINFO_SET
+============
+
+``LINKINFO_SET`` request allows setting some of the attributes reported by
+``LINKINFO_GET``.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_LINKINFO_HEADER``         nested  request header
+  ``ETHTOOL_A_LINKINFO_PORT``           u8      physical port
+  ``ETHTOOL_A_LINKINFO_PHYADDR``        u8      phy MDIO address
+  ``ETHTOOL_A_LINKINFO_TP_MDIX_CTRL``   u8      MDI(-X) control
+  ====================================  ======  ==========================
+
+MDI(-X) status and transceiver cannot be set, request with the corresponding
+attributes is rejected.
+
+
+LINKMODES_GET
+=============
+
+Requests link modes (supported, advertised and peer advertised) and related
+information (autonegotiation status, link speed and duplex) as provided by
+``ETHTOOL_GLINKSETTINGS``. The request does not use any attributes.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_LINKMODES_HEADER``        nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ==========================================  ======  ==========================
+  ``ETHTOOL_A_LINKMODES_HEADER``              nested  reply header
+  ``ETHTOOL_A_LINKMODES_AUTONEG``             u8      autonegotiation status
+  ``ETHTOOL_A_LINKMODES_OURS``                bitset  advertised link modes
+  ``ETHTOOL_A_LINKMODES_PEER``                bitset  partner link modes
+  ``ETHTOOL_A_LINKMODES_SPEED``               u32     link speed (Mb/s)
+  ``ETHTOOL_A_LINKMODES_DUPLEX``              u8      duplex mode
+  ``ETHTOOL_A_LINKMODES_MASTER_SLAVE_CFG``    u8      Master/slave port mode
+  ``ETHTOOL_A_LINKMODES_MASTER_SLAVE_STATE``  u8      Master/slave port state
+  ==========================================  ======  ==========================
+
+For ``ETHTOOL_A_LINKMODES_OURS``, value represents advertised modes and mask
+represents supported modes. ``ETHTOOL_A_LINKMODES_PEER`` in the reply is a bit
+list.
+
+``LINKMODES_GET`` allows dump requests (kernel returns reply messages for all
+devices supporting the request).
+
+
+LINKMODES_SET
+=============
+
+Request contents:
+
+  ==========================================  ======  ==========================
+  ``ETHTOOL_A_LINKMODES_HEADER``              nested  request header
+  ``ETHTOOL_A_LINKMODES_AUTONEG``             u8      autonegotiation status
+  ``ETHTOOL_A_LINKMODES_OURS``                bitset  advertised link modes
+  ``ETHTOOL_A_LINKMODES_PEER``                bitset  partner link modes
+  ``ETHTOOL_A_LINKMODES_SPEED``               u32     link speed (Mb/s)
+  ``ETHTOOL_A_LINKMODES_DUPLEX``              u8      duplex mode
+  ``ETHTOOL_A_LINKMODES_MASTER_SLAVE_CFG``    u8      Master/slave port mode
+  ==========================================  ======  ==========================
+
+``ETHTOOL_A_LINKMODES_OURS`` bit set allows setting advertised link modes. If
+autonegotiation is on (either set now or kept from before), advertised modes
+are not changed (no ``ETHTOOL_A_LINKMODES_OURS`` attribute) and at least one
+of speed and duplex is specified, kernel adjusts advertised modes to all
+supported modes matching speed, duplex or both (whatever is specified). This
+autoselection is done on ethtool side with ioctl interface, netlink interface
+is supposed to allow requesting changes without knowing what exactly kernel
+supports.
+
+
+LINKSTATE_GET
+=============
+
+Requests link state information. Link up/down flag (as provided by
+``ETHTOOL_GLINK`` ioctl command) is provided. Optionally, extended state might
+be provided as well. In general, extended state describes reasons for why a port
+is down, or why it operates in some non-obvious mode. This request does not have
+any attributes.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_LINKSTATE_HEADER``        nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ============================
+  ``ETHTOOL_A_LINKSTATE_HEADER``        nested  reply header
+  ``ETHTOOL_A_LINKSTATE_LINK``          bool    link state (up/down)
+  ``ETHTOOL_A_LINKSTATE_SQI``           u32     Current Signal Quality Index
+  ``ETHTOOL_A_LINKSTATE_SQI_MAX``       u32     Max support SQI value
+  ``ETHTOOL_A_LINKSTATE_EXT_STATE``     u8      link extended state
+  ``ETHTOOL_A_LINKSTATE_EXT_SUBSTATE``  u8      link extended substate
+  ====================================  ======  ============================
+
+For most NIC drivers, the value of ``ETHTOOL_A_LINKSTATE_LINK`` returns
+carrier flag provided by ``netif_carrier_ok()`` but there are drivers which
+define their own handler.
+
+``ETHTOOL_A_LINKSTATE_EXT_STATE`` and ``ETHTOOL_A_LINKSTATE_EXT_SUBSTATE`` are
+optional values. ethtool core can provide either both
+``ETHTOOL_A_LINKSTATE_EXT_STATE`` and ``ETHTOOL_A_LINKSTATE_EXT_SUBSTATE``,
+or only ``ETHTOOL_A_LINKSTATE_EXT_STATE``, or none of them.
+
+``LINKSTATE_GET`` allows dump requests (kernel returns reply messages for all
+devices supporting the request).
+
+
+Link extended states:
+
+  ================================================      ============================================
+  ``ETHTOOL_LINK_EXT_STATE_AUTONEG``                    States relating to the autonegotiation or
+                                                        issues therein
+
+  ``ETHTOOL_LINK_EXT_STATE_LINK_TRAINING_FAILURE``      Failure during link training
+
+  ``ETHTOOL_LINK_EXT_STATE_LINK_LOGICAL_MISMATCH``      Logical mismatch in physical coding sublayer
+                                                        or forward error correction sublayer
+
+  ``ETHTOOL_LINK_EXT_STATE_BAD_SIGNAL_INTEGRITY``       Signal integrity issues
+
+  ``ETHTOOL_LINK_EXT_STATE_NO_CABLE``                   No cable connected
+
+  ``ETHTOOL_LINK_EXT_STATE_CABLE_ISSUE``                Failure is related to cable,
+                                                        e.g., unsupported cable
+
+  ``ETHTOOL_LINK_EXT_STATE_EEPROM_ISSUE``               Failure is related to EEPROM, e.g., failure
+                                                        during reading or parsing the data
+
+  ``ETHTOOL_LINK_EXT_STATE_CALIBRATION_FAILURE``        Failure during calibration algorithm
+
+  ``ETHTOOL_LINK_EXT_STATE_POWER_BUDGET_EXCEEDED``      The hardware is not able to provide the
+                                                        power required from cable or module
+
+  ``ETHTOOL_LINK_EXT_STATE_OVERHEAT``                   The module is overheated
+  ================================================      ============================================
+
+Link extended substates:
+
+  Autoneg substates:
+
+  ===============================================================   ================================
+  ``ETHTOOL_LINK_EXT_SUBSTATE_AN_NO_PARTNER_DETECTED``              Peer side is down
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_AN_ACK_NOT_RECEIVED``                 Ack not received from peer side
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_AN_NEXT_PAGE_EXCHANGE_FAILED``        Next page exchange failed
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_AN_NO_PARTNER_DETECTED_FORCE_MODE``   Peer side is down during force
+                                                                    mode or there is no agreement of
+                                                                    speed
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_AN_FEC_MISMATCH_DURING_OVERRIDE``     Forward error correction modes
+                                                                    in both sides are mismatched
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_AN_NO_HCD``                           No Highest Common Denominator
+  ===============================================================   ================================
+
+  Link training substates:
+
+  ===========================================================================   ====================
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LT_KR_FRAME_LOCK_NOT_ACQUIRED``                    Frames were not
+                                                                                 recognized, the
+                                                                                 lock failed
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LT_KR_LINK_INHIBIT_TIMEOUT``                       The lock did not
+                                                                                 occur before
+                                                                                 timeout
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LT_KR_LINK_PARTNER_DID_NOT_SET_RECEIVER_READY``    Peer side did not
+                                                                                 send ready signal
+                                                                                 after training
+                                                                                 process
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LT_REMOTE_FAULT``                                  Remote side is not
+                                                                                 ready yet
+  ===========================================================================   ====================
+
+  Link logical mismatch substates:
+
+  ================================================================   ===============================
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LLM_PCS_DID_NOT_ACQUIRE_BLOCK_LOCK``   Physical coding sublayer was
+                                                                     not locked in first phase -
+                                                                     block lock
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LLM_PCS_DID_NOT_ACQUIRE_AM_LOCK``      Physical coding sublayer was
+                                                                     not locked in second phase -
+                                                                     alignment markers lock
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LLM_PCS_DID_NOT_GET_ALIGN_STATUS``     Physical coding sublayer did
+                                                                     not get align status
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LLM_FC_FEC_IS_NOT_LOCKED``             FC forward error correction is
+                                                                     not locked
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_LLM_RS_FEC_IS_NOT_LOCKED``             RS forward error correction is
+                                                                     not locked
+  ================================================================   ===============================
+
+  Bad signal integrity substates:
+
+  =================================================================    =============================
+  ``ETHTOOL_LINK_EXT_SUBSTATE_BSI_LARGE_NUMBER_OF_PHYSICAL_ERRORS``    Large number of physical
+                                                                       errors
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_BSI_UNSUPPORTED_RATE``                   The system attempted to
+                                                                       operate the cable at a rate
+                                                                       that is not formally
+                                                                       supported, which led to
+                                                                       signal integrity issues
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_BSI_SERDES_REFERENCE_CLOCK_LOST``        The external clock signal for
+                                                                       SerDes is too weak or
+                                                                       unavailable.
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_BSI_SERDES_ALOS``                        The received signal for
+                                                                       SerDes is too weak because
+                                                                       analog loss of signal.
+  =================================================================    =============================
+
+  Cable issue substates:
+
+  ===================================================   ============================================
+  ``ETHTOOL_LINK_EXT_SUBSTATE_CI_UNSUPPORTED_CABLE``    Unsupported cable
+
+  ``ETHTOOL_LINK_EXT_SUBSTATE_CI_CABLE_TEST_FAILURE``   Cable test failure
+  ===================================================   ============================================
+
+DEBUG_GET
+=========
+
+Requests debugging settings of a device. At the moment, only message mask is
+provided.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_DEBUG_HEADER``            nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_DEBUG_HEADER``            nested  reply header
+  ``ETHTOOL_A_DEBUG_MSGMASK``           bitset  message mask
+  ====================================  ======  ==========================
+
+The message mask (``ETHTOOL_A_DEBUG_MSGMASK``) is equal to message level as
+provided by ``ETHTOOL_GMSGLVL`` and set by ``ETHTOOL_SMSGLVL`` in ioctl
+interface. While it is called message level there for historical reasons, most
+drivers and almost all newer drivers use it as a mask of enabled message
+classes (represented by ``NETIF_MSG_*`` constants); therefore netlink
+interface follows its actual use in practice.
+
+``DEBUG_GET`` allows dump requests (kernel returns reply messages for all
+devices supporting the request).
+
+
+DEBUG_SET
+=========
+
+Set or update debugging settings of a device. At the moment, only message mask
+is supported.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_DEBUG_HEADER``            nested  request header
+  ``ETHTOOL_A_DEBUG_MSGMASK``           bitset  message mask
+  ====================================  ======  ==========================
+
+``ETHTOOL_A_DEBUG_MSGMASK`` bit set allows setting or modifying mask of
+enabled debugging message types for the device.
+
+
+WOL_GET
+=======
+
+Query device wake-on-lan settings. Unlike most "GET" type requests,
+``ETHTOOL_MSG_WOL_GET`` requires (netns) ``CAP_NET_ADMIN`` privileges as it
+(potentially) provides SecureOn(tm) password which is confidential.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_WOL_HEADER``              nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_WOL_HEADER``              nested  reply header
+  ``ETHTOOL_A_WOL_MODES``               bitset  mask of enabled WoL modes
+  ``ETHTOOL_A_WOL_SOPASS``              binary  SecureOn(tm) password
+  ====================================  ======  ==========================
+
+In reply, ``ETHTOOL_A_WOL_MODES`` mask consists of modes supported by the
+device, value of modes which are enabled. ``ETHTOOL_A_WOL_SOPASS`` is only
+included in reply if ``WAKE_MAGICSECURE`` mode is supported.
+
+
+WOL_SET
+=======
+
+Set or update wake-on-lan settings.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_WOL_HEADER``              nested  request header
+  ``ETHTOOL_A_WOL_MODES``               bitset  enabled WoL modes
+  ``ETHTOOL_A_WOL_SOPASS``              binary  SecureOn(tm) password
+  ====================================  ======  ==========================
+
+``ETHTOOL_A_WOL_SOPASS`` is only allowed for devices supporting
+``WAKE_MAGICSECURE`` mode.
+
+
+FEATURES_GET
+============
+
+Gets netdev features like ``ETHTOOL_GFEATURES`` ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_FEATURES_HEADER``         nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_FEATURES_HEADER``         nested  reply header
+  ``ETHTOOL_A_FEATURES_HW``             bitset  dev->hw_features
+  ``ETHTOOL_A_FEATURES_WANTED``         bitset  dev->wanted_features
+  ``ETHTOOL_A_FEATURES_ACTIVE``         bitset  dev->features
+  ``ETHTOOL_A_FEATURES_NOCHANGE``       bitset  NETIF_F_NEVER_CHANGE
+  ====================================  ======  ==========================
+
+Bitmaps in kernel response have the same meaning as bitmaps used in ioctl
+interference but attribute names are different (they are based on
+corresponding members of struct net_device). Legacy "flags" are not provided,
+if userspace needs them (most likely only ethtool for backward compatibility),
+it can calculate their values from related feature bits itself.
+ETHA_FEATURES_HW uses mask consisting of all features recognized by kernel (to
+provide all names when using verbose bitmap format), the other three use no
+mask (simple bit lists).
+
+
+FEATURES_SET
+============
+
+Request to set netdev features like ``ETHTOOL_SFEATURES`` ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_FEATURES_HEADER``         nested  request header
+  ``ETHTOOL_A_FEATURES_WANTED``         bitset  requested features
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_FEATURES_HEADER``         nested  reply header
+  ``ETHTOOL_A_FEATURES_WANTED``         bitset  diff wanted vs. result
+  ``ETHTOOL_A_FEATURES_ACTIVE``         bitset  diff old vs. new active
+  ====================================  ======  ==========================
+
+Request constains only one bitset which can be either value/mask pair (request
+to change specific feature bits and leave the rest) or only a value (request
+to set all features to specified set).
+
+As request is subject to netdev_change_features() sanity checks, optional
+kernel reply (can be suppressed by ``ETHTOOL_FLAG_OMIT_REPLY`` flag in request
+header) informs client about the actual result. ``ETHTOOL_A_FEATURES_WANTED``
+reports the difference between client request and actual result: mask consists
+of bits which differ between requested features and result (dev->features
+after the operation), value consists of values of these bits in the request
+(i.e. negated values from resulting features). ``ETHTOOL_A_FEATURES_ACTIVE``
+reports the difference between old and new dev->features: mask consists of
+bits which have changed, values are their values in new dev->features (after
+the operation).
+
+``ETHTOOL_MSG_FEATURES_NTF`` notification is sent not only if device features
+are modified using ``ETHTOOL_MSG_FEATURES_SET`` request or on of ethtool ioctl
+request but also each time features are modified with netdev_update_features()
+or netdev_change_features().
+
+
+PRIVFLAGS_GET
+=============
+
+Gets private flags like ``ETHTOOL_GPFLAGS`` ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_PRIVFLAGS_HEADER``        nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_PRIVFLAGS_HEADER``        nested  reply header
+  ``ETHTOOL_A_PRIVFLAGS_FLAGS``         bitset  private flags
+  ====================================  ======  ==========================
+
+``ETHTOOL_A_PRIVFLAGS_FLAGS`` is a bitset with values of device private flags.
+These flags are defined by driver, their number and names (and also meaning)
+are device dependent. For compact bitset format, names can be retrieved as
+``ETH_SS_PRIV_FLAGS`` string set. If verbose bitset format is requested,
+response uses all private flags supported by the device as mask so that client
+gets the full information without having to fetch the string set with names.
+
+
+PRIVFLAGS_SET
+=============
+
+Sets or modifies values of device private flags like ``ETHTOOL_SPFLAGS``
+ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_PRIVFLAGS_HEADER``        nested  request header
+  ``ETHTOOL_A_PRIVFLAGS_FLAGS``         bitset  private flags
+  ====================================  ======  ==========================
+
+``ETHTOOL_A_PRIVFLAGS_FLAGS`` can either set the whole set of private flags or
+modify only values of some of them.
+
+
+RINGS_GET
+=========
+
+Gets ring sizes like ``ETHTOOL_GRINGPARAM`` ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_RINGS_HEADER``            nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_RINGS_HEADER``            nested  reply header
+  ``ETHTOOL_A_RINGS_RX_MAX``            u32     max size of RX ring
+  ``ETHTOOL_A_RINGS_RX_MINI_MAX``       u32     max size of RX mini ring
+  ``ETHTOOL_A_RINGS_RX_JUMBO_MAX``      u32     max size of RX jumbo ring
+  ``ETHTOOL_A_RINGS_TX_MAX``            u32     max size of TX ring
+  ``ETHTOOL_A_RINGS_RX``                u32     size of RX ring
+  ``ETHTOOL_A_RINGS_RX_MINI``           u32     size of RX mini ring
+  ``ETHTOOL_A_RINGS_RX_JUMBO``          u32     size of RX jumbo ring
+  ``ETHTOOL_A_RINGS_TX``                u32     size of TX ring
+  ====================================  ======  ==========================
+
+
+RINGS_SET
+=========
+
+Sets ring sizes like ``ETHTOOL_SRINGPARAM`` ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_RINGS_HEADER``            nested  reply header
+  ``ETHTOOL_A_RINGS_RX``                u32     size of RX ring
+  ``ETHTOOL_A_RINGS_RX_MINI``           u32     size of RX mini ring
+  ``ETHTOOL_A_RINGS_RX_JUMBO``          u32     size of RX jumbo ring
+  ``ETHTOOL_A_RINGS_TX``                u32     size of TX ring
+  ====================================  ======  ==========================
+
+Kernel checks that requested ring sizes do not exceed limits reported by
+driver. Driver may impose additional constraints and may not suspport all
+attributes.
+
+
+CHANNELS_GET
+============
+
+Gets channel counts like ``ETHTOOL_GCHANNELS`` ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_CHANNELS_HEADER``         nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_CHANNELS_HEADER``          nested  reply header
+  ``ETHTOOL_A_CHANNELS_RX_MAX``          u32     max receive channels
+  ``ETHTOOL_A_CHANNELS_TX_MAX``          u32     max transmit channels
+  ``ETHTOOL_A_CHANNELS_OTHER_MAX``       u32     max other channels
+  ``ETHTOOL_A_CHANNELS_COMBINED_MAX``    u32     max combined channels
+  ``ETHTOOL_A_CHANNELS_RX_COUNT``        u32     receive channel count
+  ``ETHTOOL_A_CHANNELS_TX_COUNT``        u32     transmit channel count
+  ``ETHTOOL_A_CHANNELS_OTHER_COUNT``     u32     other channel count
+  ``ETHTOOL_A_CHANNELS_COMBINED_COUNT``  u32     combined channel count
+  =====================================  ======  ==========================
+
+
+CHANNELS_SET
+============
+
+Sets channel counts like ``ETHTOOL_SCHANNELS`` ioctl request.
+
+Request contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_CHANNELS_HEADER``          nested  request header
+  ``ETHTOOL_A_CHANNELS_RX_COUNT``        u32     receive channel count
+  ``ETHTOOL_A_CHANNELS_TX_COUNT``        u32     transmit channel count
+  ``ETHTOOL_A_CHANNELS_OTHER_COUNT``     u32     other channel count
+  ``ETHTOOL_A_CHANNELS_COMBINED_COUNT``  u32     combined channel count
+  =====================================  ======  ==========================
+
+Kernel checks that requested channel counts do not exceed limits reported by
+driver. Driver may impose additional constraints and may not suspport all
+attributes.
+
+
+COALESCE_GET
+============
+
+Gets coalescing parameters like ``ETHTOOL_GCOALESCE`` ioctl request.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_COALESCE_HEADER``         nested  request header
+  ====================================  ======  ==========================
+
+Kernel response contents:
+
+  ===========================================  ======  =======================
+  ``ETHTOOL_A_COALESCE_HEADER``                nested  reply header
+  ``ETHTOOL_A_COALESCE_RX_USECS``              u32     delay (us), normal Rx
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES``         u32     max packets, normal Rx
+  ``ETHTOOL_A_COALESCE_RX_USECS_IRQ``          u32     delay (us), Rx in IRQ
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES_IRQ``     u32     max packets, Rx in IRQ
+  ``ETHTOOL_A_COALESCE_TX_USECS``              u32     delay (us), normal Tx
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES``         u32     max packets, normal Tx
+  ``ETHTOOL_A_COALESCE_TX_USECS_IRQ``          u32     delay (us), Tx in IRQ
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES_IRQ``     u32     IRQ packets, Tx in IRQ
+  ``ETHTOOL_A_COALESCE_STATS_BLOCK_USECS``     u32     delay of stats update
+  ``ETHTOOL_A_COALESCE_USE_ADAPTIVE_RX``       bool    adaptive Rx coalesce
+  ``ETHTOOL_A_COALESCE_USE_ADAPTIVE_TX``       bool    adaptive Tx coalesce
+  ``ETHTOOL_A_COALESCE_PKT_RATE_LOW``          u32     threshold for low rate
+  ``ETHTOOL_A_COALESCE_RX_USECS_LOW``          u32     delay (us), low Rx
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES_LOW``     u32     max packets, low Rx
+  ``ETHTOOL_A_COALESCE_TX_USECS_LOW``          u32     delay (us), low Tx
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES_LOW``     u32     max packets, low Tx
+  ``ETHTOOL_A_COALESCE_PKT_RATE_HIGH``         u32     threshold for high rate
+  ``ETHTOOL_A_COALESCE_RX_USECS_HIGH``         u32     delay (us), high Rx
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES_HIGH``    u32     max packets, high Rx
+  ``ETHTOOL_A_COALESCE_TX_USECS_HIGH``         u32     delay (us), high Tx
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES_HIGH``    u32     max packets, high Tx
+  ``ETHTOOL_A_COALESCE_RATE_SAMPLE_INTERVAL``  u32     rate sampling interval
+  ===========================================  ======  =======================
+
+Attributes are only included in reply if their value is not zero or the
+corresponding bit in ``ethtool_ops::supported_coalesce_params`` is set (i.e.
+they are declared as supported by driver).
+
+
+COALESCE_SET
+============
+
+Sets coalescing parameters like ``ETHTOOL_SCOALESCE`` ioctl request.
+
+Request contents:
+
+  ===========================================  ======  =======================
+  ``ETHTOOL_A_COALESCE_HEADER``                nested  request header
+  ``ETHTOOL_A_COALESCE_RX_USECS``              u32     delay (us), normal Rx
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES``         u32     max packets, normal Rx
+  ``ETHTOOL_A_COALESCE_RX_USECS_IRQ``          u32     delay (us), Rx in IRQ
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES_IRQ``     u32     max packets, Rx in IRQ
+  ``ETHTOOL_A_COALESCE_TX_USECS``              u32     delay (us), normal Tx
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES``         u32     max packets, normal Tx
+  ``ETHTOOL_A_COALESCE_TX_USECS_IRQ``          u32     delay (us), Tx in IRQ
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES_IRQ``     u32     IRQ packets, Tx in IRQ
+  ``ETHTOOL_A_COALESCE_STATS_BLOCK_USECS``     u32     delay of stats update
+  ``ETHTOOL_A_COALESCE_USE_ADAPTIVE_RX``       bool    adaptive Rx coalesce
+  ``ETHTOOL_A_COALESCE_USE_ADAPTIVE_TX``       bool    adaptive Tx coalesce
+  ``ETHTOOL_A_COALESCE_PKT_RATE_LOW``          u32     threshold for low rate
+  ``ETHTOOL_A_COALESCE_RX_USECS_LOW``          u32     delay (us), low Rx
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES_LOW``     u32     max packets, low Rx
+  ``ETHTOOL_A_COALESCE_TX_USECS_LOW``          u32     delay (us), low Tx
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES_LOW``     u32     max packets, low Tx
+  ``ETHTOOL_A_COALESCE_PKT_RATE_HIGH``         u32     threshold for high rate
+  ``ETHTOOL_A_COALESCE_RX_USECS_HIGH``         u32     delay (us), high Rx
+  ``ETHTOOL_A_COALESCE_RX_MAX_FRAMES_HIGH``    u32     max packets, high Rx
+  ``ETHTOOL_A_COALESCE_TX_USECS_HIGH``         u32     delay (us), high Tx
+  ``ETHTOOL_A_COALESCE_TX_MAX_FRAMES_HIGH``    u32     max packets, high Tx
+  ``ETHTOOL_A_COALESCE_RATE_SAMPLE_INTERVAL``  u32     rate sampling interval
+  ===========================================  ======  =======================
+
+Request is rejected if it attributes declared as unsupported by driver (i.e.
+such that the corresponding bit in ``ethtool_ops::supported_coalesce_params``
+is not set), regardless of their values. Driver may impose additional
+constraints on coalescing parameters and their values.
+
+
+PAUSE_GET
+============
+
+Gets channel counts like ``ETHTOOL_GPAUSE`` ioctl request.
+
+Request contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_PAUSE_HEADER``             nested  request header
+  =====================================  ======  ==========================
+
+Kernel response contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_PAUSE_HEADER``             nested  request header
+  ``ETHTOOL_A_PAUSE_AUTONEG``            bool    pause autonegotiation
+  ``ETHTOOL_A_PAUSE_RX``                 bool    receive pause frames
+  ``ETHTOOL_A_PAUSE_TX``                 bool    transmit pause frames
+  ``ETHTOOL_A_PAUSE_STATS``              nested  pause statistics
+  =====================================  ======  ==========================
+
+``ETHTOOL_A_PAUSE_STATS`` are reported if ``ETHTOOL_FLAG_STATS`` was set
+in ``ETHTOOL_A_HEADER_FLAGS``.
+It will be empty if driver did not report any statistics. Drivers fill in
+the statistics in the following structure:
+
+.. kernel-doc:: include/linux/ethtool.h
+    :identifiers: ethtool_pause_stats
+
+Each member has a corresponding attribute defined.
+
+PAUSE_SET
+============
+
+Sets pause parameters like ``ETHTOOL_GPAUSEPARAM`` ioctl request.
+
+Request contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_PAUSE_HEADER``             nested  request header
+  ``ETHTOOL_A_PAUSE_AUTONEG``            bool    pause autonegotiation
+  ``ETHTOOL_A_PAUSE_RX``                 bool    receive pause frames
+  ``ETHTOOL_A_PAUSE_TX``                 bool    transmit pause frames
+  =====================================  ======  ==========================
+
+
+EEE_GET
+=======
+
+Gets channel counts like ``ETHTOOL_GEEE`` ioctl request.
+
+Request contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_EEE_HEADER``               nested  request header
+  =====================================  ======  ==========================
+
+Kernel response contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_EEE_HEADER``               nested  request header
+  ``ETHTOOL_A_EEE_MODES_OURS``           bool    supported/advertised modes
+  ``ETHTOOL_A_EEE_MODES_PEER``           bool    peer advertised link modes
+  ``ETHTOOL_A_EEE_ACTIVE``               bool    EEE is actively used
+  ``ETHTOOL_A_EEE_ENABLED``              bool    EEE is enabled
+  ``ETHTOOL_A_EEE_TX_LPI_ENABLED``       bool    Tx lpi enabled
+  ``ETHTOOL_A_EEE_TX_LPI_TIMER``         u32     Tx lpi timeout (in us)
+  =====================================  ======  ==========================
+
+In ``ETHTOOL_A_EEE_MODES_OURS``, mask consists of link modes for which EEE is
+enabled, value of link modes for which EEE is advertised. Link modes for which
+peer advertises EEE are listed in ``ETHTOOL_A_EEE_MODES_PEER`` (no mask). The
+netlink interface allows reporting EEE status for all link modes but only
+first 32 are provided by the ``ethtool_ops`` callback.
+
+
+EEE_SET
+=======
+
+Sets pause parameters like ``ETHTOOL_GEEEPARAM`` ioctl request.
+
+Request contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_EEE_HEADER``               nested  request header
+  ``ETHTOOL_A_EEE_MODES_OURS``           bool    advertised modes
+  ``ETHTOOL_A_EEE_ENABLED``              bool    EEE is enabled
+  ``ETHTOOL_A_EEE_TX_LPI_ENABLED``       bool    Tx lpi enabled
+  ``ETHTOOL_A_EEE_TX_LPI_TIMER``         u32     Tx lpi timeout (in us)
+  =====================================  ======  ==========================
+
+``ETHTOOL_A_EEE_MODES_OURS`` is used to either list link modes to advertise
+EEE for (if there is no mask) or specify changes to the list (if there is
+a mask). The netlink interface allows reporting EEE status for all link modes
+but only first 32 can be set at the moment as that is what the ``ethtool_ops``
+callback supports.
+
+
+TSINFO_GET
+==========
+
+Gets timestamping information like ``ETHTOOL_GET_TS_INFO`` ioctl request.
+
+Request contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_TSINFO_HEADER``            nested  request header
+  =====================================  ======  ==========================
+
+Kernel response contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_TSINFO_HEADER``            nested  request header
+  ``ETHTOOL_A_TSINFO_TIMESTAMPING``      bitset  SO_TIMESTAMPING flags
+  ``ETHTOOL_A_TSINFO_TX_TYPES``          bitset  supported Tx types
+  ``ETHTOOL_A_TSINFO_RX_FILTERS``        bitset  supported Rx filters
+  ``ETHTOOL_A_TSINFO_PHC_INDEX``         u32     PTP hw clock index
+  =====================================  ======  ==========================
+
+``ETHTOOL_A_TSINFO_PHC_INDEX`` is absent if there is no associated PHC (there
+is no special value for this case). The bitset attributes are omitted if they
+would be empty (no bit set).
+
+CABLE_TEST
+==========
+
+Start a cable test.
+
+Request contents:
+
+  ====================================  ======  ==========================
+  ``ETHTOOL_A_CABLE_TEST_HEADER``       nested  request header
+  ====================================  ======  ==========================
+
+Notification contents:
+
+An Ethernet cable typically contains 1, 2 or 4 pairs. The length of
+the pair can only be measured when there is a fault in the pair and
+hence a reflection. Information about the fault may not be available,
+depending on the specific hardware. Hence the contents of the notify
+message are mostly optional. The attributes can be repeated an
+arbitrary number of times, in an arbitrary order, for an arbitrary
+number of pairs.
+
+The example shows the notification sent when the test is completed for
+a T2 cable, i.e. two pairs. One pair is OK and hence has no length
+information. The second pair has a fault and does have length
+information.
+
+ +---------------------------------------------+--------+---------------------+
+ | ``ETHTOOL_A_CABLE_TEST_HEADER``             | nested | reply header        |
+ +---------------------------------------------+--------+---------------------+
+ | ``ETHTOOL_A_CABLE_TEST_STATUS``             | u8     | completed           |
+ +---------------------------------------------+--------+---------------------+
+ | ``ETHTOOL_A_CABLE_TEST_NTF_NEST``           | nested | all the results     |
+ +-+-------------------------------------------+--------+---------------------+
+ | | ``ETHTOOL_A_CABLE_NEST_RESULT``           | nested | cable test result   |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_CABLE_RESULTS_PAIR``        | u8     | pair number         |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_CABLE_RESULTS_CODE``        | u8     | result code         |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | ``ETHTOOL_A_CABLE_NEST_RESULT``           | nested | cable test results  |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_CABLE_RESULTS_PAIR``        | u8     | pair number         |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_CABLE_RESULTS_CODE``        | u8     | result code         |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | ``ETHTOOL_A_CABLE_NEST_FAULT_LENGTH``     | nested | cable length        |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_CABLE_FAULT_LENGTH_PAIR``   | u8     | pair number         |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_CABLE_FAULT_LENGTH_CM``     | u32    | length in cm        |
+ +-+-+-----------------------------------------+--------+---------------------+
+
+CABLE_TEST TDR
+==============
+
+Start a cable test and report raw TDR data
+
+Request contents:
+
+ +--------------------------------------------+--------+-----------------------+
+ | ``ETHTOOL_A_CABLE_TEST_TDR_HEADER``        | nested | reply header          |
+ +--------------------------------------------+--------+-----------------------+
+ | ``ETHTOOL_A_CABLE_TEST_TDR_CFG``           | nested | test configuration    |
+ +-+------------------------------------------+--------+-----------------------+
+ | | ``ETHTOOL_A_CABLE_STEP_FIRST_DISTANCE``  | u32    | first data distance   |
+ +-+-+----------------------------------------+--------+-----------------------+
+ | | ``ETHTOOL_A_CABLE_STEP_LAST_DISTANCE``   | u32    | last data distance    |
+ +-+-+----------------------------------------+--------+-----------------------+
+ | | ``ETHTOOL_A_CABLE_STEP_STEP_DISTANCE``   | u32    | distance of each step |
+ +-+-+----------------------------------------+--------+-----------------------+
+ | | ``ETHTOOL_A_CABLE_TEST_TDR_CFG_PAIR``    | u8     | pair to test          |
+ +-+-+----------------------------------------+--------+-----------------------+
+
+The ETHTOOL_A_CABLE_TEST_TDR_CFG is optional, as well as all members
+of the nest. All distances are expressed in centimeters. The PHY takes
+the distances as a guide, and rounds to the nearest distance it
+actually supports. If a pair is passed, only that one pair will be
+tested. Otherwise all pairs are tested.
+
+Notification contents:
+
+Raw TDR data is gathered by sending a pulse down the cable and
+recording the amplitude of the reflected pulse for a given distance.
+
+It can take a number of seconds to collect TDR data, especial if the
+full 100 meters is probed at 1 meter intervals. When the test is
+started a notification will be sent containing just
+ETHTOOL_A_CABLE_TEST_TDR_STATUS with the value
+ETHTOOL_A_CABLE_TEST_NTF_STATUS_STARTED.
+
+When the test has completed a second notification will be sent
+containing ETHTOOL_A_CABLE_TEST_TDR_STATUS with the value
+ETHTOOL_A_CABLE_TEST_NTF_STATUS_COMPLETED and the TDR data.
+
+The message may optionally contain the amplitude of the pulse send
+down the cable. This is measured in mV. A reflection should not be
+bigger than transmitted pulse.
+
+Before the raw TDR data should be an ETHTOOL_A_CABLE_TDR_NEST_STEP
+nest containing information about the distance along the cable for the
+first reading, the last reading, and the step between each
+reading. Distances are measured in centimeters. These should be the
+exact values the PHY used. These may be different to what the user
+requested, if the native measurement resolution is greater than 1 cm.
+
+For each step along the cable, a ETHTOOL_A_CABLE_TDR_NEST_AMPLITUDE is
+used to report the amplitude of the reflection for a given pair.
+
+ +---------------------------------------------+--------+----------------------+
+ | ``ETHTOOL_A_CABLE_TEST_TDR_HEADER``         | nested | reply header         |
+ +---------------------------------------------+--------+----------------------+
+ | ``ETHTOOL_A_CABLE_TEST_TDR_STATUS``         | u8     | completed            |
+ +---------------------------------------------+--------+----------------------+
+ | ``ETHTOOL_A_CABLE_TEST_TDR_NTF_NEST``       | nested | all the results      |
+ +-+-------------------------------------------+--------+----------------------+
+ | | ``ETHTOOL_A_CABLE_TDR_NEST_PULSE``        | nested | TX Pulse amplitude   |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_PULSE_mV``            | s16    | Pulse amplitude      |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | ``ETHTOOL_A_CABLE_NEST_STEP``             | nested | TDR step info        |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_STEP_FIRST_DISTANCE`` | u32    | First data distance  |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_STEP_LAST_DISTANCE``  | u32    | Last data distance   |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_STEP_STEP_DISTANCE``  | u32    | distance of each step|
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | ``ETHTOOL_A_CABLE_TDR_NEST_AMPLITUDE``    | nested | Reflection amplitude |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_RESULTS_PAIR``        | u8     | pair number          |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_AMPLITUDE_mV``        | s16    | Reflection amplitude |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | ``ETHTOOL_A_CABLE_TDR_NEST_AMPLITUDE``    | nested | Reflection amplitude |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_RESULTS_PAIR``        | u8     | pair number          |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_AMPLITUDE_mV``        | s16    | Reflection amplitude |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | ``ETHTOOL_A_CABLE_TDR_NEST_AMPLITUDE``    | nested | Reflection amplitude |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_RESULTS_PAIR``        | u8     | pair number          |
+ +-+-+-----------------------------------------+--------+----------------------+
+ | | | ``ETHTOOL_A_CABLE_AMPLITUDE_mV``        | s16    | Reflection amplitude |
+ +-+-+-----------------------------------------+--------+----------------------+
+
+TUNNEL_INFO
+===========
+
+Gets information about the tunnel state NIC is aware of.
+
+Request contents:
+
+  =====================================  ======  ==========================
+  ``ETHTOOL_A_TUNNEL_INFO_HEADER``       nested  request header
+  =====================================  ======  ==========================
+
+Kernel response contents:
+
+ +---------------------------------------------+--------+---------------------+
+ | ``ETHTOOL_A_TUNNEL_INFO_HEADER``            | nested | reply header        |
+ +---------------------------------------------+--------+---------------------+
+ | ``ETHTOOL_A_TUNNEL_INFO_UDP_PORTS``         | nested | all UDP port tables |
+ +-+-------------------------------------------+--------+---------------------+
+ | | ``ETHTOOL_A_TUNNEL_UDP_TABLE``            | nested | one UDP port table  |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_TUNNEL_UDP_TABLE_SIZE``     | u32    | max size of the     |
+ | | |                                         |        | table               |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_TUNNEL_UDP_TABLE_TYPES``    | bitset | tunnel types which  |
+ | | |                                         |        | table can hold      |
+ +-+-+-----------------------------------------+--------+---------------------+
+ | | | ``ETHTOOL_A_TUNNEL_UDP_TABLE_ENTRY``    | nested | offloaded UDP port  |
+ +-+-+-+---------------------------------------+--------+---------------------+
+ | | | | ``ETHTOOL_A_TUNNEL_UDP_ENTRY_PORT``   | be16   | UDP port            |
+ +-+-+-+---------------------------------------+--------+---------------------+
+ | | | | ``ETHTOOL_A_TUNNEL_UDP_ENTRY_TYPE``   | u32    | tunnel type         |
+ +-+-+-+---------------------------------------+--------+---------------------+
+
+For UDP tunnel table empty ``ETHTOOL_A_TUNNEL_UDP_TABLE_TYPES`` indicates that
+the table contains static entries, hard-coded by the NIC.
+
+Request translation
+===================
+
+The following table maps ioctl commands to netlink commands providing their
+functionality. Entries with "n/a" in right column are commands which do not
+have their netlink replacement yet. Entries which "n/a" in the left column
+are netlink only.
+
+  =================================== =====================================
+  ioctl command                       netlink command
+  =================================== =====================================
+  ``ETHTOOL_GSET``                    ``ETHTOOL_MSG_LINKINFO_GET``
+                                      ``ETHTOOL_MSG_LINKMODES_GET``
+  ``ETHTOOL_SSET``                    ``ETHTOOL_MSG_LINKINFO_SET``
+                                      ``ETHTOOL_MSG_LINKMODES_SET``
+  ``ETHTOOL_GDRVINFO``                n/a
+  ``ETHTOOL_GREGS``                   n/a
+  ``ETHTOOL_GWOL``                    ``ETHTOOL_MSG_WOL_GET``
+  ``ETHTOOL_SWOL``                    ``ETHTOOL_MSG_WOL_SET``
+  ``ETHTOOL_GMSGLVL``                 ``ETHTOOL_MSG_DEBUG_GET``
+  ``ETHTOOL_SMSGLVL``                 ``ETHTOOL_MSG_DEBUG_SET``
+  ``ETHTOOL_NWAY_RST``                n/a
+  ``ETHTOOL_GLINK``                   ``ETHTOOL_MSG_LINKSTATE_GET``
+  ``ETHTOOL_GEEPROM``                 n/a
+  ``ETHTOOL_SEEPROM``                 n/a
+  ``ETHTOOL_GCOALESCE``               ``ETHTOOL_MSG_COALESCE_GET``
+  ``ETHTOOL_SCOALESCE``               ``ETHTOOL_MSG_COALESCE_SET``
+  ``ETHTOOL_GRINGPARAM``              ``ETHTOOL_MSG_RINGS_GET``
+  ``ETHTOOL_SRINGPARAM``              ``ETHTOOL_MSG_RINGS_SET``
+  ``ETHTOOL_GPAUSEPARAM``             ``ETHTOOL_MSG_PAUSE_GET``
+  ``ETHTOOL_SPAUSEPARAM``             ``ETHTOOL_MSG_PAUSE_SET``
+  ``ETHTOOL_GRXCSUM``                 ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_SRXCSUM``                 ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GTXCSUM``                 ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_STXCSUM``                 ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GSG``                     ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_SSG``                     ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_TEST``                    n/a
+  ``ETHTOOL_GSTRINGS``                ``ETHTOOL_MSG_STRSET_GET``
+  ``ETHTOOL_PHYS_ID``                 n/a
+  ``ETHTOOL_GSTATS``                  n/a
+  ``ETHTOOL_GTSO``                    ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_STSO``                    ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GPERMADDR``               rtnetlink ``RTM_GETLINK``
+  ``ETHTOOL_GUFO``                    ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_SUFO``                    ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GGSO``                    ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_SGSO``                    ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GFLAGS``                  ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_SFLAGS``                  ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GPFLAGS``                 ``ETHTOOL_MSG_PRIVFLAGS_GET``
+  ``ETHTOOL_SPFLAGS``                 ``ETHTOOL_MSG_PRIVFLAGS_SET``
+  ``ETHTOOL_GRXFH``                   n/a
+  ``ETHTOOL_SRXFH``                   n/a
+  ``ETHTOOL_GGRO``                    ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_SGRO``                    ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GRXRINGS``                n/a
+  ``ETHTOOL_GRXCLSRLCNT``             n/a
+  ``ETHTOOL_GRXCLSRULE``              n/a
+  ``ETHTOOL_GRXCLSRLALL``             n/a
+  ``ETHTOOL_SRXCLSRLDEL``             n/a
+  ``ETHTOOL_SRXCLSRLINS``             n/a
+  ``ETHTOOL_FLASHDEV``                n/a
+  ``ETHTOOL_RESET``                   n/a
+  ``ETHTOOL_SRXNTUPLE``               n/a
+  ``ETHTOOL_GRXNTUPLE``               n/a
+  ``ETHTOOL_GSSET_INFO``              ``ETHTOOL_MSG_STRSET_GET``
+  ``ETHTOOL_GRXFHINDIR``              n/a
+  ``ETHTOOL_SRXFHINDIR``              n/a
+  ``ETHTOOL_GFEATURES``               ``ETHTOOL_MSG_FEATURES_GET``
+  ``ETHTOOL_SFEATURES``               ``ETHTOOL_MSG_FEATURES_SET``
+  ``ETHTOOL_GCHANNELS``               ``ETHTOOL_MSG_CHANNELS_GET``
+  ``ETHTOOL_SCHANNELS``               ``ETHTOOL_MSG_CHANNELS_SET``
+  ``ETHTOOL_SET_DUMP``                n/a
+  ``ETHTOOL_GET_DUMP_FLAG``           n/a
+  ``ETHTOOL_GET_DUMP_DATA``           n/a
+  ``ETHTOOL_GET_TS_INFO``             ``ETHTOOL_MSG_TSINFO_GET``
+  ``ETHTOOL_GMODULEINFO``             n/a
+  ``ETHTOOL_GMODULEEEPROM``           n/a
+  ``ETHTOOL_GEEE``                    ``ETHTOOL_MSG_EEE_GET``
+  ``ETHTOOL_SEEE``                    ``ETHTOOL_MSG_EEE_SET``
+  ``ETHTOOL_GRSSH``                   n/a
+  ``ETHTOOL_SRSSH``                   n/a
+  ``ETHTOOL_GTUNABLE``                n/a
+  ``ETHTOOL_STUNABLE``                n/a
+  ``ETHTOOL_GPHYSTATS``               n/a
+  ``ETHTOOL_PERQUEUE``                n/a
+  ``ETHTOOL_GLINKSETTINGS``           ``ETHTOOL_MSG_LINKINFO_GET``
+                                      ``ETHTOOL_MSG_LINKMODES_GET``
+  ``ETHTOOL_SLINKSETTINGS``           ``ETHTOOL_MSG_LINKINFO_SET``
+                                      ``ETHTOOL_MSG_LINKMODES_SET``
+  ``ETHTOOL_PHY_GTUNABLE``            n/a
+  ``ETHTOOL_PHY_STUNABLE``            n/a
+  ``ETHTOOL_GFECPARAM``               n/a
+  ``ETHTOOL_SFECPARAM``               n/a
+  n/a                                 ''ETHTOOL_MSG_CABLE_TEST_ACT''
+  n/a                                 ''ETHTOOL_MSG_CABLE_TEST_TDR_ACT''
+  n/a                                 ``ETHTOOL_MSG_TUNNEL_INFO_GET``
+  =================================== =====================================
-- 
2.34.1

