From 0d601a6e3b21b7c151ea7b58e02e13115983a0d0 Mon Sep 17 00:00:00 2001
From: Guangbin Huang <huangguangbin2@huawei.com>
Date: Tue, 28 Sep 2021 11:52:04 +0800
Subject: [PATCH 112/283] net: hns3: refactor function
 hclgevf_parse_capability()

mainline inclusion
from mainline-v5.15-rc1
commit 81414ba71356b174d62370195a2bb99592e1b2a2
category: feature
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EMYT
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=81414ba71356b174d62370195a2bb99592e1b2a2

----------------------------------------------------------------------

The function hclgevf_parse_capability() will add more if statement in the
future, to improve code readability, maintainability and simplicity,
refactor this function by using a bit mapping array of IMP capabilities
and driver capabilities.

Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Reviewed-by: Yongxin Li <liyongxin1@huawei.com>
Signed-off-by: Junxin Chen <chenjunxin1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>

 Conflicts:
	drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.c
---
 .../hisilicon/hns3/hns3vf/hclgevf_cmd.c       | 23 +++++++++++--------
 .../hisilicon/hns3/hns3vf/hclgevf_cmd.h       |  8 +++++++
 2 files changed, 22 insertions(+), 9 deletions(-)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.c b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.c
index 67d44d21814e..6e5d549f0adf 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.c
@@ -358,21 +358,26 @@ static void hclgevf_set_default_capability(struct hclgevf_dev *hdev)
 	set_bit(HNAE3_DEV_SUPPORT_FEC_B, ae_dev->caps);
 }
 
+const struct hclgevf_caps_bit_map hclgevf_cmd_caps_bit_map0[] = {
+	{HCLGEVF_CAP_UDP_GSO_B, HNAE3_DEV_SUPPORT_UDP_GSO_B},
+	{HCLGEVF_CAP_INT_QL_B, HNAE3_DEV_SUPPORT_INT_QL_B},
+	{HCLGEVF_CAP_TQP_TXRX_INDEP_B, HNAE3_DEV_SUPPORT_TQP_TXRX_INDEP_B},
+	{HCLGEVF_CAP_HW_TX_CSUM_B, HNAE3_DEV_SUPPORT_HW_TX_CSUM_B},
+	{HCLGEVF_CAP_UDP_TUNNEL_CSUM_B, HNAE3_DEV_SUPPORT_UDP_TUNNEL_CSUM_B},
+	{HCLGEVF_CAP_RXD_ADV_LAYOUT_B, HNAE3_DEV_SUPPORT_RXD_ADV_LAYOUT_B},
+};
+
 static void hclgevf_parse_capability(struct hclgevf_dev *hdev,
 				     struct hclgevf_query_version_cmd *cmd)
 {
 	struct hnae3_ae_dev *ae_dev = pci_get_drvdata(hdev->pdev);
-	u32 caps;
+	u32 caps, i;
 
 	caps = __le32_to_cpu(cmd->caps[0]);
-	if (hnae3_get_bit(caps, HCLGEVF_CAP_UDP_GSO_B))
-		set_bit(HNAE3_DEV_SUPPORT_UDP_GSO_B, ae_dev->caps);
-	if (hnae3_get_bit(caps, HCLGEVF_CAP_INT_QL_B))
-		set_bit(HNAE3_DEV_SUPPORT_INT_QL_B, ae_dev->caps);
-	if (hnae3_get_bit(caps, HCLGEVF_CAP_TQP_TXRX_INDEP_B))
-		set_bit(HNAE3_DEV_SUPPORT_TQP_TXRX_INDEP_B, ae_dev->caps);
-	if (hnae3_get_bit(caps, HCLGEVF_CAP_HW_TX_CSUM_B))
-		set_bit(HNAE3_DEV_SUPPORT_HW_TX_CSUM_B, ae_dev->caps);
+	for (i = 0; i < ARRAY_SIZE(hclgevf_cmd_caps_bit_map0); i++)
+		if (hnae3_get_bit(caps, hclgevf_cmd_caps_bit_map0[i].imp_bit))
+			set_bit(hclgevf_cmd_caps_bit_map0[i].local_bit,
+				ae_dev->caps);
 }
 
 static int hclgevf_cmd_query_version_and_capability(struct hclgevf_dev *hdev)
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.h b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.h
index 6a018a189097..824414e5fdf0 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_cmd.h
@@ -156,6 +156,8 @@ enum HCLGEVF_CAP_BITS {
 	HCLGEVF_CAP_TQP_TXRX_INDEP_B,
 	HCLGEVF_CAP_HW_PAD_B,
 	HCLGEVF_CAP_STASH_B,
+	HCLGEVF_CAP_UDP_TUNNEL_CSUM_B,
+	HCLGEVF_CAP_RXD_ADV_LAYOUT_B = 15,
 };
 
 #define HCLGEVF_QUERY_CAP_LENGTH		3
@@ -285,6 +287,12 @@ struct hclgevf_dev_specs_1_cmd {
        u8 rsv1[18];
 };
 
+/* capabilities bits map between imp firmware and local driver */
+struct hclgevf_caps_bit_map {
+	u16 imp_bit;
+	u16 local_bit;
+};
+
 static inline void hclgevf_write_reg(void __iomem *base, u32 reg, u32 value)
 {
 	writel(value, base + reg);
-- 
2.34.1

