From 3efcdbc96a9e44d11a381e2700d3e66c7077dbfc Mon Sep 17 00:00:00 2001
From: Peng Li <lipeng321@huawei.com>
Date: Tue, 28 Sep 2021 11:51:57 +0800
Subject: [PATCH 106/283] net: hns3: use memcpy to simplify code

mainline inclusion
from mainline-v5.15-rc1
commit 304cd8e776ddca5021dd9c1d7603ea40afc48ec6
category: feature
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EMYT
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=304cd8e776ddca5021dd9c1d7603ea40afc48ec6

----------------------------------------------------------------------

Use memcpy to copy req->msg.resp_data to resp->additional_info,
to simplify the code and improve a little efficiency.

Signed-off-by: Peng Li <lipeng321@huawei.com>
Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Reviewed-by: Yongxin Li <liyongxin1@huawei.com>
Signed-off-by: Junxin Chen <chenjunxin1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>
---
 drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_mbx.c | 9 ++-------
 1 file changed, 2 insertions(+), 7 deletions(-)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_mbx.c b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_mbx.c
index 244b83e22f53..41e303a42a9d 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_mbx.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_mbx.c
@@ -189,8 +189,6 @@ void hclgevf_mbx_handler(struct hclgevf_dev *hdev)
 	struct hclgevf_desc *desc;
 	u16 *msg_q;
 	u16 flag;
-	u8 *temp;
-	int i;
 
 	resp = &hdev->mbx_resp;
 	crq = &hdev->hw.cmq.crq;
@@ -237,11 +235,8 @@ void hclgevf_mbx_handler(struct hclgevf_dev *hdev)
 			resp->resp_status =
 				hclgevf_resp_to_errno(req->msg.resp_status);
 
-			temp = (u8 *)req->msg.resp_data;
-			for (i = 0; i < HCLGE_MBX_MAX_RESP_DATA_SIZE; i++) {
-				resp->additional_info[i] = *temp;
-				temp++;
-			}
+			memcpy(resp->additional_info, req->msg.resp_data,
+			       HCLGE_MBX_MAX_RESP_DATA_SIZE * sizeof(u8));
 
 			/* ensure additional_info will be seen before setting
 			 * received_resp
-- 
2.34.1

