From 9336c101918a51d00f6a5508cd5290be5c1596ee Mon Sep 17 00:00:00 2001
From: John Garry <john.garry@huawei.com>
Date: Fri, 28 Feb 2020 23:18:51 +0800
Subject: [PATCH 28/39] spi: HiSilicon v3xx: Use DMI quirk to set controller
 buswidth override bits

mainline inclusion
from mainline-v5.7-rc1
commit 34e608b023e96f51b31274435b49c8ae61e2389f
category: feature
bugzilla: https://gitee.com/openeuler/kernel/issues/I8CSBP
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=34e608b023e96f51b31274435b49c8ae61e2389f

----------------------------------------------------------------------------

The Huawei D06 board (and variants) can support Quad mode of operation.

Since we have no current method in ACPI SPI bus device resource description
to describe this information, use DMI to detect the board, and set the
controller buswidth override bits.

Signed-off-by: John Garry <john.garry@huawei.com>
Link: https://lore.kernel.org/r/1582903131-160033-4-git-send-email-john.garry@huawei.com
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: YunYi Yang <yangyunyi2@huawei.com>
---
 drivers/spi/spi-hisi-sfc-v3xx.c | 56 ++++++++++++++++++++++++++++++++-
 1 file changed, 55 insertions(+), 1 deletion(-)

diff --git a/drivers/spi/spi-hisi-sfc-v3xx.c b/drivers/spi/spi-hisi-sfc-v3xx.c
index 8c2eea439d5b..c46812f004b7 100644
--- a/drivers/spi/spi-hisi-sfc-v3xx.c
+++ b/drivers/spi/spi-hisi-sfc-v3xx.c
@@ -7,6 +7,7 @@
 
 #include <linux/acpi.h>
 #include <linux/bitops.h>
+#include <linux/dmi.h>
 #include <linux/iopoll.h>
 #include <linux/module.h>
 #include <linux/platform_device.h>
@@ -246,6 +247,44 @@ static const struct spi_controller_mem_ops hisi_sfc_v3xx_mem_ops = {
 	.exec_op = hisi_sfc_v3xx_exec_op,
 };
 
+static int hisi_sfc_v3xx_buswidth_override_bits;
+
+/*
+ * ACPI FW does not allow us to currently set the device buswidth, so quirk it
+ * depending on the board.
+ */
+static int __init hisi_sfc_v3xx_dmi_quirk(const struct dmi_system_id *d)
+{
+	hisi_sfc_v3xx_buswidth_override_bits = SPI_RX_QUAD | SPI_TX_QUAD;
+
+	return 0;
+}
+
+static const struct dmi_system_id hisi_sfc_v3xx_dmi_quirk_table[]  = {
+	{
+	.callback = hisi_sfc_v3xx_dmi_quirk,
+	.matches = {
+		DMI_MATCH(DMI_SYS_VENDOR, "Huawei"),
+		DMI_MATCH(DMI_PRODUCT_NAME, "D06"),
+	},
+	},
+	{
+	.callback = hisi_sfc_v3xx_dmi_quirk,
+	.matches = {
+		DMI_MATCH(DMI_SYS_VENDOR, "Huawei"),
+		DMI_MATCH(DMI_PRODUCT_NAME, "TaiShan 2280 V2"),
+	},
+	},
+	{
+	.callback = hisi_sfc_v3xx_dmi_quirk,
+	.matches = {
+		DMI_MATCH(DMI_SYS_VENDOR, "Huawei"),
+		DMI_MATCH(DMI_PRODUCT_NAME, "TaiShan 200 (Model 2280)"),
+	},
+	},
+	{}
+};
+
 static int hisi_sfc_v3xx_probe(struct platform_device *pdev)
 {
 	struct device *dev = &pdev->dev;
@@ -261,6 +300,8 @@ static int hisi_sfc_v3xx_probe(struct platform_device *pdev)
 	ctlr->mode_bits = SPI_RX_DUAL | SPI_RX_QUAD |
 			  SPI_TX_DUAL | SPI_TX_QUAD;
 
+	ctlr->buswidth_override_bits = hisi_sfc_v3xx_buswidth_override_bits;
+
 	host = spi_controller_get_devdata(ctlr);
 	host->dev = dev;
 
@@ -316,7 +357,20 @@ static struct platform_driver hisi_sfc_v3xx_spi_driver = {
 	.probe	= hisi_sfc_v3xx_probe,
 };
 
-module_platform_driver(hisi_sfc_v3xx_spi_driver);
+static int __init hisi_sfc_v3xx_spi_init(void)
+{
+	dmi_check_system(hisi_sfc_v3xx_dmi_quirk_table);
+
+	return platform_driver_register(&hisi_sfc_v3xx_spi_driver);
+}
+
+static void __exit hisi_sfc_v3xx_spi_exit(void)
+{
+	platform_driver_unregister(&hisi_sfc_v3xx_spi_driver);
+}
+
+module_init(hisi_sfc_v3xx_spi_init);
+module_exit(hisi_sfc_v3xx_spi_exit);
 
 MODULE_LICENSE("GPL");
 MODULE_AUTHOR("John Garry <john.garry@huawei.com>");
-- 
2.27.0

