From e01061aeb9fc278e1c9f0b2c6d667a7edaea41ec Mon Sep 17 00:00:00 2001
From: Hao Chen <chenhao288@hisilicon.com>
Date: Sat, 26 Mar 2022 17:51:01 +0800
Subject: [PATCH 271/283] net: hns3: add max order judgement for tx spare
 buffer

mainline inclusion
from mainline-v5.18-rc1
commit a89cbb16995bf15582e0d1bdb922ad1a54a2fa8c
category: bugfix
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EN49

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=a89cbb16995bf15582e0d1bdb922ad1a54a2fa8c

--------------------------------

Add max order judgement for tx spare buffer to avoid triggering
call trace, print related fail information instead, when user
set tx spare buf size to a large value which causes order
exceeding 10.

Fixes: e445f08af2b1 ("net: hns3: add support to set/get tx copybreak buf size via ethtool for hns3 driver")
Signed-off-by: Hao Chen <chenhao288@hisilicon.com>
Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>
---
 drivers/net/ethernet/hisilicon/hns3/hns3_enet.c | 6 ++++++
 1 file changed, 6 insertions(+)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c
index f9dacf01ddd6..5c723c532289 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c
@@ -746,6 +746,12 @@ static void hns3_init_tx_spare_buffer(struct hns3_enet_ring *ring)
 		return;
 
 	order = get_order(alloc_size);
+	if (order >= MAX_ORDER) {
+		if (net_ratelimit())
+			dev_warn(ring_to_dev(ring), "failed to allocate tx spare buffer, exceed to max order\n");
+		return;
+	}
+
 	tx_spare = devm_kzalloc(ring_to_dev(ring), sizeof(*tx_spare),
 				GFP_KERNEL);
 	if (!tx_spare) {
-- 
2.34.1

