From 3fb5bcdbcd9ceaf3d8d69f8ba5a20c692c3ba105 Mon Sep 17 00:00:00 2001
From: Ard Biesheuvel <ard.biesheuvel@linaro.org>
Date: Thu, 30 May 2019 13:16:34 +0200
Subject: [PATCH 22/39] spi/acpi: enumerate all SPI slaves in the namespace

mainline inclusion
from mainline-v5.3-rc1
commit 4c3c59544f33e97cf8557f27e05a9904ead16363
category: bugfix
bugzilla: https://gitee.com/openeuler/kernel/issues/I8CSBP
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=4c3c59544f33e97cf8557f27e05a9904ead16363

----------------------------------------------------------------------------

Currently, the ACPI enumeration that takes place when registering a
SPI master only considers immediate child devices in the ACPI namespace,
rather than checking the ResourceSource field in the SpiSerialBus()
resource descriptor.

This is incorrect: SPI slaves could reside anywhere in the ACPI
namespace, and so we should enumerate the entire namespace and look for
any device that refers to the newly registered SPI master in its
resource descriptor.

So refactor the existing code and use a lookup structure so that
allocating the SPI device structure is deferred until we have identified
the device as an actual child of the controller. This approach is
loosely based on the way the I2C subsystem handles ACPI enumeration.

Note that Apple x86 hardware does not rely on SpiSerialBus() resources
in _CRS but uses nested devices below the controller's device node in
the ACPI namespace, with a special set of device properties. This means
we have to take care to only parse those properties for device nodes
that are direct children of the controller node.

Cc: Mika Westerberg <mika.westerberg@linux.intel.com>
Cc: linux-spi@vger.kernel.org
Cc: broonie@kernel.org
Cc: andy.shevchenko@gmail.com
Cc: masahisa.kojima@linaro.org
Cc: "Rafael J. Wysocki" <rjw@rjwysocki.net>
Cc: Jarkko Nikula <jarkko.nikula@linux.intel.com>
Cc: linux-acpi@vger.kernel.org
Cc: Lukas Wunner <lukas@wunner.de>

Signed-off-by: Ard Biesheuvel <ard.biesheuvel@linaro.org>
Signed-off-by: Mark Brown <broonie@kernel.org>
Signed-off-by: YunYi Yang <yangyunyi2@huawei.com>
---
 drivers/spi/spi.c | 104 ++++++++++++++++++++++++++++++++--------------
 1 file changed, 73 insertions(+), 31 deletions(-)

diff --git a/drivers/spi/spi.c b/drivers/spi/spi.c
index 08c7c8ee3271..c6e272edd806 100644
--- a/drivers/spi/spi.c
+++ b/drivers/spi/spi.c
@@ -1732,9 +1732,18 @@ static void of_register_spi_devices(struct spi_controller *ctlr) { }
 #endif
 
 #ifdef CONFIG_ACPI
-static void acpi_spi_parse_apple_properties(struct spi_device *spi)
+struct acpi_spi_lookup {
+	struct spi_controller   *ctlr;
+	u32			max_speed_hz;
+	u32			mode;
+	int			irq;
+	u8			bits_per_word;
+	u8			chip_select;
+};
+
+static void acpi_spi_parse_apple_properties(struct acpi_device *dev,
+					    struct acpi_spi_lookup *lookup)
 {
-	struct acpi_device *dev = ACPI_COMPANION(&spi->dev);
 	const union acpi_object *obj;
 
 	if (!x86_apple_machine)
@@ -1742,35 +1751,47 @@ static void acpi_spi_parse_apple_properties(struct spi_device *spi)
 
 	if (!acpi_dev_get_property(dev, "spiSclkPeriod", ACPI_TYPE_BUFFER, &obj)
 	    && obj->buffer.length >= 4)
-		spi->max_speed_hz  = NSEC_PER_SEC / *(u32 *)obj->buffer.pointer;
+		lookup->max_speed_hz  = NSEC_PER_SEC /
+					*(u32 *)obj->buffer.pointer;
 
 	if (!acpi_dev_get_property(dev, "spiWordSize", ACPI_TYPE_BUFFER, &obj)
 	    && obj->buffer.length == 8)
-		spi->bits_per_word = *(u64 *)obj->buffer.pointer;
+		lookup->bits_per_word = *(u64 *)obj->buffer.pointer;
 
 	if (!acpi_dev_get_property(dev, "spiBitOrder", ACPI_TYPE_BUFFER, &obj)
 	    && obj->buffer.length == 8 && !*(u64 *)obj->buffer.pointer)
-		spi->mode |= SPI_LSB_FIRST;
+		lookup->mode |= SPI_LSB_FIRST;
 
 	if (!acpi_dev_get_property(dev, "spiSPO", ACPI_TYPE_BUFFER, &obj)
 	    && obj->buffer.length == 8 &&  *(u64 *)obj->buffer.pointer)
-		spi->mode |= SPI_CPOL;
+		lookup->mode |= SPI_CPOL;
 
 	if (!acpi_dev_get_property(dev, "spiSPH", ACPI_TYPE_BUFFER, &obj)
 	    && obj->buffer.length == 8 &&  *(u64 *)obj->buffer.pointer)
-		spi->mode |= SPI_CPHA;
+		lookup->mode |= SPI_CPHA;
 }
 
 static int acpi_spi_add_resource(struct acpi_resource *ares, void *data)
 {
-	struct spi_device *spi = data;
-	struct spi_controller *ctlr = spi->controller;
+	struct acpi_spi_lookup *lookup = data;
+	struct spi_controller *ctlr = lookup->ctlr;
 
 	if (ares->type == ACPI_RESOURCE_TYPE_SERIAL_BUS) {
 		struct acpi_resource_spi_serialbus *sb;
+		acpi_handle parent_handle;
+		acpi_status status;
 
 		sb = &ares->data.spi_serial_bus;
 		if (sb->type == ACPI_RESOURCE_SERIAL_TYPE_SPI) {
+
+			status = acpi_get_handle(NULL,
+						 sb->resource_source.string_ptr,
+						 &parent_handle);
+
+			if (!status ||
+			    ACPI_HANDLE(ctlr->dev.parent) != parent_handle)
+				return -ENODEV;
+
 			/*
 			 * ACPI DeviceSelection numbering is handled by the
 			 * host controller driver in Windows and can vary
@@ -1783,25 +1804,25 @@ static int acpi_spi_add_resource(struct acpi_resource *ares, void *data)
 						sb->device_selection);
 				if (cs < 0)
 					return cs;
-				spi->chip_select = cs;
+				lookup->chip_select = cs;
 			} else {
-				spi->chip_select = sb->device_selection;
+				lookup->chip_select = sb->device_selection;
 			}
 
-			spi->max_speed_hz = sb->connection_speed;
+			lookup->max_speed_hz = sb->connection_speed;
 
 			if (sb->clock_phase == ACPI_SPI_SECOND_PHASE)
-				spi->mode |= SPI_CPHA;
+				lookup->mode |= SPI_CPHA;
 			if (sb->clock_polarity == ACPI_SPI_START_HIGH)
-				spi->mode |= SPI_CPOL;
+				lookup->mode |= SPI_CPOL;
 			if (sb->device_polarity == ACPI_SPI_ACTIVE_HIGH)
-				spi->mode |= SPI_CS_HIGH;
+				lookup->mode |= SPI_CS_HIGH;
 		}
-	} else if (spi->irq < 0) {
+	} else if (lookup->irq < 0) {
 		struct resource r;
 
 		if (acpi_dev_resource_interrupt(ares, 0, &r))
-			spi->irq = r.start;
+			lookup->irq = r.start;
 	}
 
 	/* Always tell the ACPI core to skip this resource */
@@ -1811,7 +1832,9 @@ static int acpi_spi_add_resource(struct acpi_resource *ares, void *data)
 static acpi_status acpi_register_spi_device(struct spi_controller *ctlr,
 					    struct acpi_device *adev)
 {
+	acpi_handle parent_handle = NULL;
 	struct list_head resource_list;
+	struct acpi_spi_lookup lookup;
 	struct spi_device *spi;
 	int ret;
 
@@ -1819,28 +1842,44 @@ static acpi_status acpi_register_spi_device(struct spi_controller *ctlr,
 	    acpi_device_enumerated(adev))
 		return AE_OK;
 
-	spi = spi_alloc_device(ctlr);
-	if (!spi) {
-		dev_err(&ctlr->dev, "failed to allocate SPI device for %s\n",
-			dev_name(&adev->dev));
-		return AE_NO_MEMORY;
-	}
-
-	ACPI_COMPANION_SET(&spi->dev, adev);
-	spi->irq = -1;
+	lookup.ctlr		= ctlr;
+	lookup.mode		= 0;
+	lookup.bits_per_word	= 0;
+	lookup.irq		= -1;
 
 	INIT_LIST_HEAD(&resource_list);
 	ret = acpi_dev_get_resources(adev, &resource_list,
-				     acpi_spi_add_resource, spi);
+				     acpi_spi_add_resource, &lookup);
 	acpi_dev_free_resource_list(&resource_list);
 
-	acpi_spi_parse_apple_properties(spi);
+	if (ret < 0)
+		/* found SPI in _CRS but it points to another controller */
+		return AE_OK;
 
-	if (ret < 0 || !spi->max_speed_hz) {
-		spi_dev_put(spi);
+	if (!lookup.max_speed_hz &&
+	    !ACPI_FAILURE(acpi_get_parent(adev->handle, &parent_handle)) &&
+	    ACPI_HANDLE(ctlr->dev.parent) == parent_handle) {
+		/* Apple does not use _CRS but nested devices for SPI slaves */
+		acpi_spi_parse_apple_properties(adev, &lookup);
+	}
+
+	if (!lookup.max_speed_hz)
 		return AE_OK;
+
+	spi = spi_alloc_device(ctlr);
+	if (!spi) {
+		dev_err(&ctlr->dev, "failed to allocate SPI device for %s\n",
+			dev_name(&adev->dev));
+		return AE_NO_MEMORY;
 	}
 
+	ACPI_COMPANION_SET(&spi->dev, adev);
+	spi->max_speed_hz	= lookup.max_speed_hz;
+	spi->mode		= lookup.mode;
+	spi->irq		= lookup.irq;
+	spi->bits_per_word	= lookup.bits_per_word;
+	spi->chip_select	= lookup.chip_select;
+
 	acpi_set_modalias(adev, acpi_device_hid(adev), spi->modalias,
 			  sizeof(spi->modalias));
 
@@ -1872,6 +1911,8 @@ static acpi_status acpi_spi_add_device(acpi_handle handle, u32 level,
 	return acpi_register_spi_device(ctlr, adev);
 }
 
+#define SPI_ACPI_ENUMERATE_MAX_DEPTH		32
+
 static void acpi_register_spi_devices(struct spi_controller *ctlr)
 {
 	acpi_status status;
@@ -1881,7 +1922,8 @@ static void acpi_register_spi_devices(struct spi_controller *ctlr)
 	if (!handle)
 		return;
 
-	status = acpi_walk_namespace(ACPI_TYPE_DEVICE, handle, 1,
+	status = acpi_walk_namespace(ACPI_TYPE_DEVICE, ACPI_ROOT_OBJECT,
+				     SPI_ACPI_ENUMERATE_MAX_DEPTH,
 				     acpi_spi_add_device, NULL, ctlr, NULL);
 	if (ACPI_FAILURE(status))
 		dev_warn(&ctlr->dev, "failed to enumerate SPI slaves\n");
-- 
2.27.0

