From 9b807d024192580ae0e7dfda33f72a06379047f8 Mon Sep 17 00:00:00 2001
From: John Garry <john.garry@huawei.com>
Date: Tue, 15 Nov 2022 23:03:48 +0800
Subject: [PATCH 091/108] scsi: hisi_sas: Fix rescan after deleting a disk

mainline inclusion
from mainline-v5.19-rc1
commit e9dedc13bb11bc553754abecb322e5e41d1b4fef
category: bugfix
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8F85H

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=e9dedc13bb11bc553754abecb322e5e41d1b4fef

----------------------------------------------------------------------

Removing an ATA device via sysfs means that the device may not be found
through re-scanning:

root@ubuntu:/home/john# lsscsi
[0:0:0:0] disk SanDisk LT0200MO P404 /dev/sda
[0:0:1:0] disk ATA HGST HUS724040AL A8B0 /dev/sdb
[0:0:8:0] enclosu 12G SAS Expander RevB -
root@ubuntu:/home/john# echo 1 > /sys/block/sdb/device/delete
root@ubuntu:/home/john# echo "- - -" > /sys/class/scsi_host/host0/scan
root@ubuntu:/home/john# lsscsi
[0:0:0:0] disk SanDisk LT0200MO P404 /dev/sda
[0:0:8:0] enclosu 12G SAS Expander RevB -
root@ubuntu:/home/john#

The problem is that the rescan of the device may conflict with the device
in being re-initialized, as follows:

 - In the rescan we call hisi_sas_slave_alloc() in store_scan() ->
   sas_user_scan() -> [__]scsi_scan_target() -> scsi_probe_and_add_lunc()
   -> scsi_alloc_sdev() -> hisi_sas_slave_alloc() -> hisi_sas_init_device()
   In hisi_sas_init_device() we issue an IT nexus reset for ATA devices

 - That IT nexus causes the remote PHY to go down and this triggers a bcast
   event

 - In parallel libsas processes the bcast event, finds that the phy is down
   and marks the device as gone

The hard reset issued in hisi_sas_init_device() is unncessary - as
described in the code comment - so remove it. Also set dev status as
HISI_SAS_DEV_NORMAL as the hisi_sas_init_device() call.

Link: https://lore.kernel.org/r/1652354134-171343-4-git-send-email-john.garry@huawei.com
Fixes: 36c6b7613ef1 ("scsi: hisi_sas: Initialise devices in .slave_alloc callback")
Tested-by: Yihang Li <liyihang6@hisilicon.com>
Reviewed-by: Xiang Chen <chenxiang66@hisilicon.com>
Signed-off-by: John Garry <john.garry@huawei.com>
Signed-off-by: Martin K. Petersen <martin.petersen@oracle.com>
Signed-off-by: xiabing <xiabing12@h-partners.com>
Reviewed-by: Jason Yan <yanaijie@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: YunYi Yang <yangyunyi2@huawei.com>

 Conflicts:
	drivers/scsi/hisi_sas/hisi_sas_main.c
---
 drivers/scsi/hisi_sas/hisi_sas_main.c | 48 ++++++++++-----------------
 1 file changed, 18 insertions(+), 30 deletions(-)

diff --git a/drivers/scsi/hisi_sas/hisi_sas_main.c b/drivers/scsi/hisi_sas/hisi_sas_main.c
index 48831be1b912..e53444568c12 100644
--- a/drivers/scsi/hisi_sas/hisi_sas_main.c
+++ b/drivers/scsi/hisi_sas/hisi_sas_main.c
@@ -704,8 +704,6 @@ static int hisi_sas_init_device(struct domain_device *device)
 	struct hisi_sas_tmf_task tmf_task;
 	int retry = HISI_SAS_DISK_RECOVER_CNT;
 	struct hisi_hba *hisi_hba = dev_to_hisi_hba(device);
-	struct device *dev = hisi_hba->dev;
-	struct sas_phy *local_phy;
 
 	switch (device->dev_type) {
 	case SAS_END_DEVICE:
@@ -726,31 +724,18 @@ static int hisi_sas_init_device(struct domain_device *device)
 	case SAS_SATA_PM_PORT:
 	case SAS_SATA_PENDING:
 		/*
-		 * send HARD RESET to clear previous affiliation of
-		 * STP target port
+		 * If an expander is swapped when a SATA disk is attached then
+		 * we should issue a hard reset to clear previous affiliation
+		 * of STP target port, see SPL (chapter 6.19.4).
+		 *
+		 * However we don't need to issue a hard reset here for these
+		 * reasons:
+		 * a. When probing the device, libsas/libata already issues a
+		 * hard reset in sas_probe_sata() -> ata_sas_async_probe().
+		 * Note that in hisi_sas_debug_I_T_nexus_reset() we take care
+		 * to issue a hard reset by checking the dev status (== INIT).
+		 * b. When resetting the controller, this is simply unnecessary.
 		 */
-		local_phy = sas_get_local_phy(device);
-		if (!scsi_is_sas_phy_local(local_phy) &&
-		    !test_bit(HISI_SAS_RESET_BIT, &hisi_hba->flags)) {
-			unsigned long deadline = ata_deadline(jiffies, 20000);
-			struct sata_device *sata_dev = &device->sata_dev;
-			struct ata_host *ata_host = sata_dev->ata_host;
-			struct ata_port_operations *ops = ata_host->ops;
-			struct ata_port *ap = sata_dev->ap;
-			struct ata_link *link;
-			unsigned int classes;
-
-			ata_for_each_link(link, ap, EDGE)
-				rc = ops->hardreset(link, &classes,
-						    deadline);
-		}
-		sas_put_local_phy(local_phy);
-		if (rc) {
-			dev_warn(dev, "SATA disk hardreset fail: %d\n",
-				 rc);
-			return rc;
-		}
-
 		while (retry-- > 0) {
 			rc = hisi_sas_softreset_ata_disk(device);
 			if (!rc)
@@ -766,15 +751,19 @@ static int hisi_sas_init_device(struct domain_device *device)
 
 int hisi_sas_slave_alloc(struct scsi_device *sdev)
 {
-	struct domain_device *ddev;
+	struct domain_device *ddev = sdev_to_domain_dev(sdev);
+	struct hisi_sas_device *sas_dev = ddev->lldd_dev;
 	int rc;
 
 	rc = sas_slave_alloc(sdev);
 	if (rc)
 		return rc;
-	ddev = sdev_to_domain_dev(sdev);
 
-	return hisi_sas_init_device(ddev);
+	rc = hisi_sas_init_device(ddev);
+	if (rc)
+		return rc;
+	sas_dev->dev_status = HISI_SAS_DEV_NORMAL;
+	return 0;
 }
 EXPORT_SYMBOL_GPL(hisi_sas_slave_alloc);
 
@@ -824,7 +813,6 @@ static int hisi_sas_dev_found(struct domain_device *device)
 	dev_info(dev, "dev[%d:%x] found\n",
 		sas_dev->device_id, sas_dev->dev_type);
 
-	sas_dev->dev_status = HISI_SAS_DEV_NORMAL;
 	return 0;
 
 err_out:
-- 
2.27.0

