From 2a1e73290fad59f6de2535591b2aa6ef6218a9f0 Mon Sep 17 00:00:00 2001
From: Huazhong Tan <tanhuazhong@huawei.com>
Date: Thu, 18 Nov 2021 20:44:40 +0800
Subject: [PATCH 253/283] net: hns3: add debugfs support for interrupt coalesce

mainline inclusion
from mainline-v5.16-rc1
commit c99fead7cb07979f5db38035ccb5f02ad2c7106a
category: feature
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EN49
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=c99fead7cb07979f5db38035ccb5f02ad2c7106a

----------------------------------------------------------------------

Since user may need to check the current configuration of the
interrupt coalesce, so add debugfs support for query this info.

Create a single file "coalesce_info" for it, and query it by
"cat coalesce_info", return the result to userspace.

For device whose version is above V3(include V3), the GL's register
contains usecs and 1us unit configuration. When get the usecs
configuration from this register, it will include the confusing unit
configuration, so add a GL mask to get the correct value, and add
a QL mask for the frames configuration as well.

The display style is below:
$ cat coalesce_info
tx interrupt coalesce info:
VEC_ID  ALGO_STATE  PROFILE_ID  CQE_MODE  TUNE_STATE  STEPS_LEFT...
0       IN_PROG     4           EQE       ON_TOP      0...
1       START       3           EQE       LEFT        1...

rx interrupt coalesce info:
VEC_ID  ALGO_STATE  PROFILE_ID  CQE_MODE  TUNE_STATE  STEPS_LEFT...
0       IN_PROG     3           EQE       LEFT        1...
1       IN_PROG     0           EQE       ON_TOP      0...

Signed-off-by: Huazhong Tan <tanhuazhong@huawei.com>
Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Reviewed-by: Yongxin Li <liyongxin1@huawei.com>
Signed-off-by: Junxin Chen <chenjunxin1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>

 Conflicts:
	drivers/net/ethernet/hisilicon/hns3/hnae3.h
	drivers/net/ethernet/hisilicon/hns3/hns3_enet.h
---
 .../ethernet/hisilicon/hns3/hns3_debugfs.c    | 108 ++++++++++++++++++
 .../net/ethernet/hisilicon/hns3/hns3_enet.h   |   2 +
 2 files changed, 110 insertions(+)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_debugfs.c b/drivers/net/ethernet/hisilicon/hns3/hns3_debugfs.c
index 5e4be179cf99..e96d44e3e716 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_debugfs.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_debugfs.c
@@ -322,6 +322,13 @@ static struct hns3_dbg_cmd_info hns3_dbg_cmd[] = {
 		.buf_len = HNS3_DBG_READ_LEN,
 		.init = hns3_dbg_common_file_init,
 	},
+	{
+		.name = "coalesce_info",
+		.cmd = HNAE3_DBG_CMD_COAL_INFO,
+		.dentry = HNS3_DBG_DENTRY_COMMON,
+		.buf_len = HNS3_DBG_READ_LEN_1MB,
+		.init = hns3_dbg_common_file_init,
+	},
 };
 
 static struct hns3_dbg_cap_info hns3_dbg_cap[] = {
@@ -379,6 +386,26 @@ static struct hns3_dbg_cap_info hns3_dbg_cap[] = {
 	}
 };
 
+static const struct hns3_dbg_item coal_info_items[] = {
+	{ "VEC_ID", 2 },
+	{ "ALGO_STATE", 2 },
+	{ "PROFILE_ID", 2 },
+	{ "CQE_MODE", 2 },
+	{ "TUNE_STATE", 2 },
+	{ "STEPS_LEFT", 2 },
+	{ "STEPS_RIGHT", 2 },
+	{ "TIRED", 2 },
+	{ "SW_GL", 2 },
+	{ "SW_QL", 2 },
+	{ "HW_GL", 2 },
+	{ "HW_QL", 2 },
+};
+
+static const char * const dim_cqe_mode_str[] = { "EQE", "CQE" };
+static const char * const dim_state_str[] = { "START", "IN_PROG", "APPLY" };
+static const char * const
+dim_tune_stat_str[] = { "ON_TOP", "TIRED", "RIGHT", "LEFT" };
+
 static void hns3_dbg_fill_content(char *content, u16 len,
 				  const struct hns3_dbg_item *items,
 				  const char **result, u16 size)
@@ -417,6 +444,83 @@ static void hns3_dbg_fill_content(char *content, u16 len,
 	*pos++ = '\0';
 }
 
+static void hns3_get_coal_info(struct hns3_enet_tqp_vector *tqp_vector,
+			       char **result, int i, bool is_tx)
+{
+	unsigned int gl_offset, ql_offset;
+	struct hns3_enet_coalesce *coal;
+	unsigned int reg_val;
+	unsigned int j = 0;
+	bool ql_enable;
+
+	if (is_tx) {
+		coal = &tqp_vector->tx_group.coal;
+		gl_offset = HNS3_VECTOR_GL1_OFFSET;
+		ql_offset = HNS3_VECTOR_TX_QL_OFFSET;
+		ql_enable = tqp_vector->tx_group.coal.ql_enable;
+	} else {
+		coal = &tqp_vector->rx_group.coal;
+		gl_offset = HNS3_VECTOR_GL0_OFFSET;
+		ql_offset = HNS3_VECTOR_RX_QL_OFFSET;
+		ql_enable = tqp_vector->rx_group.coal.ql_enable;
+	}
+
+	sprintf(result[j++], "%d", i);
+	sprintf(result[j++], "%u", coal->int_gl);
+	sprintf(result[j++], "%u", coal->int_ql);
+	reg_val = readl(tqp_vector->mask_addr + gl_offset) &
+		  HNS3_VECTOR_GL_MASK;
+	sprintf(result[j++], "%u", reg_val);
+	if (ql_enable) {
+		reg_val = readl(tqp_vector->mask_addr + ql_offset) &
+			  HNS3_VECTOR_QL_MASK;
+		sprintf(result[j++], "%u", reg_val);
+	} else {
+		sprintf(result[j++], "NA");
+	}
+}
+
+static void hns3_dump_coal_info(struct hnae3_handle *h, char *buf, int len,
+				int *pos, bool is_tx)
+{
+	char data_str[ARRAY_SIZE(coal_info_items)][HNS3_DBG_DATA_STR_LEN];
+	char *result[ARRAY_SIZE(coal_info_items)];
+	struct hns3_enet_tqp_vector *tqp_vector;
+	struct hns3_nic_priv *priv = h->priv;
+	char content[HNS3_DBG_INFO_LEN];
+	unsigned int i;
+
+	for (i = 0; i < ARRAY_SIZE(coal_info_items); i++)
+		result[i] = &data_str[i][0];
+
+	*pos += scnprintf(buf + *pos, len - *pos,
+			  "%s interrupt coalesce info:\n",
+			  is_tx ? "tx" : "rx");
+	hns3_dbg_fill_content(content, sizeof(content), coal_info_items,
+			      NULL, ARRAY_SIZE(coal_info_items));
+	*pos += scnprintf(buf + *pos, len - *pos, "%s", content);
+
+	for (i = 0; i < priv->vector_num; i++) {
+		tqp_vector = &priv->tqp_vector[i];
+		hns3_get_coal_info(tqp_vector, result, i, is_tx);
+		hns3_dbg_fill_content(content, sizeof(content), coal_info_items,
+				      (const char **)result,
+				      ARRAY_SIZE(coal_info_items));
+		*pos += scnprintf(buf + *pos, len - *pos, "%s", content);
+	}
+}
+
+static int hns3_dbg_coal_info(struct hnae3_handle *h, char *buf, int len)
+{
+	int pos = 0;
+
+	hns3_dump_coal_info(h, buf, len, &pos, true);
+	pos += scnprintf(buf + pos, len - pos, "\n");
+	hns3_dump_coal_info(h, buf, len, &pos, false);
+
+	return 0;
+}
+
 static const struct hns3_dbg_item tx_spare_info_items[] = {
 	{ "QUEUE_ID", 2 },
 	{ "COPYBREAK", 2 },
@@ -976,6 +1080,10 @@ static const struct hns3_dbg_func hns3_dbg_cmd_func[] = {
 		.cmd = HNAE3_DBG_CMD_DEV_INFO,
 		.dbg_dump = hns3_dbg_dev_info,
 	},
+	{
+		.cmd = HNAE3_DBG_CMD_COAL_INFO,
+		.dbg_dump = hns3_dbg_coal_info,
+	},
 };
 
 static int hns3_dbg_read_cmd(struct hns3_dbg_data *dbg_data,
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h
index 163f7cdadd54..36342762f85d 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.h
@@ -200,11 +200,13 @@ enum hns3_nic_state {
 #define HNS3_MAX_NON_TSO_SIZE			9728U
 #define HNS3_MAX_BD_SIZE_OFFSET			16
 
+#define HNS3_VECTOR_GL_MASK			GENMASK(11, 0)
 #define HNS3_VECTOR_GL0_OFFSET			0x100
 #define HNS3_VECTOR_GL1_OFFSET			0x200
 #define HNS3_VECTOR_GL2_OFFSET			0x300
 #define HNS3_VECTOR_RL_OFFSET			0x900
 #define HNS3_VECTOR_RL_EN_B			6
+#define HNS3_VECTOR_QL_MASK			GENMASK(9, 0)
 #define HNS3_VECTOR_TX_QL_OFFSET		0xe00
 #define HNS3_VECTOR_RX_QL_OFFSET		0xf00
 
-- 
2.34.1

