From 71cf98350d1423660b390740a190ce8a98502c37 Mon Sep 17 00:00:00 2001
From: Shaokun Zhang <zhangshaokun@hisilicon.com>
Date: Fri, 30 Jul 2021 15:44:09 +0800
Subject: [PATCH 20/55] drivers/perf: hisi: Add support for HiSilicon PA PMU
 driver

mainline inclusion
from mainline-v5.12-rc3
commit a0ab25cd82eeb68bfa19a4d93a097521af5011b8
category: feature
bugzilla: 175148
CVE: NA
Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=a0ab25cd82eeb68bfa19a4d93a097521af5011b8

------------------------------------------------------------------------

On HiSilicon Hip09 platform, there is a PA (Protocol Adapter) module on
each chip SICL (Super I/O Cluster) which incorporates three Hydra interface
and facilitates the cache coherency between the dies on the chip. While PA
uncore PMU model is the same as other Hip09 PMU modules and many PMU events
are supported. Let's support the PMU driver using the HiSilicon uncore PMU
framework.

PA PMU supports the following filter functions:
* tracetag_en: allows user to count events according to tt_req or
tt_core set in L3C PMU. It's the same as other PMUs.

* srcid_cmd & srcid_msk: allows user to filter statistics that come from
specific CCL/ICL by configuration source ID.

* tgtid_cmd & tgtid_msk: it is the similar function to srcid_cmd &
srcid_msk. Both are used to check where the data comes from or go to.

Cc: Mark Rutland <mark.rutland@arm.com>
Cc: Will Deacon <will@kernel.org>
Cc: John Garry <john.garry@huawei.com>
Cc: Jonathan Cameron <Jonathan.Cameron@huawei.com>
Reviewed-by: John Garry <john.garry@huawei.com>
Co-developed-by: Qi Liu <liuqi115@huawei.com>
Signed-off-by: Qi Liu <liuqi115@huawei.com>
Signed-off-by: Shaokun Zhang <zhangshaokun@hisilicon.com>
Link: https://lore.kernel.org/r/1615186237-22263-9-git-send-email-zhangshaokun@hisilicon.com
Signed-off-by: Will Deacon <will@kernel.org>
Reviewed-by: Shaokun Zhang <zhangshaokun@hisilicon.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 drivers/perf/hisilicon/Makefile             |   3 +-
 drivers/perf/hisilicon/hisi_uncore_pa_pmu.c | 500 ++++++++++++++++++++
 include/linux/cpuhotplug.h                  |   1 +
 3 files changed, 503 insertions(+), 1 deletion(-)
 create mode 100644 drivers/perf/hisilicon/hisi_uncore_pa_pmu.c

diff --git a/drivers/perf/hisilicon/Makefile b/drivers/perf/hisilicon/Makefile
index 6600a9d45dd8..7643c9f93e36 100644
--- a/drivers/perf/hisilicon/Makefile
+++ b/drivers/perf/hisilicon/Makefile
@@ -1,3 +1,4 @@
 # SPDX-License-Identifier: GPL-2.0-only
 obj-$(CONFIG_HISI_PMU) += hisi_uncore_pmu.o hisi_uncore_l3c_pmu.o \
-			  hisi_uncore_hha_pmu.o hisi_uncore_ddrc_pmu.o hisi_uncore_sllc_pmu.o
+			  hisi_uncore_hha_pmu.o hisi_uncore_ddrc_pmu.o hisi_uncore_sllc_pmu.o \
+			  hisi_uncore_pa_pmu.o
diff --git a/drivers/perf/hisilicon/hisi_uncore_pa_pmu.c b/drivers/perf/hisilicon/hisi_uncore_pa_pmu.c
new file mode 100644
index 000000000000..5517a90552ec
--- /dev/null
+++ b/drivers/perf/hisilicon/hisi_uncore_pa_pmu.c
@@ -0,0 +1,500 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * HiSilicon PA uncore Hardware event counters support
+ *
+ * Copyright (C) 2020 HiSilicon Limited
+ * Author: Shaokun Zhang <zhangshaokun@hisilicon.com>
+ *
+ * This code is based on the uncore PMUs like arm-cci and arm-ccn.
+ */
+#include <linux/acpi.h>
+#include <linux/cpuhotplug.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+#include <linux/list.h>
+#include <linux/smp.h>
+
+#include "hisi_uncore_pmu.h"
+
+/* PA register definition */
+#define PA_PERF_CTRL			0x1c00
+#define PA_EVENT_CTRL			0x1c04
+#define PA_TT_CTRL			0x1c08
+#define PA_TGTID_CTRL			0x1c14
+#define PA_SRCID_CTRL			0x1c18
+#define PA_INT_MASK			0x1c70
+#define PA_INT_STATUS			0x1c78
+#define PA_INT_CLEAR			0x1c7c
+#define PA_EVENT_TYPE0			0x1c80
+#define PA_PMU_VERSION			0x1cf0
+#define PA_EVENT_CNT0_L			0x1d00
+
+#define PA_EVTYPE_MASK			0xff
+#define PA_NR_COUNTERS			0x8
+#define PA_PERF_CTRL_EN			BIT(0)
+#define PA_TRACETAG_EN			BIT(4)
+#define PA_TGTID_EN			BIT(11)
+#define PA_SRCID_EN			BIT(11)
+#define PA_TGTID_NONE			0
+#define PA_SRCID_NONE			0
+#define PA_TGTID_MSK_SHIFT		12
+#define PA_SRCID_MSK_SHIFT		12
+
+HISI_PMU_EVENT_ATTR_EXTRACTOR(tgtid_cmd, config1, 10, 0);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(tgtid_msk, config1, 21, 11);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(srcid_cmd, config1, 32, 22);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(srcid_msk, config1, 43, 33);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(tracetag_en, config1, 44, 44);
+
+static void hisi_pa_pmu_enable_tracetag(struct perf_event *event)
+{
+	struct hisi_pmu *pa_pmu = to_hisi_pmu(event->pmu);
+	u32 tt_en = hisi_get_tracetag_en(event);
+
+	if (tt_en) {
+		u32 val;
+
+		val = readl(pa_pmu->base + PA_TT_CTRL);
+		val |= PA_TRACETAG_EN;
+		writel(val, pa_pmu->base + PA_TT_CTRL);
+	}
+}
+
+static void hisi_pa_pmu_clear_tracetag(struct perf_event *event)
+{
+	struct hisi_pmu *pa_pmu = to_hisi_pmu(event->pmu);
+	u32 tt_en = hisi_get_tracetag_en(event);
+
+	if (tt_en) {
+		u32 val;
+
+		val = readl(pa_pmu->base + PA_TT_CTRL);
+		val &= ~PA_TRACETAG_EN;
+		writel(val, pa_pmu->base + PA_TT_CTRL);
+	}
+}
+
+static void hisi_pa_pmu_config_tgtid(struct perf_event *event)
+{
+	struct hisi_pmu *pa_pmu = to_hisi_pmu(event->pmu);
+	u32 cmd = hisi_get_tgtid_cmd(event);
+
+	if (cmd) {
+		u32 msk = hisi_get_tgtid_msk(event);
+		u32 val = cmd | PA_TGTID_EN | (msk << PA_TGTID_MSK_SHIFT);
+
+		writel(val, pa_pmu->base + PA_TGTID_CTRL);
+	}
+}
+
+static void hisi_pa_pmu_clear_tgtid(struct perf_event *event)
+{
+	struct hisi_pmu *pa_pmu = to_hisi_pmu(event->pmu);
+	u32 cmd = hisi_get_tgtid_cmd(event);
+
+	if (cmd)
+		writel(PA_TGTID_NONE, pa_pmu->base + PA_TGTID_CTRL);
+}
+
+static void hisi_pa_pmu_config_srcid(struct perf_event *event)
+{
+	struct hisi_pmu *pa_pmu = to_hisi_pmu(event->pmu);
+	u32 cmd = hisi_get_srcid_cmd(event);
+
+	if (cmd) {
+		u32 msk = hisi_get_srcid_msk(event);
+		u32 val = cmd | PA_SRCID_EN | (msk << PA_SRCID_MSK_SHIFT);
+
+		writel(val, pa_pmu->base + PA_SRCID_CTRL);
+	}
+}
+
+static void hisi_pa_pmu_clear_srcid(struct perf_event *event)
+{
+	struct hisi_pmu *pa_pmu = to_hisi_pmu(event->pmu);
+	u32 cmd = hisi_get_srcid_cmd(event);
+
+	if (cmd)
+		writel(PA_SRCID_NONE, pa_pmu->base + PA_SRCID_CTRL);
+}
+
+static void hisi_pa_pmu_enable_filter(struct perf_event *event)
+{
+	if (event->attr.config1 != 0x0) {
+		hisi_pa_pmu_enable_tracetag(event);
+		hisi_pa_pmu_config_srcid(event);
+		hisi_pa_pmu_config_tgtid(event);
+	}
+}
+
+static void hisi_pa_pmu_disable_filter(struct perf_event *event)
+{
+	if (event->attr.config1 != 0x0) {
+		hisi_pa_pmu_clear_tgtid(event);
+		hisi_pa_pmu_clear_srcid(event);
+		hisi_pa_pmu_clear_tracetag(event);
+	}
+}
+
+static u32 hisi_pa_pmu_get_counter_offset(int idx)
+{
+	return (PA_EVENT_CNT0_L + idx * 8);
+}
+
+static u64 hisi_pa_pmu_read_counter(struct hisi_pmu *pa_pmu,
+				    struct hw_perf_event *hwc)
+{
+	return readq(pa_pmu->base + hisi_pa_pmu_get_counter_offset(hwc->idx));
+}
+
+static void hisi_pa_pmu_write_counter(struct hisi_pmu *pa_pmu,
+				      struct hw_perf_event *hwc, u64 val)
+{
+	writeq(val, pa_pmu->base + hisi_pa_pmu_get_counter_offset(hwc->idx));
+}
+
+static void hisi_pa_pmu_write_evtype(struct hisi_pmu *pa_pmu, int idx,
+				     u32 type)
+{
+	u32 reg, reg_idx, shift, val;
+
+	/*
+	 * Select the appropriate event select register(PA_EVENT_TYPE0/1).
+	 * There are 2 event select registers for the 8 hardware counters.
+	 * Event code is 8-bits and for the former 4 hardware counters,
+	 * PA_EVENT_TYPE0 is chosen. For the latter 4 hardware counters,
+	 * PA_EVENT_TYPE1 is chosen.
+	 */
+	reg = PA_EVENT_TYPE0 + (idx / 4) * 4;
+	reg_idx = idx % 4;
+	shift = 8 * reg_idx;
+
+	/* Write event code to pa_EVENT_TYPEx Register */
+	val = readl(pa_pmu->base + reg);
+	val &= ~(PA_EVTYPE_MASK << shift);
+	val |= (type << shift);
+	writel(val, pa_pmu->base + reg);
+}
+
+static void hisi_pa_pmu_start_counters(struct hisi_pmu *pa_pmu)
+{
+	u32 val;
+
+	val = readl(pa_pmu->base + PA_PERF_CTRL);
+	val |= PA_PERF_CTRL_EN;
+	writel(val, pa_pmu->base + PA_PERF_CTRL);
+}
+
+static void hisi_pa_pmu_stop_counters(struct hisi_pmu *pa_pmu)
+{
+	u32 val;
+
+	val = readl(pa_pmu->base + PA_PERF_CTRL);
+	val &= ~(PA_PERF_CTRL_EN);
+	writel(val, pa_pmu->base + PA_PERF_CTRL);
+}
+
+static void hisi_pa_pmu_enable_counter(struct hisi_pmu *pa_pmu,
+				       struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Enable counter index in PA_EVENT_CTRL register */
+	val = readl(pa_pmu->base + PA_EVENT_CTRL);
+	val |= 1 << hwc->idx;
+	writel(val, pa_pmu->base + PA_EVENT_CTRL);
+}
+
+static void hisi_pa_pmu_disable_counter(struct hisi_pmu *pa_pmu,
+					struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Clear counter index in PA_EVENT_CTRL register */
+	val = readl(pa_pmu->base + PA_EVENT_CTRL);
+	val &= ~(1 << hwc->idx);
+	writel(val, pa_pmu->base + PA_EVENT_CTRL);
+}
+
+static void hisi_pa_pmu_enable_counter_int(struct hisi_pmu *pa_pmu,
+					   struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Write 0 to enable interrupt */
+	val = readl(pa_pmu->base + PA_INT_MASK);
+	val &= ~(1 << hwc->idx);
+	writel(val, pa_pmu->base + PA_INT_MASK);
+}
+
+static void hisi_pa_pmu_disable_counter_int(struct hisi_pmu *pa_pmu,
+					    struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Write 1 to mask interrupt */
+	val = readl(pa_pmu->base + PA_INT_MASK);
+	val |= 1 << hwc->idx;
+	writel(val, pa_pmu->base + PA_INT_MASK);
+}
+
+static u32 hisi_pa_pmu_get_int_status(struct hisi_pmu *pa_pmu)
+{
+	return readl(pa_pmu->base + PA_INT_STATUS);
+}
+
+static void hisi_pa_pmu_clear_int_status(struct hisi_pmu *pa_pmu, int idx)
+{
+	writel(1 << idx, pa_pmu->base + PA_INT_CLEAR);
+}
+
+static const struct acpi_device_id hisi_pa_pmu_acpi_match[] = {
+	{ "HISI0273", },
+	{}
+};
+MODULE_DEVICE_TABLE(acpi, hisi_pa_pmu_acpi_match);
+
+static int hisi_pa_pmu_init_data(struct platform_device *pdev,
+				   struct hisi_pmu *pa_pmu)
+{
+	/*
+	 * Use the SCCL_ID and the index ID to identify the PA PMU,
+	 * while SCCL_ID is the nearst SCCL_ID from this SICL and
+	 * CPU core is chosen from this SCCL to manage this PMU.
+	 */
+	if (device_property_read_u32(&pdev->dev, "hisilicon,scl-id",
+				     &pa_pmu->sccl_id)) {
+		dev_err(&pdev->dev, "Cannot read sccl-id!\n");
+		return -EINVAL;
+	}
+
+	if (device_property_read_u32(&pdev->dev, "hisilicon,idx-id",
+				     &pa_pmu->index_id)) {
+		dev_err(&pdev->dev, "Cannot read idx-id!\n");
+		return -EINVAL;
+	}
+
+	pa_pmu->ccl_id = -1;
+
+	pa_pmu->base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(pa_pmu->base)) {
+		dev_err(&pdev->dev, "ioremap failed for pa_pmu resource.\n");
+		return PTR_ERR(pa_pmu->base);
+	}
+
+	pa_pmu->identifier = readl(pa_pmu->base + PA_PMU_VERSION);
+
+	return 0;
+}
+
+static struct attribute *hisi_pa_pmu_v2_format_attr[] = {
+	HISI_PMU_FORMAT_ATTR(event, "config:0-7"),
+	HISI_PMU_FORMAT_ATTR(tgtid_cmd, "config1:0-10"),
+	HISI_PMU_FORMAT_ATTR(tgtid_msk, "config1:11-21"),
+	HISI_PMU_FORMAT_ATTR(srcid_cmd, "config1:22-32"),
+	HISI_PMU_FORMAT_ATTR(srcid_msk, "config1:33-43"),
+	HISI_PMU_FORMAT_ATTR(tracetag_en, "config1:44"),
+	NULL,
+};
+
+static const struct attribute_group hisi_pa_pmu_v2_format_group = {
+	.name = "format",
+	.attrs = hisi_pa_pmu_v2_format_attr,
+};
+
+static struct attribute *hisi_pa_pmu_v2_events_attr[] = {
+	HISI_PMU_EVENT_ATTR(rx_req,		0x40),
+	HISI_PMU_EVENT_ATTR(tx_req,             0x5c),
+	HISI_PMU_EVENT_ATTR(cycle,		0x78),
+	NULL
+};
+
+static const struct attribute_group hisi_pa_pmu_v2_events_group = {
+	.name = "events",
+	.attrs = hisi_pa_pmu_v2_events_attr,
+};
+
+static DEVICE_ATTR(cpumask, 0444, hisi_cpumask_sysfs_show, NULL);
+
+static struct attribute *hisi_pa_pmu_cpumask_attrs[] = {
+	&dev_attr_cpumask.attr,
+	NULL
+};
+
+static const struct attribute_group hisi_pa_pmu_cpumask_attr_group = {
+	.attrs = hisi_pa_pmu_cpumask_attrs,
+};
+
+static struct device_attribute hisi_pa_pmu_identifier_attr =
+	__ATTR(identifier, 0444, hisi_uncore_pmu_identifier_attr_show, NULL);
+
+static struct attribute *hisi_pa_pmu_identifier_attrs[] = {
+	&hisi_pa_pmu_identifier_attr.attr,
+	NULL
+};
+
+static struct attribute_group hisi_pa_pmu_identifier_group = {
+	.attrs = hisi_pa_pmu_identifier_attrs,
+};
+
+static const struct attribute_group *hisi_pa_pmu_v2_attr_groups[] = {
+	&hisi_pa_pmu_v2_format_group,
+	&hisi_pa_pmu_v2_events_group,
+	&hisi_pa_pmu_cpumask_attr_group,
+	&hisi_pa_pmu_identifier_group,
+	NULL
+};
+
+static const struct hisi_uncore_ops hisi_uncore_pa_ops = {
+	.write_evtype		= hisi_pa_pmu_write_evtype,
+	.get_event_idx		= hisi_uncore_pmu_get_event_idx,
+	.start_counters		= hisi_pa_pmu_start_counters,
+	.stop_counters		= hisi_pa_pmu_stop_counters,
+	.enable_counter		= hisi_pa_pmu_enable_counter,
+	.disable_counter	= hisi_pa_pmu_disable_counter,
+	.enable_counter_int	= hisi_pa_pmu_enable_counter_int,
+	.disable_counter_int	= hisi_pa_pmu_disable_counter_int,
+	.write_counter		= hisi_pa_pmu_write_counter,
+	.read_counter		= hisi_pa_pmu_read_counter,
+	.get_int_status		= hisi_pa_pmu_get_int_status,
+	.clear_int_status	= hisi_pa_pmu_clear_int_status,
+	.enable_filter		= hisi_pa_pmu_enable_filter,
+	.disable_filter		= hisi_pa_pmu_disable_filter,
+};
+
+static int hisi_pa_pmu_dev_probe(struct platform_device *pdev,
+				 struct hisi_pmu *pa_pmu)
+{
+	int ret;
+
+	ret = hisi_pa_pmu_init_data(pdev, pa_pmu);
+	if (ret)
+		return ret;
+
+	ret = hisi_uncore_pmu_init_irq(pa_pmu, pdev);
+	if (ret)
+		return ret;
+
+	pa_pmu->pmu_events.attr_groups = hisi_pa_pmu_v2_attr_groups;
+	pa_pmu->num_counters = PA_NR_COUNTERS;
+	pa_pmu->ops = &hisi_uncore_pa_ops;
+	pa_pmu->check_event = 0xB0;
+	pa_pmu->counter_bits = 64;
+	pa_pmu->dev = &pdev->dev;
+	pa_pmu->on_cpu = -1;
+
+	return 0;
+}
+
+static int hisi_pa_pmu_probe(struct platform_device *pdev)
+{
+	struct hisi_pmu *pa_pmu;
+	char *name;
+	int ret;
+
+	pa_pmu = devm_kzalloc(&pdev->dev, sizeof(*pa_pmu), GFP_KERNEL);
+	if (!pa_pmu)
+		return -ENOMEM;
+
+	ret = hisi_pa_pmu_dev_probe(pdev, pa_pmu);
+	if (ret)
+		return ret;
+	/*
+	 * PA is attached in SICL and the CPU core is chosen to manage this
+	 * PMU which is the nearest SCCL, while its SCCL_ID is greater than
+	 * one with the SICL_ID.
+	 */
+	name = devm_kasprintf(&pdev->dev, GFP_KERNEL, "hisi_sicl%u_pa%u",
+			      pa_pmu->sccl_id - 1, pa_pmu->index_id);
+	if (!name)
+		return -ENOMEM;
+
+	ret = cpuhp_state_add_instance(CPUHP_AP_PERF_ARM_HISI_PA_ONLINE,
+				       &pa_pmu->node);
+	if (ret) {
+		dev_err(&pdev->dev, "Error %d registering hotplug\n", ret);
+		return ret;
+	}
+
+	pa_pmu->pmu = (struct pmu) {
+		.module		= THIS_MODULE,
+		.task_ctx_nr	= perf_invalid_context,
+		.event_init	= hisi_uncore_pmu_event_init,
+		.pmu_enable	= hisi_uncore_pmu_enable,
+		.pmu_disable	= hisi_uncore_pmu_disable,
+		.add		= hisi_uncore_pmu_add,
+		.del		= hisi_uncore_pmu_del,
+		.start		= hisi_uncore_pmu_start,
+		.stop		= hisi_uncore_pmu_stop,
+		.read		= hisi_uncore_pmu_read,
+		.attr_groups    = pa_pmu->pmu_events.attr_groups,
+		.capabilities	= PERF_PMU_CAP_NO_EXCLUDE,
+	};
+
+	ret = perf_pmu_register(&pa_pmu->pmu, name, -1);
+	if (ret) {
+		dev_err(pa_pmu->dev, "PMU register failed, ret = %d\n", ret);
+		cpuhp_state_remove_instance(CPUHP_AP_PERF_ARM_HISI_PA_ONLINE,
+					    &pa_pmu->node);
+		irq_set_affinity_hint(pa_pmu->irq, NULL);
+		return ret;
+	}
+
+	platform_set_drvdata(pdev, pa_pmu);
+	return ret;
+}
+
+static int hisi_pa_pmu_remove(struct platform_device *pdev)
+{
+	struct hisi_pmu *pa_pmu = platform_get_drvdata(pdev);
+
+	perf_pmu_unregister(&pa_pmu->pmu);
+	cpuhp_state_remove_instance_nocalls(CPUHP_AP_PERF_ARM_HISI_PA_ONLINE,
+					    &pa_pmu->node);
+	irq_set_affinity_hint(pa_pmu->irq, NULL);
+
+	return 0;
+}
+
+static struct platform_driver hisi_pa_pmu_driver = {
+	.driver = {
+		.name = "hisi_pa_pmu",
+		.acpi_match_table = hisi_pa_pmu_acpi_match,
+		.suppress_bind_attrs = true,
+	},
+	.probe = hisi_pa_pmu_probe,
+	.remove = hisi_pa_pmu_remove,
+};
+
+static int __init hisi_pa_pmu_module_init(void)
+{
+	int ret;
+
+	ret = cpuhp_setup_state_multi(CPUHP_AP_PERF_ARM_HISI_PA_ONLINE,
+				      "AP_PERF_ARM_HISI_PA_ONLINE",
+				      hisi_uncore_pmu_online_cpu,
+				      hisi_uncore_pmu_offline_cpu);
+	if (ret) {
+		pr_err("PA PMU: cpuhp state setup failed, ret = %d\n", ret);
+		return ret;
+	}
+
+	ret = platform_driver_register(&hisi_pa_pmu_driver);
+	if (ret)
+		cpuhp_remove_multi_state(CPUHP_AP_PERF_ARM_HISI_PA_ONLINE);
+
+	return ret;
+}
+module_init(hisi_pa_pmu_module_init);
+
+static void __exit hisi_pa_pmu_module_exit(void)
+{
+	platform_driver_unregister(&hisi_pa_pmu_driver);
+	cpuhp_remove_multi_state(CPUHP_AP_PERF_ARM_HISI_PA_ONLINE);
+}
+module_exit(hisi_pa_pmu_module_exit);
+
+MODULE_DESCRIPTION("HiSilicon Protocol Adapter uncore PMU driver");
+MODULE_LICENSE("GPL v2");
+MODULE_AUTHOR("Shaokun Zhang <zhangshaokun@hisilicon.com>");
+MODULE_AUTHOR("Qi Liu <liuqi115@huawei.com>");
diff --git a/include/linux/cpuhotplug.h b/include/linux/cpuhotplug.h
index b5c55a408a30..225b095a96db 100644
--- a/include/linux/cpuhotplug.h
+++ b/include/linux/cpuhotplug.h
@@ -161,6 +161,7 @@ enum cpuhp_state {
 	CPUHP_AP_PERF_ARM_HISI_DDRC_ONLINE,
 	CPUHP_AP_PERF_ARM_HISI_HHA_ONLINE,
 	CPUHP_AP_PERF_ARM_HISI_L3_ONLINE,
+	CPUHP_AP_PERF_ARM_HISI_PA_ONLINE,
 	CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE,
 	CPUHP_AP_PERF_ARM_L2X0_ONLINE,
 	CPUHP_AP_PERF_ARM_QCOM_L2_ONLINE,
-- 
2.27.0

