From 5428287200dbce2d9e5dbd50e4f32c5cf81a953f Mon Sep 17 00:00:00 2001
From: Leo Yan <leo.yan@linaro.org>
Date: Fri, 31 Dec 2021 13:32:13 +0800
Subject: [PATCH 16/21] perf arm-spe: Add new function
 arm_spe_pkt_desc_op_type()

mainline inclusion
from mainline-v5.11-rc1
commit 7488ffc4d981e19feddfe36a619051bf6216c7a1
category: feature
bugzilla: https://gitee.com/openeuler/kernel/issues/I4NGPV
CVE: NA

-------------------------------------------------

The operation type packet is complex and contains subclass; the parsing
flow causes deep indentation; for more readable, this patch introduces
a new function arm_spe_pkt_desc_op_type() which is used for operation
type parsing.

Signed-off-by: Leo Yan <leo.yan@linaro.org>
Reviewed-by: Andre Przywara <andre.przywara@arm.com>
Acked-by: Will Deacon <will@kernel.org>
Cc: Alexander Shishkin <alexander.shishkin@linux.intel.com>
Cc: Al Grant <Al.Grant@arm.com>
Cc: Arnaldo Carvalho de Melo <acme@kernel.org>
Cc: Dave Martin <Dave.Martin@arm.com>
Cc: Ingo Molnar <mingo@redhat.com>
Cc: James Clark <james.clark@arm.com>
Cc: Jiri Olsa <jolsa@redhat.com>
Cc: John Garry <john.garry@huawei.com>
Cc: Mark Rutland <mark.rutland@arm.com>
Cc: Mathieu Poirier <mathieu.poirier@linaro.org>
Cc: Namhyung Kim <namhyung@kernel.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Wei Li <liwei391@huawei.com>
Link: https://lore.kernel.org/r/20201119152441.6972-13-leo.yan@linaro.org
Signed-off-by: Arnaldo Carvalho de Melo <acme@redhat.com>
Signed-off-by: Wei Li <liwei391@huawei.com>
Reviewed-by: Yang Jihong <yangjihong1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 .../arm-spe-decoder/arm-spe-pkt-decoder.c     | 79 +++++++++++--------
 1 file changed, 45 insertions(+), 34 deletions(-)

diff --git a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
index 88bcf7e5be76..d6c060f119b4 100644
--- a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
+++ b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
@@ -321,6 +321,50 @@ static int arm_spe_pkt_desc_event(const struct arm_spe_pkt *packet,
 	return err;
 }
 
+static int arm_spe_pkt_desc_op_type(const struct arm_spe_pkt *packet,
+				    char *buf, size_t buf_len)
+{
+	u64 payload = packet->payload;
+	int err = 0;
+
+	switch (packet->index) {
+	case 0:
+		arm_spe_pkt_out_string(&err, &buf, &buf_len,
+				payload & 0x1 ? "COND-SELECT" : "INSN-OTHER");
+		break;
+	case 1:
+		arm_spe_pkt_out_string(&err, &buf, &buf_len,
+				       payload & 0x1 ? "ST" : "LD");
+
+		if (payload & 0x2) {
+			if (payload & 0x4)
+				arm_spe_pkt_out_string(&err, &buf, &buf_len, " AT");
+			if (payload & 0x8)
+				arm_spe_pkt_out_string(&err, &buf, &buf_len, " EXCL");
+			if (payload & 0x10)
+				arm_spe_pkt_out_string(&err, &buf, &buf_len, " AR");
+		} else if (payload & 0x4) {
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " SIMD-FP");
+		}
+		break;
+	case 2:
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, "B");
+
+		if (payload & 0x1)
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " COND");
+		if (payload & 0x2)
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " IND");
+
+		break;
+	default:
+		/* Unknown index */
+		err = -1;
+		break;
+	}
+
+	return err;
+}
+
 static int arm_spe_pkt_desc_addr(const struct arm_spe_pkt *packet,
 				 char *buf, size_t buf_len)
 {
@@ -404,40 +448,7 @@ int arm_spe_pkt_desc(const struct arm_spe_pkt *packet, char *buf,
 		err = arm_spe_pkt_desc_event(packet, buf, buf_len);
 		break;
 	case ARM_SPE_OP_TYPE:
-		switch (idx) {
-		case 0:
-			arm_spe_pkt_out_string(&err, &buf, &blen,
-					payload & 0x1 ? "COND-SELECT" : "INSN-OTHER");
-			break;
-		case 1:
-			arm_spe_pkt_out_string(&err, &buf, &blen,
-					       payload & 0x1 ? "ST" : "LD");
-
-			if (payload & 0x2) {
-				if (payload & 0x4)
-					arm_spe_pkt_out_string(&err, &buf, &blen, " AT");
-				if (payload & 0x8)
-					arm_spe_pkt_out_string(&err, &buf, &blen, " EXCL");
-				if (payload & 0x10)
-					arm_spe_pkt_out_string(&err, &buf, &blen, " AR");
-			} else if (payload & 0x4) {
-				arm_spe_pkt_out_string(&err, &buf, &blen, " SIMD-FP");
-			}
-			break;
-		case 2:
-			arm_spe_pkt_out_string(&err, &buf, &blen, "B");
-
-			if (payload & 0x1)
-				arm_spe_pkt_out_string(&err, &buf, &blen, " COND");
-			if (payload & 0x2)
-				arm_spe_pkt_out_string(&err, &buf, &blen, " IND");
-
-			break;
-		default:
-			/* Unknown index */
-			err = -1;
-			break;
-		}
+		err = arm_spe_pkt_desc_op_type(packet, buf, buf_len);
 		break;
 	case ARM_SPE_DATA_SOURCE:
 	case ARM_SPE_TIMESTAMP:
-- 
2.27.0

