From 7df3c74b37355c06afee870ace0a8eb1491130dc Mon Sep 17 00:00:00 2001
From: Jay Fang <f.fangjian@huawei.com>
Date: Mon, 9 Aug 2021 20:18:16 +0800
Subject: [PATCH 106/109] spi: Add HiSilicon SPI Controller Driver for Kunpeng
 SoCs

mainline inclusion
from mainline-v5.13-rc1
commit c770d8631e1810d8f1ce21b18ad5dd67eeb39e5c
category: feature
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8DDF5
Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=c770d8631e1810d8f1ce21b18ad5dd67eeb39e5c

----------------------------------------------------------------------

This driver supports SPI Controller for HiSilicon Kunpeng SoCs. This
driver supports SPI operations using FIFO mode of transfer.

DMA is not supported, and we just use IRQ mode for operation completion
notification.

Only ACPI firmware is supported.

Signed-off-by: Jay Fang <f.fangjian@huawei.com>
Link: https://lore.kernel.org/r/1616836200-45827-1-git-send-email-f.fangjian@huawei.com
Signed-off-by: Mark Brown <broonie@kernel.org>
Reviewed-by: Chengwen Feng <fengchengwen@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: YunYi Yang <yangyunyi2@huawei.com>

 Conflicts:
	MAINTAINERS
	drivers/spi/Kconfig
	drivers/spi/Makefile
---
 MAINTAINERS                    |   7 +
 drivers/spi/Kconfig            |  10 +
 drivers/spi/Makefile           |   1 +
 drivers/spi/spi-hisi-kunpeng.c | 504 +++++++++++++++++++++++++++++++++
 4 files changed, 522 insertions(+)
 create mode 100644 drivers/spi/spi-hisi-kunpeng.c

diff --git a/MAINTAINERS b/MAINTAINERS
index 3ad1e1b1da4a..29d7531d0595 100644
--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -6679,6 +6679,13 @@ S:	Maintained
 F:	drivers/infiniband/hw/hns/Makefile
 F:	drivers/infiniband/hw/hns/roce-customer/
 
+HISILICON SPI Controller DRIVER FOR KUNPENG SOCS
+M:	Jay Fang <f.fangjian@huawei.com>
+L:	linux-spi@vger.kernel.org
+S:	Maintained
+W:	http://www.hisilicon.com
+F:	drivers/spi/spi-hisi-kunpeng.c
+
 HISILICON WARPDRIVE USER
 M:	Zaibo Xu <xuzaibo@huawei.com>
 M:	Zhou Wang <wangzhou1@hisilicon.com>
diff --git a/drivers/spi/Kconfig b/drivers/spi/Kconfig
index 0a7fd56c1ed9..7bfdf8d2cbf9 100644
--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -251,6 +251,16 @@ config SPI_FSL_LPSPI
 	help
 	  This enables Freescale i.MX LPSPI controllers in master mode.
 
+config SPI_HISI_KUNPENG
+	tristate "HiSilicon SPI Controller for Kunpeng SoCs"
+	depends on (ARM64 && ACPI) || COMPILE_TEST
+	help
+	  This enables support for HiSilicon SPI controller found on
+	  Kunpeng SoCs.
+
+	  This driver can also be built as a module. If so, the module
+	  will be called hisi-kunpeng-spi.
+
 config SPI_GPIO
 	tristate "GPIO-based bitbanging SPI Master"
 	depends on GPIOLIB || COMPILE_TEST
diff --git a/drivers/spi/Makefile b/drivers/spi/Makefile
index a90d55970036..49c499d5e1a2 100644
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -45,6 +45,7 @@ obj-$(CONFIG_SPI_FSL_ESPI)		+= spi-fsl-espi.o
 obj-$(CONFIG_SPI_FSL_LPSPI)		+= spi-fsl-lpspi.o
 obj-$(CONFIG_SPI_FSL_SPI)		+= spi-fsl-spi.o
 obj-$(CONFIG_SPI_GPIO)			+= spi-gpio.o
+obj-$(CONFIG_SPI_HISI_KUNPENG)		+= spi-hisi-kunpeng.o
 obj-$(CONFIG_SPI_IMG_SPFI)		+= spi-img-spfi.o
 obj-$(CONFIG_SPI_IMX)			+= spi-imx.o
 obj-$(CONFIG_SPI_LANTIQ_SSC)		+= spi-lantiq-ssc.o
diff --git a/drivers/spi/spi-hisi-kunpeng.c b/drivers/spi/spi-hisi-kunpeng.c
new file mode 100644
index 000000000000..ea87b4fba5d6
--- /dev/null
+++ b/drivers/spi/spi-hisi-kunpeng.c
@@ -0,0 +1,504 @@
+// SPDX-License-Identifier: GPL-2.0-only
+//
+// HiSilicon SPI Controller Driver for Kunpeng SoCs
+//
+// Copyright (c) 2021 HiSilicon Technologies Co., Ltd.
+// Author: Jay Fang <f.fangjian@huawei.com>
+//
+// This code is based on spi-dw-core.c.
+
+#include <linux/acpi.h>
+#include <linux/bitfield.h>
+#include <linux/delay.h>
+#include <linux/err.h>
+#include <linux/interrupt.h>
+#include <linux/module.h>
+#include <linux/property.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/spi/spi.h>
+
+/* Register offsets */
+#define HISI_SPI_CSCR		0x00	/* cs control register */
+#define HISI_SPI_CR		0x04	/* spi common control register */
+#define HISI_SPI_ENR		0x08	/* spi enable register */
+#define HISI_SPI_FIFOC		0x0c	/* fifo level control register */
+#define HISI_SPI_IMR		0x10	/* interrupt mask register */
+#define HISI_SPI_DIN		0x14	/* data in register */
+#define HISI_SPI_DOUT		0x18	/* data out register */
+#define HISI_SPI_SR		0x1c	/* status register */
+#define HISI_SPI_RISR		0x20	/* raw interrupt status register */
+#define HISI_SPI_ISR		0x24	/* interrupt status register */
+#define HISI_SPI_ICR		0x28	/* interrupt clear register */
+#define HISI_SPI_VERSION	0xe0	/* version register */
+
+/* Bit fields in HISI_SPI_CR */
+#define CR_LOOP_MASK		GENMASK(1, 1)
+#define CR_CPOL_MASK		GENMASK(2, 2)
+#define CR_CPHA_MASK		GENMASK(3, 3)
+#define CR_DIV_PRE_MASK		GENMASK(11, 4)
+#define CR_DIV_POST_MASK	GENMASK(19, 12)
+#define CR_BPW_MASK		GENMASK(24, 20)
+#define CR_SPD_MODE_MASK	GENMASK(25, 25)
+
+/* Bit fields in HISI_SPI_FIFOC */
+#define FIFOC_TX_MASK		GENMASK(5, 3)
+#define FIFOC_RX_MASK		GENMASK(11, 9)
+
+/* Bit fields in HISI_SPI_IMR, 4 bits */
+#define IMR_RXOF		BIT(0)		/* Receive Overflow */
+#define IMR_RXTO		BIT(1)		/* Receive Timeout */
+#define IMR_RX			BIT(2)		/* Receive */
+#define IMR_TX			BIT(3)		/* Transmit */
+#define IMR_MASK		(IMR_RXOF | IMR_RXTO | IMR_RX | IMR_TX)
+
+/* Bit fields in HISI_SPI_SR, 5 bits */
+#define SR_TXE			BIT(0)		/* Transmit FIFO empty */
+#define SR_TXNF			BIT(1)		/* Transmit FIFO not full */
+#define SR_RXNE			BIT(2)		/* Receive FIFO not empty */
+#define SR_RXF			BIT(3)		/* Receive FIFO full */
+#define SR_BUSY			BIT(4)		/* Busy Flag */
+
+/* Bit fields in HISI_SPI_ISR, 4 bits */
+#define ISR_RXOF		BIT(0)		/* Receive Overflow */
+#define ISR_RXTO		BIT(1)		/* Receive Timeout */
+#define ISR_RX			BIT(2)		/* Receive */
+#define ISR_TX			BIT(3)		/* Transmit */
+#define ISR_MASK		(ISR_RXOF | ISR_RXTO | ISR_RX | ISR_TX)
+
+/* Bit fields in HISI_SPI_ICR, 2 bits */
+#define ICR_RXOF		BIT(0)		/* Receive Overflow */
+#define ICR_RXTO		BIT(1)		/* Receive Timeout */
+#define ICR_MASK		(ICR_RXOF | ICR_RXTO)
+
+#define DIV_POST_MAX		0xFF
+#define DIV_POST_MIN		0x00
+#define DIV_PRE_MAX		0xFE
+#define DIV_PRE_MIN		0x02
+#define CLK_DIV_MAX		((1 + DIV_POST_MAX) * DIV_PRE_MAX)
+#define CLK_DIV_MIN		((1 + DIV_POST_MIN) * DIV_PRE_MIN)
+
+#define DEFAULT_NUM_CS		1
+
+#define HISI_SPI_WAIT_TIMEOUT_MS	10UL
+
+enum hisi_spi_rx_level_trig {
+	HISI_SPI_RX_1,
+	HISI_SPI_RX_4,
+	HISI_SPI_RX_8,
+	HISI_SPI_RX_16,
+	HISI_SPI_RX_32,
+	HISI_SPI_RX_64,
+	HISI_SPI_RX_128
+};
+
+enum hisi_spi_tx_level_trig {
+	HISI_SPI_TX_1_OR_LESS,
+	HISI_SPI_TX_4_OR_LESS,
+	HISI_SPI_TX_8_OR_LESS,
+	HISI_SPI_TX_16_OR_LESS,
+	HISI_SPI_TX_32_OR_LESS,
+	HISI_SPI_TX_64_OR_LESS,
+	HISI_SPI_TX_128_OR_LESS
+};
+
+enum hisi_spi_frame_n_bytes {
+	HISI_SPI_N_BYTES_NULL,
+	HISI_SPI_N_BYTES_U8,
+	HISI_SPI_N_BYTES_U16,
+	HISI_SPI_N_BYTES_U32 = 4
+};
+
+/* Slave spi_dev related */
+struct hisi_chip_data {
+	u32 cr;
+	u32 speed_hz;	/* baud rate */
+	u16 clk_div;	/* baud rate divider */
+
+	/* clk_div = (1 + div_post) * div_pre */
+	u8 div_post;	/* value from 0 to 255 */
+	u8 div_pre;	/* value from 2 to 254 (even only!) */
+};
+
+struct hisi_spi {
+	struct device		*dev;
+
+	void __iomem		*regs;
+	int			irq;
+	u32			fifo_len; /* depth of the FIFO buffer */
+
+	/* Current message transfer state info */
+	const void		*tx;
+	unsigned int		tx_len;
+	void			*rx;
+	unsigned int		rx_len;
+	u8			n_bytes; /* current is a 1/2/4 bytes op */
+};
+
+static u32 hisi_spi_busy(struct hisi_spi *hs)
+{
+	return readl(hs->regs + HISI_SPI_SR) & SR_BUSY;
+}
+
+static u32 hisi_spi_rx_not_empty(struct hisi_spi *hs)
+{
+	return readl(hs->regs + HISI_SPI_SR) & SR_RXNE;
+}
+
+static u32 hisi_spi_tx_not_full(struct hisi_spi *hs)
+{
+	return readl(hs->regs + HISI_SPI_SR) & SR_TXNF;
+}
+
+static void hisi_spi_flush_fifo(struct hisi_spi *hs)
+{
+	unsigned long limit = loops_per_jiffy << 1;
+
+	do {
+		while (hisi_spi_rx_not_empty(hs))
+			readl(hs->regs + HISI_SPI_DOUT);
+	} while (hisi_spi_busy(hs) && limit--);
+}
+
+/* Disable the controller and all interrupts */
+static void hisi_spi_disable(struct hisi_spi *hs)
+{
+	writel(0, hs->regs + HISI_SPI_ENR);
+	writel(IMR_MASK, hs->regs + HISI_SPI_IMR);
+	writel(ICR_MASK, hs->regs + HISI_SPI_ICR);
+}
+
+static u8 hisi_spi_n_bytes(struct spi_transfer *transfer)
+{
+	if (transfer->bits_per_word <= 8)
+		return HISI_SPI_N_BYTES_U8;
+	else if (transfer->bits_per_word <= 16)
+		return HISI_SPI_N_BYTES_U16;
+	else
+		return HISI_SPI_N_BYTES_U32;
+}
+
+static void hisi_spi_reader(struct hisi_spi *hs)
+{
+	u32 max = min_t(u32, hs->rx_len, hs->fifo_len);
+	u32 rxw;
+
+	while (hisi_spi_rx_not_empty(hs) && max--) {
+		rxw = readl(hs->regs + HISI_SPI_DOUT);
+		/* Check the transfer's original "rx" is not null */
+		if (hs->rx) {
+			switch (hs->n_bytes) {
+			case HISI_SPI_N_BYTES_U8:
+				*(u8 *)(hs->rx) = rxw;
+				break;
+			case HISI_SPI_N_BYTES_U16:
+				*(u16 *)(hs->rx) = rxw;
+				break;
+			case HISI_SPI_N_BYTES_U32:
+				*(u32 *)(hs->rx) = rxw;
+				break;
+			}
+			hs->rx += hs->n_bytes;
+		}
+		--hs->rx_len;
+	}
+}
+
+static void hisi_spi_writer(struct hisi_spi *hs)
+{
+	u32 max = min_t(u32, hs->tx_len, hs->fifo_len);
+	u32 txw = 0;
+
+	while (hisi_spi_tx_not_full(hs) && max--) {
+		/* Check the transfer's original "tx" is not null */
+		if (hs->tx) {
+			switch (hs->n_bytes) {
+			case HISI_SPI_N_BYTES_U8:
+				txw = *(u8 *)(hs->tx);
+				break;
+			case HISI_SPI_N_BYTES_U16:
+				txw = *(u16 *)(hs->tx);
+				break;
+			case HISI_SPI_N_BYTES_U32:
+				txw = *(u32 *)(hs->tx);
+				break;
+			}
+			hs->tx += hs->n_bytes;
+		}
+		writel(txw, hs->regs + HISI_SPI_DIN);
+		--hs->tx_len;
+	}
+}
+
+static void __hisi_calc_div_reg(struct hisi_chip_data *chip)
+{
+	chip->div_pre = DIV_PRE_MAX;
+	while (chip->div_pre >= DIV_PRE_MIN) {
+		if (chip->clk_div % chip->div_pre == 0)
+			break;
+
+		chip->div_pre -= 2;
+	}
+
+	if (chip->div_pre > chip->clk_div)
+		chip->div_pre = chip->clk_div;
+
+	chip->div_post = (chip->clk_div / chip->div_pre) - 1;
+}
+
+static u32 hisi_calc_effective_speed(struct spi_controller *master,
+			struct hisi_chip_data *chip, u32 speed_hz)
+{
+	u32 effective_speed;
+
+	/* Note clock divider doesn't support odd numbers */
+	chip->clk_div = DIV_ROUND_UP(master->max_speed_hz, speed_hz) + 1;
+	chip->clk_div &= 0xfffe;
+	if (chip->clk_div > CLK_DIV_MAX)
+		chip->clk_div = CLK_DIV_MAX;
+
+	effective_speed = master->max_speed_hz / chip->clk_div;
+	if (chip->speed_hz != effective_speed) {
+		__hisi_calc_div_reg(chip);
+		chip->speed_hz = effective_speed;
+	}
+
+	return effective_speed;
+}
+
+static u32 hisi_spi_prepare_cr(struct spi_device *spi)
+{
+	u32 cr = FIELD_PREP(CR_SPD_MODE_MASK, 1);
+
+	cr |= FIELD_PREP(CR_CPHA_MASK, (spi->mode & SPI_CPHA) ? 1 : 0);
+	cr |= FIELD_PREP(CR_CPOL_MASK, (spi->mode & SPI_CPOL) ? 1 : 0);
+	cr |= FIELD_PREP(CR_LOOP_MASK, (spi->mode & SPI_LOOP) ? 1 : 0);
+
+	return cr;
+}
+
+static void hisi_spi_hw_init(struct hisi_spi *hs)
+{
+	hisi_spi_disable(hs);
+
+	/* FIFO default config */
+	writel(FIELD_PREP(FIFOC_TX_MASK, HISI_SPI_TX_64_OR_LESS) |
+		FIELD_PREP(FIFOC_RX_MASK, HISI_SPI_RX_16),
+		hs->regs + HISI_SPI_FIFOC);
+
+	hs->fifo_len = 256;
+}
+
+static irqreturn_t hisi_spi_irq(int irq, void *dev_id)
+{
+	struct spi_controller *master = dev_id;
+	struct hisi_spi *hs = spi_controller_get_devdata(master);
+	u32 irq_status = readl(hs->regs + HISI_SPI_ISR) & ISR_MASK;
+
+	if (!irq_status)
+		return IRQ_NONE;
+
+	if (!master->cur_msg)
+		return IRQ_HANDLED;
+
+	/* Error handling */
+	if (irq_status & ISR_RXOF) {
+		dev_err(hs->dev, "interrupt_transfer: fifo overflow\n");
+		master->cur_msg->status = -EIO;
+		goto finalize_transfer;
+	}
+
+	/*
+	 * Read data from the Rx FIFO every time. If there is
+	 * nothing left to receive, finalize the transfer.
+	 */
+	hisi_spi_reader(hs);
+	if (!hs->rx_len)
+		goto finalize_transfer;
+
+	/* Send data out when Tx FIFO IRQ triggered */
+	if (irq_status & ISR_TX)
+		hisi_spi_writer(hs);
+
+	return IRQ_HANDLED;
+
+finalize_transfer:
+	hisi_spi_disable(hs);
+	spi_finalize_current_transfer(master);
+	return IRQ_HANDLED;
+}
+
+static int hisi_spi_transfer_one(struct spi_controller *master,
+		struct spi_device *spi, struct spi_transfer *transfer)
+{
+	struct hisi_spi *hs = spi_controller_get_devdata(master);
+	struct hisi_chip_data *chip = spi_get_ctldata(spi);
+	u32 cr = chip->cr;
+
+	/* Update per transfer options for speed and bpw */
+	transfer->effective_speed_hz =
+		hisi_calc_effective_speed(master, chip, transfer->speed_hz);
+	cr |= FIELD_PREP(CR_DIV_PRE_MASK, chip->div_pre);
+	cr |= FIELD_PREP(CR_DIV_POST_MASK, chip->div_post);
+	cr |= FIELD_PREP(CR_BPW_MASK, transfer->bits_per_word - 1);
+	writel(cr, hs->regs + HISI_SPI_CR);
+
+	hisi_spi_flush_fifo(hs);
+
+	hs->n_bytes = hisi_spi_n_bytes(transfer);
+	hs->tx = transfer->tx_buf;
+	hs->tx_len = transfer->len / hs->n_bytes;
+	hs->rx = transfer->rx_buf;
+	hs->rx_len = hs->tx_len;
+
+	/*
+	 * Ensure that the transfer data above has been updated
+	 * before the interrupt to start.
+	 */
+	smp_mb();
+
+	/* Enable all interrupts and the controller */
+	writel(~IMR_MASK, hs->regs + HISI_SPI_IMR);
+	writel(1, hs->regs + HISI_SPI_ENR);
+
+	return 1;
+}
+
+static void hisi_spi_handle_err(struct spi_controller *master,
+		struct spi_message *msg)
+{
+	struct hisi_spi *hs = spi_controller_get_devdata(master);
+
+	hisi_spi_disable(hs);
+
+	/*
+	 * Wait for interrupt handler that is
+	 * already in timeout to complete.
+	 */
+	msleep(HISI_SPI_WAIT_TIMEOUT_MS);
+}
+
+static int hisi_spi_setup(struct spi_device *spi)
+{
+	struct hisi_chip_data *chip;
+
+	/* Only alloc on first setup */
+	chip = spi_get_ctldata(spi);
+	if (!chip) {
+		chip = kzalloc(sizeof(*chip), GFP_KERNEL);
+		if (!chip)
+			return -ENOMEM;
+		spi_set_ctldata(spi, chip);
+	}
+
+	chip->cr = hisi_spi_prepare_cr(spi);
+
+	return 0;
+}
+
+static void hisi_spi_cleanup(struct spi_device *spi)
+{
+	struct hisi_chip_data *chip = spi_get_ctldata(spi);
+
+	kfree(chip);
+	spi_set_ctldata(spi, NULL);
+}
+
+static int hisi_spi_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct spi_controller *master;
+	struct hisi_spi *hs;
+	int ret, irq;
+
+	irq = platform_get_irq(pdev, 0);
+	if (irq < 0)
+		return irq;
+
+	master = devm_spi_alloc_master(dev, sizeof(*hs));
+	if (!master)
+		return -ENOMEM;
+
+	platform_set_drvdata(pdev, master);
+
+	hs = spi_controller_get_devdata(master);
+	hs->dev = dev;
+	hs->irq = irq;
+
+	hs->regs = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(hs->regs))
+		return PTR_ERR(hs->regs);
+
+	/* Specify maximum SPI clocking speed (master only) by firmware */
+	ret = device_property_read_u32(dev, "spi-max-frequency",
+					&master->max_speed_hz);
+	if (ret) {
+		dev_err(dev, "failed to get max SPI clocking speed, ret=%d\n",
+			ret);
+		return -EINVAL;
+	}
+
+	ret = device_property_read_u16(dev, "num-cs",
+					&master->num_chipselect);
+	if (ret)
+		master->num_chipselect = DEFAULT_NUM_CS;
+
+	master->mode_bits = SPI_CPOL | SPI_CPHA | SPI_CS_HIGH | SPI_LOOP;
+	master->bits_per_word_mask = SPI_BPW_RANGE_MASK(4, 32);
+	master->bus_num = pdev->id;
+	master->setup = hisi_spi_setup;
+	master->cleanup = hisi_spi_cleanup;
+	master->transfer_one = hisi_spi_transfer_one;
+	master->handle_err = hisi_spi_handle_err;
+	master->dev.fwnode = dev->fwnode;
+
+	hisi_spi_hw_init(hs);
+
+	ret = devm_request_irq(dev, hs->irq, hisi_spi_irq, 0, dev_name(dev),
+			master);
+	if (ret < 0) {
+		dev_err(dev, "failed to get IRQ=%d, ret=%d\n", hs->irq, ret);
+		return ret;
+	}
+
+	ret = spi_register_controller(master);
+	if (ret) {
+		dev_err(dev, "failed to register spi master, ret=%d\n", ret);
+		return ret;
+	}
+
+	dev_info(dev, "hw version:0x%x max-freq:%u kHz\n",
+		readl(hs->regs + HISI_SPI_VERSION),
+		master->max_speed_hz / 1000);
+
+	return 0;
+}
+
+static int hisi_spi_remove(struct platform_device *pdev)
+{
+	struct spi_controller *master = platform_get_drvdata(pdev);
+
+	spi_unregister_controller(master);
+
+	return 0;
+}
+
+static const struct acpi_device_id hisi_spi_acpi_match[] = {
+	{"HISI03E1", 0},
+	{}
+};
+MODULE_DEVICE_TABLE(acpi, hisi_spi_acpi_match);
+
+static struct platform_driver hisi_spi_driver = {
+	.probe		= hisi_spi_probe,
+	.remove		= hisi_spi_remove,
+	.driver		= {
+		.name	= "hisi-kunpeng-spi",
+		.acpi_match_table = hisi_spi_acpi_match,
+	},
+};
+module_platform_driver(hisi_spi_driver);
+
+MODULE_AUTHOR("Jay Fang <f.fangjian@huawei.com>");
+MODULE_DESCRIPTION("HiSilicon SPI Controller Driver for Kunpeng SoCs");
+MODULE_LICENSE("GPL v2");
-- 
2.23.0

