From 3cd5fd3c0c03b6c852586470e955334b6c4760b9 Mon Sep 17 00:00:00 2001
From: Prasad J Pandit <pjp@fedoraproject.org>
Date: Tue, 15 Sep 2020 23:52:59 +0530
Subject: [PATCH] hw: usb: hcd-ohci: check for processed TD before retire

While servicing OHCI transfer descriptors(TD), ohci_service_iso_td
retires a TD if it has passed its time frame. It does not check if
the TD was already processed once and holds an error code in TD_CC.
It may happen if the TD list has a loop. Add check to avoid an
infinite loop condition.

Signed-off-by: Prasad J Pandit <pjp@fedoraproject.org>
Reviewed-by: Li Qiang <liq3ea@gmail.com>
Message-id: 20200915182259.68522-3-ppandit@redhat.com
Signed-off-by: Gerd Hoffmann <kraxel@redhat.com>
(cherry-picked from 1be90ebe)
Fix CVE-2020-25625
Signed-off-by: Alex Chen <alex.chen@huawei.com>
---
 hw/usb/hcd-ohci.c | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/hw/usb/hcd-ohci.c b/hw/usb/hcd-ohci.c
index 4f6fdbc0a7..ffe52a09d7 100644
--- a/hw/usb/hcd-ohci.c
+++ b/hw/usb/hcd-ohci.c
@@ -689,6 +689,10 @@ static int ohci_service_iso_td(OHCIState *ohci, struct ohci_ed *ed,
            the next ISO TD of the same ED */
         trace_usb_ohci_iso_td_relative_frame_number_big(relative_frame_number,
                                                         frame_count);
+        if (OHCI_CC_DATAOVERRUN == OHCI_BM(iso_td.flags, TD_CC)) {
+            /* avoid infinite loop */
+            return 1;
+        }
         OHCI_SET_BM(iso_td.flags, TD_CC, OHCI_CC_DATAOVERRUN);
         ed->head &= ~OHCI_DPTR_MASK;
         ed->head |= (iso_td.next & OHCI_DPTR_MASK);
-- 
2.27.0

