From 3b8e4bca9d5d51219778950456d52226a9caffdf Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Philippe=20Mathieu-Daud=C3=A9?= <f4bug@amsat.org>
Date: Tue, 5 Jun 2018 22:28:51 -0300
Subject: [PATCH 4/7] hw/sd/sdcard: Simplify realize() a bit
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

We don't need to check if sd->blk is set twice.

Reviewed-by: Peter Maydell <peter.maydell@linaro.org>
Signed-off-by: Philippe Mathieu-Daudé <f4bug@amsat.org>
Reviewed-by: Alistair Francis <alistair.francis@wdc.com>
Message-Id: <20200630133912.9428-18-f4bug@amsat.org>
---
 hw/sd/sd.c | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

diff --git a/hw/sd/sd.c b/hw/sd/sd.c
index ed3eae930b..caac17e71b 100644
--- a/hw/sd/sd.c
+++ b/hw/sd/sd.c
@@ -2090,12 +2090,12 @@ static void sd_realize(DeviceState *dev, Error **errp)
         return;
     }
 
-    if (sd->blk && blk_is_read_only(sd->blk)) {
-        error_setg(errp, "Cannot use read-only drive as SD card");
-        return;
-    }
-
     if (sd->blk) {
+        if (blk_is_read_only(sd->blk)) {
+            error_setg(errp, "Cannot use read-only drive as SD card");
+            return;
+        }
+
         ret = blk_set_perm(sd->blk, BLK_PERM_CONSISTENT_READ | BLK_PERM_WRITE,
                            BLK_PERM_ALL, errp);
         if (ret < 0) {
-- 
2.17.1

