From 3fb16cbd24233829b3696e06abb12db317d68aac Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Philippe=20Mathieu-Daud=C3=A9?= <f4bug@amsat.org>
Date: Wed, 3 Jun 2020 19:59:16 +0200
Subject: [PATCH 3/7] hw/sd/sdcard: Restrict Class 6 commands to SCSD cards
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Only SCSD cards support Class 6 (Block Oriented Write Protection)
commands.

  "SD Specifications Part 1 Physical Layer Simplified Spec. v3.01"

  4.3.14 Command Functional Difference in Card Capacity Types

  * Write Protected Group

  SDHC and SDXC do not support write-protected groups. Issuing
  CMD28, CMD29 and CMD30 generates the ILLEGAL_COMMAND error.

Cc: qemu-stable@nongnu.org
Reviewed-by: Peter Maydell <peter.maydell@linaro.org>
Signed-off-by: Philippe Mathieu-Daudé <f4bug@amsat.org>
Reviewed-by: Alistair Francis <alistair.francis@wdc.com>
Message-Id: <20200630133912.9428-7-f4bug@amsat.org>
---
 hw/sd/sd.c | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/hw/sd/sd.c b/hw/sd/sd.c
index 917195a65b..ed3eae930b 100644
--- a/hw/sd/sd.c
+++ b/hw/sd/sd.c
@@ -905,6 +905,11 @@ static sd_rsp_type_t sd_normal_command(SDState *sd, SDRequest req)
         sd->multi_blk_cnt = 0;
     }
 
+    if (sd_cmd_class[req.cmd] == 6 && FIELD_EX32(sd->ocr, OCR, CARD_CAPACITY)) {
+        /* Only Standard Capacity cards support class 6 commands */
+        return sd_illegal;
+    }
+
     switch (req.cmd) {
     /* Basic commands (Class 0 and Class 1) */
     case 0:	/* CMD0:   GO_IDLE_STATE */
-- 
2.17.1

