From 0bf68c660e932e76087dc8c87f8b1dacba89c2be Mon Sep 17 00:00:00 2001
From: Weifeng Li <liweifeng96@126.com>
Date: Sat, 18 Jul 2020 12:35:38 +0800
Subject: net/bonding: change state machine to defaulted

A dpdk bonding 802.3ad network as follows:
+----------+                        +-----------+
|dpdk lacp |bond1.1 <------> bond2.1|switch lacp|
|          |bond1.2 <------> bond2.2|           |
+----------+                        +-----------+
If a fiber optic go wrong about single pass during normal running like
this:
bond1.2 -----> bond2.2 ok
bond1.2 <--x-- bond2.2 error: bond1.2 receive no LACPDU Some packets
			      from switch to dpdk will choose bond2.2
			      and lost.

DPDK lacp state machine will transits to the expired state if no LACPDU
is received before the current_while_timer expires. But if no LACPDU is
received before the current_while_timer expires again, DPDK lacp state
machine has no change. Bond2.2 can not change to inactive depend on the
received LACPDU.
According to IEEE 802.3ad, if no lacpdu is received before the
current_while_timer expires again, the state machine should transits
from expired to defaulted. Bond2.2 will change to inactive depend on the
LACPDU with defaulted state.

This patch adds a state machine change from expired to defaulted when no
lacpdu is received before the current_while_timer expires again
according to IEEE 802.3ad:
If no LACPDU is received before the current_while timer expires again,
the state machine transits to the DEFAULTED state. The record Default
function overwrites the current operational parameters for the Partner
with administratively configured values. This allows configuration of
aggregations and individual links when no protocol partner is present,
while still permitting an active partner to override default settings.
The update_Default_Selected function sets the Selected variable FALSE
if the Link Aggregation Group has changed. Since all operational
parameters are now set to locally administered values there can be no
disagreement as to the Link Aggregation Group, so the Matched variable
is set TRUE.

The relevant description is in the chapter 43.4.12 of the link below:
https://ieeexplore.ieee.org/stamp/stamp.jsp?tp=&arnumber=850426

Signed-off-by: Weifeng Li <liweifeng96@126.com>
Acked-by: Wei Hu (Xavier) <xavier.huwei@huawei.com>
---
 drivers/net/bonding/eth_bond_8023ad_private.h |  3 +++
 drivers/net/bonding/rte_eth_bond_8023ad.c     | 21 +++++++++++++++++----
 2 files changed, 20 insertions(+), 4 deletions(-)

(limited to 'drivers/net/bonding')

diff --git a/drivers/net/bonding/eth_bond_8023ad_private.h b/drivers/net/bonding/eth_bond_8023ad_private.h
index 6e44ffdb1c..9b5738afee 100644
--- a/drivers/net/bonding/eth_bond_8023ad_private.h
+++ b/drivers/net/bonding/eth_bond_8023ad_private.h
@@ -50,6 +50,7 @@
 #define SM_FLAGS_MOVED                      0x0100
 #define SM_FLAGS_PARTNER_SHORT_TIMEOUT      0x0200
 #define SM_FLAGS_NTT                        0x0400
+#define SM_FLAGS_EXPIRED                    0x0800
 
 #define BOND_LINK_FULL_DUPLEX_KEY           0x01
 #define BOND_LINK_SPEED_KEY_10M             0x02
@@ -103,6 +104,8 @@ struct port {
 
 	/** The operational Partner's port parameters */
 	struct port_params partner;
+	/** Partner administrative parameter values */
+	struct port_params partner_admin;
 
 	/* Additional port parameters not listed in documentation */
 	/** State machine flags */
diff --git a/drivers/net/bonding/rte_eth_bond_8023ad.c b/drivers/net/bonding/rte_eth_bond_8023ad.c
index b24a446862..67ca0730fa 100644
--- a/drivers/net/bonding/rte_eth_bond_8023ad.c
+++ b/drivers/net/bonding/rte_eth_bond_8023ad.c
@@ -356,16 +356,28 @@ rx_machine(struct bond_dev_private *internals, uint16_t slave_id,
 
 		timer_set(&port->current_while_timer, timeout);
 		ACTOR_STATE_CLR(port, EXPIRED);
+		SM_FLAG_CLR(port, EXPIRED);
 		return; /* No state change */
 	}
 
 	/* If CURRENT state timer is not running (stopped or expired)
 	 * transit to EXPIRED state from DISABLED or CURRENT */
 	if (!timer_is_running(&port->current_while_timer)) {
-		ACTOR_STATE_SET(port, EXPIRED);
-		PARTNER_STATE_CLR(port, SYNCHRONIZATION);
-		PARTNER_STATE_SET(port, LACP_SHORT_TIMEOUT);
-		timer_set(&port->current_while_timer, internals->mode4.short_timeout);
+		if (SM_FLAG(port, EXPIRED)) {
+			port->selected = UNSELECTED;
+			memcpy(&port->partner, &port->partner_admin,
+				sizeof(struct port_params));
+			record_default(port);
+			ACTOR_STATE_CLR(port, EXPIRED);
+			timer_cancel(&port->current_while_timer);
+		} else {
+			SM_FLAG_SET(port, EXPIRED);
+			ACTOR_STATE_SET(port, EXPIRED);
+			PARTNER_STATE_CLR(port, SYNCHRONIZATION);
+			PARTNER_STATE_SET(port, LACP_SHORT_TIMEOUT);
+			timer_set(&port->current_while_timer,
+				internals->mode4.short_timeout);
+		}
 	}
 }
 
@@ -1021,6 +1033,7 @@ bond_mode_8023ad_activate_slave(struct rte_eth_dev *bond_dev,
 	port->actor.port_number = rte_cpu_to_be_16(slave_id + 1);
 
 	memcpy(&port->partner, &initial, sizeof(struct port_params));
+	memcpy(&port->partner_admin, &initial, sizeof(struct port_params));
 
 	/* default states */
 	port->actor_state = STATE_AGGREGATION | STATE_LACP_ACTIVE | STATE_DEFAULTED;
-- 
cgit v1.2.1


