From fad80ab3698e7f7d3e9c2a28c371da6a17fbc477 Mon Sep 17 00:00:00 2001
From: Vadim Podovinnikov <podovinnikov@protei.ru>
Date: Wed, 17 Feb 2021 16:26:55 +0000
Subject: net/bonding: fix LACP system address check

In bond (LACP) we have several NICs (ports), when we have negotiation
with peer about what port we prefer, we send information about what
system we preferred in partner system name field. Peer also sends us
what partner system name it prefer.

When we receive a message from it we must compare its preferred system
name with our system name, but not with our port mac address

In my test I have several problems with that:
1. If master port (mac address same as system address) shuts down (I
   have two ports) I loose connection
2. If secondary port (mac address not same as system address) receives
   message before master port, my connection is not established.

Fixes: 56cbc0817399 ("net/bonding: fix LACP negotiation")
Cc: stable@dpdk.org

Signed-off-by: Vadim Podovinnikov <podovinnikov@protei.ru>
Acked-by: Min Hu (Connor) <humin29@huawei.com>
---
 drivers/net/bonding/rte_eth_bond_8023ad.c | 17 ++++++++++++++++-
 1 file changed, 16 insertions(+), 1 deletion(-)

(limited to 'drivers/net/bonding')

diff --git a/drivers/net/bonding/rte_eth_bond_8023ad.c b/drivers/net/bonding/rte_eth_bond_8023ad.c
index 5fe004e551..128754f459 100644
--- a/drivers/net/bonding/rte_eth_bond_8023ad.c
+++ b/drivers/net/bonding/rte_eth_bond_8023ad.c
@@ -804,19 +804,34 @@ rx_machine_update(struct bond_dev_private *internals, uint16_t slave_id,
 		struct rte_mbuf *lacp_pkt) {
 	struct lacpdu_header *lacp;
 	struct lacpdu_actor_partner_params *partner;
+	struct port *port, *agg;
 
 	if (lacp_pkt != NULL) {
 		lacp = rte_pktmbuf_mtod(lacp_pkt, struct lacpdu_header *);
 		RTE_ASSERT(lacp->lacpdu.subtype == SLOW_SUBTYPE_LACP);
 
 		partner = &lacp->lacpdu.partner;
+		port = &bond_mode_8023ad_ports[slave_id];
+		agg = &bond_mode_8023ad_ports[port->aggregator_port_id];
+
 		if (rte_is_zero_ether_addr(&partner->port_params.system) ||
 			rte_is_same_ether_addr(&partner->port_params.system,
-			&internals->mode4.mac_addr)) {
+				&agg->actor.system)) {
 			/* This LACP frame is sending to the bonding port
 			 * so pass it to rx_machine.
 			 */
 			rx_machine(internals, slave_id, &lacp->lacpdu);
+		} else {
+			char preferred_system_name[RTE_ETHER_ADDR_FMT_SIZE];
+			char self_system_name[RTE_ETHER_ADDR_FMT_SIZE];
+
+			rte_ether_format_addr(preferred_system_name,
+				RTE_ETHER_ADDR_FMT_SIZE, &partner->port_params.system);
+			rte_ether_format_addr(self_system_name,
+				RTE_ETHER_ADDR_FMT_SIZE, &agg->actor.system);
+			MODE4_DEBUG("preferred partner system %s "
+				"is not equal with self system: %s\n",
+				preferred_system_name, self_system_name);
 		}
 		rte_pktmbuf_free(lacp_pkt);
 	} else
-- 
cgit v1.2.1


