From 947dbf5874fd55dd5fe536fe02b3ff699d4efbf5 Mon Sep 17 00:00:00 2001
From: Leo Yan <leo.yan@linaro.org>
Date: Fri, 31 Dec 2021 13:32:10 +0800
Subject: [PATCH 13/21] perf arm-spe: Add new function arm_spe_pkt_desc_event()

mainline inclusion
from mainline-v5.11-rc1
commit e66f6d75960220001ce94afe93c981826235c003
category: feature
bugzilla: https://gitee.com/openeuler/kernel/issues/I4NGPV
CVE: NA

-------------------------------------------------

This patch moves out the event packet parsing from arm_spe_pkt_desc()
to the new function arm_spe_pkt_desc_event().

Signed-off-by: Leo Yan <leo.yan@linaro.org>
Reviewed-by: Andre Przywara <andre.przywara@arm.com>
Acked-by: Will Deacon <will@kernel.org>
Cc: Alexander Shishkin <alexander.shishkin@linux.intel.com>
Cc: Al Grant <Al.Grant@arm.com>
Cc: Arnaldo Carvalho de Melo <acme@kernel.org>
Cc: Dave Martin <Dave.Martin@arm.com>
Cc: Ingo Molnar <mingo@redhat.com>
Cc: James Clark <james.clark@arm.com>
Cc: Jiri Olsa <jolsa@redhat.com>
Cc: John Garry <john.garry@huawei.com>
Cc: Mark Rutland <mark.rutland@arm.com>
Cc: Mathieu Poirier <mathieu.poirier@linaro.org>
Cc: Namhyung Kim <namhyung@kernel.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Wei Li <liwei391@huawei.com>
Link: https://lore.kernel.org/r/20201119152441.6972-10-leo.yan@linaro.org
Signed-off-by: Arnaldo Carvalho de Melo <acme@redhat.com>
Signed-off-by: Wei Li <liwei391@huawei.com>
Reviewed-by: Yang Jihong <yangjihong1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 .../arm-spe-decoder/arm-spe-pkt-decoder.c     | 63 +++++++++++--------
 1 file changed, 37 insertions(+), 26 deletions(-)

diff --git a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
index 52f4339b1f0c..da6b9f76739c 100644
--- a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
+++ b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
@@ -287,6 +287,42 @@ static int arm_spe_pkt_out_string(int *err, char **buf_p, size_t *blen,
 	return ret;
 }
 
+static int arm_spe_pkt_desc_event(const struct arm_spe_pkt *packet,
+				  char *buf, size_t buf_len)
+{
+	u64 payload = packet->payload;
+	int err = 0;
+
+	arm_spe_pkt_out_string(&err, &buf, &buf_len, "EV");
+
+	if (payload & 0x1)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " EXCEPTION-GEN");
+	if (payload & 0x2)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " RETIRED");
+	if (payload & 0x4)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " L1D-ACCESS");
+	if (payload & 0x8)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " L1D-REFILL");
+	if (payload & 0x10)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " TLB-ACCESS");
+	if (payload & 0x20)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " TLB-REFILL");
+	if (payload & 0x40)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " NOT-TAKEN");
+	if (payload & 0x80)
+		arm_spe_pkt_out_string(&err, &buf, &buf_len, " MISPRED");
+	if (packet->index > 1) {
+		if (payload & 0x100)
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " LLC-ACCESS");
+		if (payload & 0x200)
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " LLC-REFILL");
+		if (payload & 0x400)
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " REMOTE-ACCESS");
+	}
+
+	return err;
+}
+
 static int arm_spe_pkt_desc_addr(const struct arm_spe_pkt *packet,
 				 char *buf, size_t buf_len)
 {
@@ -367,32 +403,7 @@ int arm_spe_pkt_desc(const struct arm_spe_pkt *packet, char *buf,
 		arm_spe_pkt_out_string(&err, &buf, &blen, "%s", name);
 		break;
 	case ARM_SPE_EVENTS:
-		arm_spe_pkt_out_string(&err, &buf, &blen, "EV");
-
-		if (payload & 0x1)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " EXCEPTION-GEN");
-		if (payload & 0x2)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " RETIRED");
-		if (payload & 0x4)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " L1D-ACCESS");
-		if (payload & 0x8)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " L1D-REFILL");
-		if (payload & 0x10)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " TLB-ACCESS");
-		if (payload & 0x20)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " TLB-REFILL");
-		if (payload & 0x40)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " NOT-TAKEN");
-		if (payload & 0x80)
-			arm_spe_pkt_out_string(&err, &buf, &blen, " MISPRED");
-		if (idx > 1) {
-			if (payload & 0x100)
-				arm_spe_pkt_out_string(&err, &buf, &blen, " LLC-ACCESS");
-			if (payload & 0x200)
-				arm_spe_pkt_out_string(&err, &buf, &blen, " LLC-REFILL");
-			if (payload & 0x400)
-				arm_spe_pkt_out_string(&err, &buf, &blen, " REMOTE-ACCESS");
-		}
+		err = arm_spe_pkt_desc_event(packet, buf, buf_len);
 		break;
 	case ARM_SPE_OP_TYPE:
 		switch (idx) {
-- 
2.27.0

