From 574ebcfb7fa23c87ee9bf03f46db5e4a9fb99b7d Mon Sep 17 00:00:00 2001
From: Leo Yan <leo.yan@linaro.org>
Date: Fri, 31 Dec 2021 13:32:15 +0800
Subject: [PATCH 18/21] perf arm-spe: Add more sub classes for operation packet

mainline inclusion
from mainline-v5.11-rc1
commit 3d829724b16c5d2de42e6c9601c696c93a10bc61
category: feature
bugzilla: https://gitee.com/openeuler/kernel/issues/I4NGPV
CVE: NA

-------------------------------------------------

For the operation type packet payload with load/store class, it misses
to support these sub classes:

  - A load/store targeting the general-purpose registers;
  - A load/store targeting unspecified registers;
  - The ARMv8.4 nested virtualisation extension can redirect system
    register accesses to a memory page controlled by the hypervisor.
    The SPE profiling feature in newer implementations can tag those
    memory accesses accordingly.

Add the bit pattern describing load/store sub classes, so that the perf
tool can decode it properly.

Inspired by Andre Przywara, refined the commit log and code for more
clear description.

Co-developed-by: Andre Przywara <andre.przywara@arm.com>
Signed-off-by: Leo Yan <leo.yan@linaro.org>
Reviewed-by: Andre Przywara <andre.przywara@arm.com>
Acked-by: Will Deacon <will@kernel.org>
Cc: Alexander Shishkin <alexander.shishkin@linux.intel.com>
Cc: Al Grant <Al.Grant@arm.com>
Cc: Arnaldo Carvalho de Melo <acme@kernel.org>
Cc: Dave Martin <Dave.Martin@arm.com>
Cc: Ingo Molnar <mingo@redhat.com>
Cc: James Clark <james.clark@arm.com>
Cc: Jiri Olsa <jolsa@redhat.com>
Cc: John Garry <john.garry@huawei.com>
Cc: Mark Rutland <mark.rutland@arm.com>
Cc: Mathieu Poirier <mathieu.poirier@linaro.org>
Cc: Namhyung Kim <namhyung@kernel.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Wei Li <liwei391@huawei.com>
Link: https://lore.kernel.org/r/20201119152441.6972-15-leo.yan@linaro.org
Signed-off-by: Arnaldo Carvalho de Melo <acme@redhat.com>
Signed-off-by: Wei Li <liwei391@huawei.com>
Reviewed-by: Yang Jihong <yangjihong1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 .../util/arm-spe-decoder/arm-spe-pkt-decoder.c | 18 ++++++++++++++++--
 1 file changed, 16 insertions(+), 2 deletions(-)

diff --git a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
index 1d1354a0eef4..84d661aab54f 100644
--- a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
+++ b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
@@ -343,9 +343,23 @@ static int arm_spe_pkt_desc_op_type(const struct arm_spe_pkt *packet,
 				arm_spe_pkt_out_string(&err, &buf, &buf_len, " EXCL");
 			if (payload & SPE_OP_PKT_AR)
 				arm_spe_pkt_out_string(&err, &buf, &buf_len, " AR");
-		} else if (SPE_OP_PKT_LDST_SUBCLASS_GET(payload) ==
-					SPE_OP_PKT_LDST_SUBCLASS_SIMD_FP) {
+		}
+
+		switch (SPE_OP_PKT_LDST_SUBCLASS_GET(payload)) {
+		case SPE_OP_PKT_LDST_SUBCLASS_SIMD_FP:
 			arm_spe_pkt_out_string(&err, &buf, &buf_len, " SIMD-FP");
+			break;
+		case SPE_OP_PKT_LDST_SUBCLASS_GP_REG:
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " GP-REG");
+			break;
+		case SPE_OP_PKT_LDST_SUBCLASS_UNSPEC_REG:
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " UNSPEC-REG");
+			break;
+		case SPE_OP_PKT_LDST_SUBCLASS_NV_SYSREG:
+			arm_spe_pkt_out_string(&err, &buf, &buf_len, " NV-SYSREG");
+			break;
+		default:
+			break;
 		}
 		break;
 	case SPE_OP_PKT_HDR_CLASS_BR_ERET:
-- 
2.27.0

