From 0585219f59a01f01b116e47a9cd5b90bf6bba025 Mon Sep 17 00:00:00 2001
From: Hao Chen <chenhao288@hisilicon.com>
Date: Sat, 26 Mar 2022 17:51:00 +0800
Subject: [PATCH 270/283] net: hns3: fix ethtool tx copybreak buf size
 indicating not aligned issue

mainline inclusion
from mainline-v5.18-rc1
commit 8778372118023e2258612c03573c47efef41d755
category: bugfix
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EN49

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=8778372118023e2258612c03573c47efef41d755

--------------------------------

When use ethtoool set tx copybreak buf size to a large value
which causes order exceeding 10 or memory is not enough,
it causes allocating tx copybreak buffer failed and print
"the active tx spare buf is 0, not enabled tx spare buffer",
however, use --get-tunable parameter query tx copybreak buf
size and it indicates setting value not 0.

So, it's necessary to change the print value from setting
value to 0.

Set kinfo.tx_spare_buf_size to 0 when set tx copybreak buf size failed.

Fixes: e445f08af2b1 ("net: hns3: add support to set/get tx copybreak buf size via ethtool for hns3 driver")
Signed-off-by: Hao Chen <chenhao288@hisilicon.com>
Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>
---
 .../net/ethernet/hisilicon/hns3/hns3_enet.c   | 20 +++++++++++--------
 .../ethernet/hisilicon/hns3/hns3_ethtool.c    |  3 ++-
 2 files changed, 14 insertions(+), 9 deletions(-)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c
index 18d0a218040a..f9dacf01ddd6 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_enet.c
@@ -736,13 +736,12 @@ static bool hns3_can_use_tx_sgl(struct hns3_enet_ring *ring,
 
 static void hns3_init_tx_spare_buffer(struct hns3_enet_ring *ring)
 {
+	u32 alloc_size = ring->tqp->handle->kinfo.tx_spare_buf_size;
 	struct hns3_tx_spare *tx_spare;
 	struct page *page;
-	u32 alloc_size;
 	dma_addr_t dma;
 	int order;
 
-	alloc_size = ring->tqp->handle->kinfo.tx_spare_buf_size;
 	if (!alloc_size)
 		return;
 
@@ -752,30 +751,35 @@ static void hns3_init_tx_spare_buffer(struct hns3_enet_ring *ring)
 	if (!tx_spare) {
 		/* The driver still work without the tx spare buffer */
 		dev_warn(ring_to_dev(ring), "failed to allocate hns3_tx_spare\n");
-		return;
+		goto devm_kzalloc_error;
 	}
 
 	page = alloc_pages_node(dev_to_node(ring_to_dev(ring)),
 				GFP_KERNEL, order);
 	if (!page) {
 		dev_warn(ring_to_dev(ring), "failed to allocate tx spare pages\n");
-		devm_kfree(ring_to_dev(ring), tx_spare);
-		return;
+		goto alloc_pages_error;
 	}
 
 	dma = dma_map_page(ring_to_dev(ring), page, 0,
 			   PAGE_SIZE << order, DMA_TO_DEVICE);
 	if (dma_mapping_error(ring_to_dev(ring), dma)) {
 		dev_warn(ring_to_dev(ring), "failed to map pages for tx spare\n");
-		put_page(page);
-		devm_kfree(ring_to_dev(ring), tx_spare);
-		return;
+		goto dma_mapping_error;
 	}
 
 	tx_spare->dma = dma;
 	tx_spare->buf = page_address(page);
 	tx_spare->len = PAGE_SIZE << order;
 	ring->tx_spare = tx_spare;
+	return;
+
+dma_mapping_error:
+	put_page(page);
+alloc_pages_error:
+	devm_kfree(ring_to_dev(ring), tx_spare);
+devm_kzalloc_error:
+	ring->tqp->handle->kinfo.tx_spare_buf_size = 0;
 }
 
 /* Use hns3_tx_spare_space() to make sure there is enough buffer
diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3_ethtool.c b/drivers/net/ethernet/hisilicon/hns3/hns3_ethtool.c
index a6f339c6046d..8ac71b53ddf0 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3_ethtool.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3_ethtool.c
@@ -1879,7 +1879,8 @@ static int hns3_set_tunable(struct net_device *netdev,
 		old_tx_spare_buf_size = h->kinfo.tx_spare_buf_size;
 		new_tx_spare_buf_size = *(u32 *)data;
 		ret = hns3_set_tx_spare_buf_size(netdev, new_tx_spare_buf_size);
-		if (ret) {
+		if (ret ||
+		    (!priv->ring->tx_spare && new_tx_spare_buf_size != 0)) {
 			int ret1;
 
 			netdev_warn(netdev,
-- 
2.34.1

