From eac9484827942af027d362264f1730824e162108 Mon Sep 17 00:00:00 2001
From: Andre Przywara <andre.przywara@arm.com>
Date: Fri, 31 Dec 2021 13:32:16 +0800
Subject: [PATCH 19/21] perf arm_spe: Decode memory tagging properties

mainline inclusion
from mainline-v5.11-rc1
commit 3601e605501df289db149785e1e6a8d16e557d31
category: feature
bugzilla: https://gitee.com/openeuler/kernel/issues/I4NGPV
CVE: NA

-------------------------------------------------

When SPE records a physical address, it can additionally tag the event
with information from the Memory Tagging architecture extension.

Decode the two additional fields in the SPE event payload.

[leoy: Refined patch to use predefined macros]

Signed-off-by: Andre Przywara <andre.przywara@arm.com>
Signed-off-by: Leo Yan <leo.yan@linaro.org>
Reviewed-by: Dave Martin <Dave.Martin@arm.com>
Acked-by: Will Deacon <will@kernel.org>
Cc: Alexander Shishkin <alexander.shishkin@linux.intel.com>
Cc: Al Grant <Al.Grant@arm.com>
Cc: Arnaldo Carvalho de Melo <acme@kernel.org>
Cc: Ingo Molnar <mingo@redhat.com>
Cc: James Clark <james.clark@arm.com>
Cc: Jiri Olsa <jolsa@redhat.com>
Cc: John Garry <john.garry@huawei.com>
Cc: Mark Rutland <mark.rutland@arm.com>
Cc: Mathieu Poirier <mathieu.poirier@linaro.org>
Cc: Namhyung Kim <namhyung@kernel.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Wei Li <liwei391@huawei.com>
Link: https://lore.kernel.org/r/20201119152441.6972-16-leo.yan@linaro.org
Signed-off-by: Arnaldo Carvalho de Melo <acme@redhat.com>
Signed-off-by: Wei Li <liwei391@huawei.com>
Reviewed-by: Yang Jihong <yangjihong1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c | 6 +++++-
 tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.h | 2 ++
 2 files changed, 7 insertions(+), 1 deletion(-)

diff --git a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
index 84d661aab54f..57c01ce27915 100644
--- a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
+++ b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
@@ -385,6 +385,7 @@ static int arm_spe_pkt_desc_addr(const struct arm_spe_pkt *packet,
 				 char *buf, size_t buf_len)
 {
 	int ns, el, idx = packet->index;
+	int ch, pat;
 	u64 payload = packet->payload;
 	int err = 0;
 
@@ -404,9 +405,12 @@ static int arm_spe_pkt_desc_addr(const struct arm_spe_pkt *packet,
 		break;
 	case SPE_ADDR_PKT_HDR_INDEX_DATA_PHYS:
 		ns = !!SPE_ADDR_PKT_GET_NS(payload);
+		ch = !!SPE_ADDR_PKT_GET_CH(payload);
+		pat = SPE_ADDR_PKT_GET_PAT(payload);
 		payload = SPE_ADDR_PKT_ADDR_GET_BYTES_0_6(payload);
 		arm_spe_pkt_out_string(&err, &buf, &buf_len,
-				       "PA 0x%llx ns=%d", payload, ns);
+				       "PA 0x%llx ns=%d ch=%d pat=%x",
+				       payload, ns, ch, pat);
 		break;
 	default:
 		/* Unknown index */
diff --git a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.h b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.h
index 7032fc141ad4..1ad14885c2a1 100644
--- a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.h
+++ b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.h
@@ -73,6 +73,8 @@ struct arm_spe_pkt {
 
 #define SPE_ADDR_PKT_GET_NS(v)			(((v) & BIT_ULL(63)) >> 63)
 #define SPE_ADDR_PKT_GET_EL(v)			(((v) & GENMASK_ULL(62, 61)) >> 61)
+#define SPE_ADDR_PKT_GET_CH(v)			(((v) & BIT_ULL(62)) >> 62)
+#define SPE_ADDR_PKT_GET_PAT(v)			(((v) & GENMASK_ULL(59, 56)) >> 56)
 
 #define SPE_ADDR_PKT_EL0			0
 #define SPE_ADDR_PKT_EL1			1
-- 
2.27.0

